VRRP probe commands -- display system internal vrrp kernel

Use display system internal vrrp kernel to display IPv4 VRRP kernel information.

Syntax

Centralized devices:

display system internal vrrp kernel { virtual-ip | virtual-router } [ interface interface-type interface number [ vrid virtual-router-id ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal vrrp kernel { virtual-ip | virtual-router } [ interface interface-type interface number [ vrid virtual-router-id ] ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal vrrp kernel { virtual-ip | virtual-router } [ interface interface-type interface number [ vrid virtual-router-id ] ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

virtual-ip: Displays virtual IP address information.

virtual-router: Displays virtual router information.

interface interface-type interface-number: Specifies an interface by its type and number.

vrid virtual-router-id: Specifies an IPv4 VRRP group by its virtual router ID.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VRRP probe commands -- display system internal vrrp ipv6 kernel

Use display system internal vrrp ipv6 kernel to display IPv6 VRRP kernel information.

Syntax

Centralized devices:

display system internal vrrp ipv6 kernel { virtual-ip | virtual-router } [ interface interface-type interface number [ vrid virtual-router-id ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal vrrp ipv6 kernel { virtual-ip | virtual-router } [ interface interface-type interface number [ vrid virtual-router-id ] ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal vrrp ipv6 kernel { virtual-ip | virtual-router } [ interface interface-type interface number [ vrid virtual-router-id ] ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

virtual-ip: Displays virtual IP address information.

virtual-router: Displays virtual router information.

interface interface-type interface-number: Specifies an interface by its type and number.

vrid virtual-router-id: Specifies an IPv6 VRRP group by its virtual router ID.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.