BGP probe commands -- display system internal bgp address-family statistics

Use display system internal bgp address-family statistics to display BGP instance statistics.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] address-family { ipv4 | ipv6 | vpnv4 } [ vpn-instance vpn-instance-name ] [ rib | send ] statistics

display system internal bgp [ instance instance-name ] address-family { l2vpn [ evpn ] | vpnv6 } [ rib | send ] statistics

display system internal bgp [ instance instance-name ] address-family ipv4 mdt [ rib | send ] statistics

display system internal bgp [ instance instance-name ] address-family { ipv4 | ipv6 } multicast [ rib | send ] statistics

display system internal bgp [ instance instance-name ] address-family link-state [ rib | send ] statistics

display system internal bgp [ instance instance-name ] address-family rtfilter [ rib | send ] statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] address-family { ipv4 | ipv6 | vpnv4 } [ vpn-instance vpn-instance-name ] [ rib | send ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family { l2vpn [ evpn ] | vpnv6 } [ rib | send ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family { ipv4 | ipv6 } multicast [ rib | send ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family link-state [ rib | send ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family rtfilter [ rib | send ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] address-family { ipv4 | ipv6 | vpnv4 } [ vpn-instance vpn-instance-name ] [ rib | send ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family { l2vpn [ evpn ] | vpnv6 } [ rib | send ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family { ipv4 | ipv6 } multicast [ rib | send ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family link-state [ rib | send ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] address-family rtfilter [ rib | send ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays statistics for the default BGP instance.

ipv4: Displays BGP instance statistics for IPv4 address family.

ipv6: Displays BGP instance statistics for IPv6 address family.

vpnv4: Displays BGP instance statistics for VPNv4 address family.

l2vpn: Displays BGP instance statistics for L2VPN address family.

evpn: Displays BGP instance statistics for EVPN address family.

vpnv6: Displays BGP instance statistics for VPNv6 address family.

mdt: Displays BGP instance statistics for MDT address family.

multicast: Displays BGP instance statistics for multicast address family.

link-state: Displays BGP instance statistics for LS address family.

rtfilter: Displays BGP instance statistics for RT filter address family.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP instance statistics for the public network.

rib: Displays statistics for the BGP instance route module.

send: Displays statistics for the BGP instance sending module.

standby: Displays BGP instance statistics for a standby BGP process. If you do not specify a standby BGP process, this command displays BGP instance statistics for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify the rib keyword or the send keyword, this command displays BGP instance statistics for the specified address family.

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp graceful-restart statistics

Use display system internal bgp graceful-restart statistics to display BGP GR statistics.

Syntax

display system internal bgp [ instance instance-name ] graceful-restart statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays GR statistics for the default BGP instance.

BGP probe commands -- display system internal bgp interface

Use display system internal bgp interface to display BGP interface information.

Syntax

display system internal bgp [ instance instance-name ] interface ipv4 [ vpn-instance vpn-instance-name] [ interface-type interface-number | ipv4-address { mask-length | mask } ]

display system internal bgp [ instance instance-name ] interface ipv6 [ vpn-instance vpn-instance-name] [ interface-type interface-number | ipv6-address prefix-length ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays interface information for the default BGP instance.

ipv4: Displays BGP interface information for IPv4 address family.

ipv6: Displays BGP interface information for IPv6 address family.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP interface information for the public network.

interface-type interface-number: Specifies a BGP interface by its type and number.

ipv4-address: Specifies a BGP interface by its IPv4 address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a mask in dotted decimal notation.

ipv6-address prefix-length: Specifies a BGP interface by its IPv6 address. The prefix-length argument specifies the prefix length in the range of 0 to 128.

Usage guidelines

If you do not specify the interface-type interface-number argument, the ipv4-address { mask-length | mask } argument, or the ipv6-address prefix-length argument, this command displays information about all BGP interfaces.

BGP probe commands -- display system internal bgp l2vpn auto-discovery advertise-info

Use display system internal bgp l2vpn auto-discovery advertise-info to display advertisement information for a VPLS PE discovered by BGP.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery route-distinguisher route-distinguisher pe-address ip-address advertise-info

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery route-distinguisher route-distinguisher pe-address ip-address advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery route-distinguisher route-distinguisher pe-address ip-address advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

pe-address ip-address: Specifies a PE by its IP address.

standby: Displays BGP-discovered VPLS PE advertisement information for a standby BGP process. If you do not specify this keyword, the command displays BGP-discovered VPLS PE advertisement information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp l2vpn auto-discovery standby

Use display system internal bgp l2vpn auto-discovery standby to display information about VPLS PEs discovered by BGP for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery [ peer ip-address { advertised | received } [ statistics ] | route-distinguisher route-distinguisher [ pe-address ip-address ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery [ peer ip-address { advertised | received } [ statistics ] | route-distinguisher route-distinguisher [ pe-address ip-address ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

peer ip-address: Specifies a BGP peer by its IP address.

advertised: Displays BGP-discovered VPLS PE information advertised to the BGP peer.

received: Displays BGP-discovered VPLS PE information received from the BGP peer.

statistics: Displays BGP-discovered VPLS PE statistics.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

pe-address ip-address: Specifies a PE by its IP address.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all VPLS PEs discovered by BGP.

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp l2vpn auto-discovery verbose

Use display system internal bgp l2vpn auto-discovery verbose to display detailed information about a VPLS PE discovered by BGP.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery route-distinguisher route-distinguisher pe-address ip-address verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery route-distinguisher route-distinguisher pe-address ip-address verbose [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] l2vpn auto-discovery route-distinguisher route-distinguisher pe-address ip-address verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

pe-address ip-address: Specifies a PE by its IP address.

standby: Displays detailed information about a BGP-discovered VPLS PE for a standby BGP process. If you do not specify this keyword, the command displays detailed information about a BGP-discovered VPLS PE for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp l2vpn evpn

Use display system internal bgp l2vpn evpn to display BGP EVPN routing information.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] l2vpn evpn route-distinguisher route-distinguisher [ route-type { auto-discovery | es | imet | ip-prefix | mac-ip } ] evpn-route route-length verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] l2vpn evpn route-distinguisher route-distinguisher [ route-type { auto-discovery | es | imet | ip-prefix | mac-ip } ] evpn-route route-length verbose [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] l2vpn evpn [ peer ip-address { advertised-routes | received-routes } [ statistics ] | route-distinguisher route-distinguisher [ route-type { auto-discovery | es | imet | ip-prefix | mac-ip } ] [ evpn-route route-length [ advertise-info ] ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] l2vpn evpn route-distinguisher route-distinguisher [ route-type { auto-discovery | es | imet | ip-prefix | mac-ip } ] evpn-route route-length verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] l2vpn evpn [ peer ip-address { advertised-routes | received-routes } [ statistics ] | route-distinguisher route-distinguisher [ route-type { auto-discovery | es | imet | ip-prefix | mac-ip } ] [ evpn-route route-length [ advertise-info ] ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

route-type: Displays information about the specified type of BGP EVPN routes.

auto-discovery: Displays Ethernet auto-discovery route information.

es: Displays Ethernet segment route information.

imet: Displays inclusive multicast Ethernet tag route information.

ip-prefix: Displays IP prefix advertisement route information.

mac-ip: Displays MAC/IP advertisement route information.

evpn-route: Specifies a BGP EVPN route, a string of 1 to 512 characters.

route-length: Specifies the route length in the range of 0 to 65535 bits.

verbose: Displays detailed BGP EVPN route information.

standby: Displays BGP EVPN routing information for a standby BGP process. If you do not specify this keyword, the command displays BGP EVPN routing information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

peer ip-address: Specifies a peer by its IP address.

advertised-routes: Displays advertised BGP EVPN route information.

received-routes: Displays received BGP EVPN route information.

statistics: Displays BGP EVPN route statistics.

advertise-info: Displays BGP EVPN route advertisement information.

BGP probe commands -- display system internal bgp l2vpn signaling advertise-info

Use display system internal bgp l2vpn signaling advertise-info to display BGP L2VPN label block advertisement information.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] l2vpn signaling route-distinguisher route-distinguisher site-id site-id label-offset label-offset advertise-info

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] l2vpn signaling route-distinguisher route-distinguisher site-id site-id label-offset label-offset advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] l2vpn signaling route-distinguisher route-distinguisher site-id site-id label-offset label-offset advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

site-id site-id: Specifies a site by its ID. The site ID range depends on the device model.

label-offset label-offset: Specifies an offset in the range of 0 to 65535.

standby: Displays BGP L2VPN label block advertisement information for a standby BGP process. If you do not specify this keyword, the command displays BGP L2VPN label block advertisement information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp l2vpn signaling standby

Use display system internal bgp l2vpn signaling standby to display MPLS L2VPN label block information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] l2vpn signaling [ peer ip-address { advertised | received } [ statistics ] | route-distinguisher route-distinguisher [ site-id site-id [ label-offset label-offset ] ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] l2vpn signaling [ peer ip-address { advertised | received } [ statistics ] | route-distinguisher route-distinguisher [ site-id site-id [ label-offset label-offset ] ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

peer ip-address: Specifies a BGP peer by its IP address.

advertised: Displays MPLS L2VPN label block information advertised to the BGP peer.

received: Displays MPLS L2VPN label block information received from the BGP peer.

statistics: Displays MPLS L2VPN label block statistics.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

site-id site-id: Displays MPLS L2VPN label block information for a site specified by its ID. The site ID range varies by device model.

label-offset label-offset: Displays information about the MPLS L2VPN label block with an offset in the range of 0 to 65535.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all MPLS L2VPN label blocks.

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp l2vpn signaling verbose

Use display system internal bgp l2vpn signaling verbose to display detailed BGP L2VPN label block information.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] l2vpn signaling route-distinguisher route-distinguisher site-id site-id label-offset label-offset verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] l2vpn signaling route-distinguisher route-distinguisher site-id site-id label-offset label-offset verbose [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] l2vpn signaling route-distinguisher route-distinguisher site-id site-id label-offset label-offset verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

site-id site-id: Specifies a site by its ID. The site ID range depends on the device model.

label-offset label-offset: Specifies an offset in the range of 0 to 65535.

standby: Displays detailed BGP L2VPN label block information for a standby BGP process. If you do not specify this keyword, the command displays detailed BGP L2VPN label block information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp link-state

Use display system internal bgp link-state to display link state information advertised by an IGP and information about communication between BGP and IGP.

Syntax

display system internal bgp [ instance instance-name ] link-state ipc

display system internal bgp [ instance instance-name ] link-state log { control | data }

display system internal bgp [ instance instance-name ] link-state [ link | node | prefix | statistics ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

ipc: Displays status information for communication between BGP and IGP.

log: Displays log information for communication between BGP and IGP.

control: Displays control log information.

data: Displays data log information.

link: Displays link information advertised by an IGP.

node: Displays node information advertised by an IGP.

prefix: Displays prefix information advertised by an IGP.

statistics: Displays statistics about link state messages advertised by an IGP.

Usage guidelines

If you do not specify any of the link, node, and prefix keywords, this command displays link state information that an IGP advertises to BGP. The advertised information includes link, node and prefix information.

BGP probe commands -- display system internal bgp log

Use display system internal bgp log to display log information for a BGP process.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] log [ reverse ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] log [ reverse ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] log [ reverse ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays log information for the default BGP instance.

reverse: Displays log information in reverse chronological order.

standby: Displays log information for a standby BGP process. If you do not specify this keyword, the command displays log information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

BGP probe commands -- display system internal bgp nib

Use display system internal bgp nib to display next hop information for BGP routes.

Syntax

display system internal bgp [ instance instance-name ] nib { ipv4 | ipv6 } [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays next hop information for the default BGP instance.

ipv4: Displays BGP next hop information for IPv4 address family.

ipv6: Displays BGP next hop information for IPv6 address family.

nib-id: Specifies a next hop by its ID in the range of 1 to FFFFFFFF. If you do not specify a next hop, this commands displays information about all BGP next hops.

verbose: Displays detailed next hop information. If you do not specify this keyword, the command displays brief next hop information.

BGP probe commands -- display system internal bgp nib log

Use display system internal bgp nib log to display log information for BGP next hops.

Syntax

display system internal bgp [ instance instance-name ] [ evpn ] nib log

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

evpn: Displays log information for next hops of the EVPN address family. If you do not specify this keyword, the command displays log information for all BGP next hops.

BGP probe commands -- display system internal bgp peer received prefix-list

Use display system internal bgp peer received prefix-list to display the ORF prefix information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] peer ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } ipv4-address received prefix-list standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } ipv6-address received prefix-list standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 [ unicast ] ipv4-address received prefix-list standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer { vpnv4 | vpnv6 } ipv4-address received prefix-list standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] peer ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } ipv4-address received prefix-list standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } ipv6-address received prefix-list standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 [ unicast ] ipv4-address received prefix-list standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer { vpnv4 | vpnv6 } ipv4-address received prefix-list standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

ipv4: Displays IPv4 peer information.

ipv6: Displays IPv6 peer information.

vpnv4: Displays VPNv4 peer information.

vpnv6: Displays VPNv6 peer information.

multicast: Displays multicast peer information.

unicast: Displays unicast peer information.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the public network.

ipv4-address: Specifies a peer by its IPv4 address.

ipv6-address: Specifies a peer by its IPv6 address.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

BGP probe commands -- display system internal bgp peer standby

Use display system internal bgp peer standby to display BGP peer information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] peer ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ [ ipv4-address ] verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ [ ipv6-address ] verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 [ unicast ] [ [ ipv4-address ] verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer vpnv4 [ vpn-instance vpn-instance-name ] [ [ ipv4-address ] verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer { l2vpn [ evpn ] | vpnv6 } [ [ ipv4-address ] verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv4 rtfilter [ [ ipv4-address ] verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] peer ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ [ ipv4-address ] verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ [ ipv6-address ] verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv6 [ unicast ] [ [ ipv4-address ] verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer vpnv4 [ vpn-instance vpn-instance-name ] [ [ ipv4-address ] verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer { l2vpn [ evpn ] | vpnv6 } [ [ ipv4-address ] verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] peer ipv4 rtfilter [ [ ipv4-address ] verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP peer information for the default BGP instance.

ipv4: Displays IPv4 BGP peer information.

ipv6: Displays IPv6 BGP peer information.

vpnv4: Displays BGP VPNv4 peer information.

l2vpn: Displays BGP L2VPN peer information.

evpn: Displays BGP EVPN peer information.

vpnv6: Displays BGP VPNv6 peer information.

multicast: Displays BGP multicast peer information.

unicast: Displays BGP unicast peer information.

rtfilter: Displays BGP RT filter peer information.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP peer information for the public network.

ipv4-address: Specifies a peer by its IPv4 address. If you do not specify this argument, the command displays information about all BGP peers.

ipv6-address: Specifies a peer by its IPv6 address. If you do not specify this argument, the command displays information about all BGP peers.

verbose: Displays detailed BGP peer information. If you do not specify this keyword, the command displays brief BGP peer information.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The unicast keyword is used if you specify neither the unicast nor the multicast keyword.

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp peer statistics

Use display system internal bgp peer statistics to display BGP peer statistics.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] peer { ipv4 | vpnv4 } [ vpn-instance vpn-instance-name ] ipv4-address [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer ipv6 { ipv4-address | [ vpn-instance vpn-instance-name ] ipv6-address } [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer vpnv6 ipv6-address [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer l2vpn [ evpn ] ipv4-address [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer ipv4 mdt ipv4-address [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer ipv4 multicast ipv4-address [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer ipv6 multicast ipv6-address [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer link-state { ipv4-address | ipv6-address } [ rib | send | session ] statistics

display system internal bgp [ instance instance-name ] peer ipv4 rtfilter ipv4-address [ rib | send | session ] statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] peer { ipv4 | vpnv4 } [ vpn-instance vpn-instance-name ] ipv4-address [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv6 { ipv4-address | [ vpn-instance vpn-instance-name ] ipv6-address } [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer vpnv6 ipv6-address [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer l2vpn [ evpn ] ipv4-address [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv4 multicast ipv4-address [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv6 multicast ipv6-address [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer link-state { ipv4-address | ipv6-address } [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv4 rtfilter ipv4-address [ rib | send | session ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] peer { ipv4 | vpnv4 } [ vpn-instance vpn-instance-name ] ipv4-address [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv6 { ipv4-address | [ vpn-instance vpn-instance-name ] ipv6-address } [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer vpnv6 ipv6-address [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer l2vpn [ evpn ] ipv4-address [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv4 multicast ipv4-address [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv6 multicast ipv6-address [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer link-state { ipv4-address | ipv6-address } [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] peer ipv4 rtfilter ipv4-address [ rib | send | session ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP peer statistics for the default BGP instance.

ipv4: Displays BGP peer statistics for IPv4 address family.

ipv6: Displays BGP peer statistics for IPv6 address family.

vpnv4: Displays BGP peer statistics for VPNv4 address family.

vpnv6: Displays BGP peer statistics for VPNv6 address family.

l2vpn: Displays BGP peer statistics for L2VPN address family.

evpn: Displays BGP peer statistics for EVPN address family.

mdt: Displays BGP peer statistics for MDT address family.

multicast: Displays BGP peer statistics for multicast address family.

link-state: Displays BGP peer statistics for LS address family.

rtfilter: Displays BGP peer statistics for RT filter address family.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP peer statistics for the public network.

ipv4-address: Specifies a BGP peer by its IPv4 address.

ipv6-address: Specifies a BGP peer by its IPv6 address.

rib: Displays BGP route module information.

send: Displays BGP sending module information.

session: Displays BGP session module information.

standby: Displays BGP peer statistics for a standby BGP process. If you do not specify a standby BGP process, this command displays BGP peer statistics for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify the rib keyword, the send keyword, or the session keyword, this command displays peer statistics for the BGP protocol.

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp protocol statistics

Use display system internal bgp protocol statistics to display statistics for a BGP module.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] protocol [ bmp | calc | rib | send | session [ thread-id ] ] statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] protocol [ bmp | calc | rib | send | session [ thread-id ] ] statistics [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] protocol [ bmp | calc | rib | send | session [ thread-id ] ] statistics [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays statistics for the default BGP instance.

bmp: Displays statistics for the BGP monitoring module.

calc: Displays statistics for the BGP route comparison module.

rib: Displays statistics for the BGP route module.

send: Displays statistics for the BGP sending module.

session thread-id: Displays statistics for the BGP session module. The thread-id argument specifies a session thread by its ID in the range of 0 to 255.

standby: Displays BGP module statistics for a standby BGP process. If you do not specify a standby BGP process, this command displays BGP module statistics for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify any keywords, this command displays statistics for the BGP protocol.

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp routing-table advertise-info

Use display system internal bgp routing-table advertise-info to display BGP route advertisement information.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ vpn-instance vpn-instance-name ] ipv4-address { mask-length | mask } advertise-info

display system internal bgp [ instance instance-name ] routing-table ipv6 [ vpn-instance vpn-instance-name ] ipv6-address prefix-length advertise-info

display system internal bgp [ instance instance-name ] routing-table vpnv4 ipv4-address { mask-length | mask } advertise-info

display system internal bgp [ instance instance-name ] routing-table vpnv6 ipv6-address prefix-length advertise-info

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast ipv4-address { mask-length | mask } advertise-info

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast ipv6-address prefix-length advertise-info

display system internal bgp [ instance instance-name ] routing-table ipv4 rtfilter [ origin-as as-number ] route-target advertise-info

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ vpn-instance vpn-instance-name ] ipv4-address { mask-length | mask } advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 [ vpn-instance vpn-instance-name ] ipv6-address prefix-length advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv4 ipv4-address { mask-length | mask } advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv6 ipv6-address prefix-length advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast ipv4-address { mask-length | mask } advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast ipv6-address prefix-length advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 rtfilter [ origin-as as-number ] route-target advertise-info [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ vpn-instance vpn-instance-name ] ipv4-address { mask-length | mask } advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 [ vpn-instance vpn-instance-name ] ipv6-address prefix-length advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv4 ipv4-address { mask-length | mask } advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv6 ipv6-address prefix-length advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast ipv4-address { mask-length | mask } advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast ipv6-address prefix-length advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 rtfilter [ origin-as as-number ] route-target advertise-info [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP route advertisement information for the default BGP instance.

ipv4: Displays BGP route advertisement information for IPv4 address family.

ipv6: Displays BGP route advertisement information for IPv6 address family.

vpnv4: Displays BGP route advertisement information for VPNv4 address family.

vpnv6: Displays BGP route advertisement information for VPNv6 address family.

multicast: Displays BGP route advertisement information for multicast address family.

rtfilter: Displays BGP route advertisement information for RT filter address family.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP route advertisement information for the public network.

ipv4-address: Specifies an IPv4 destination network address.

mask-length: Specifies a mask length for the destination network address, in the range of 0 to 32.

mask: Specifies a mask for the destination network address, in dotted decimal notation.

ipv6-address: Specifies an IPv6 destination network address.

prefix-length: Specifies a prefix length for the destination network address, in the range of 0 to 128.

origin-as as-number: Specifies an origin AS by its number.

route-target: Specifies an RT, a string of 3 to 21 characters.

An RT has the following formats:

· 16-bit AS number:32-bit user-defined number. For example, 101:3.

· 32-bit IP address:16-bit user-defined number. For example, 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, where the minimum value of the AS number is 65536. For example, 65536:1.

advertise-info: Displays advertisement information for BGP IPv4 RT filter routes.

standby: Displays BGP route advertisement for a standby BGP process. If you do not specify a standby BGP process, this command displays BGP route advertisement for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp routing-table ipv4 multicast standby

Use display system internal bgp routing-table ipv4 multicast standby to display BGP IPv4 multicast routing information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast [ ip-address [ { mask-length | mask } [ longest-match ] ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ip-address { advertised-routes | received-routes } [ ip-address [ mask-length | mask ] | statistics ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast [ ip-address [ { mask-length | mask } [ longest-match ] ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ip-address { advertised-routes | received-routes } [ ip-address [ mask-length | mask ] | statistics ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP IPv4 multicast routing information for the default BGP instance.

ip-address: Specifies a destination network address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

longest-match: Specifies longest match mode, which selects the longest matching route through the following steps:

1. ANDs the specified network address with the mask of each route.

2. Matches a route if the AND result is the same as the network address of the route and the mask of the route is shorter than or equal to the specified mask.

3. Selects the route with the longest mask among the matching routes.

as-path-acl as-path-acl-number: Displays BGP IPv4 multicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv4 multicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays BGP IPv4 multicast routes exactly matching the specified community list. If you do not specify this keyword, the command displays BGP IPv4 multicast routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer ip-address: Displays BGP IPv4 multicast routing information advertised to or received from the specified peer.

advertised-routes: Displays BGP IPv4 multicast routing information advertised to the specified peer.

received-routes: Displays BGP IPv4 multicast routing information received from the specified peer.

statistics: Displays routing statistics.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all BGP IPv4 multicast routes.

If you specify only the ip-address argument, the system ANDs the network address with the mask of a route. If the result matches the network address of the route, this command displays information about the route.

If you specify the ip-address mask or ip-address mask-length argument but do not specify the longest-match keyword, this command displays information about the BGP IPv4 multicast route that matches both the specified destination network address and the mask (or mask length).

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp routing-table ipv4 unicast outlabel standby

Use display system internal bgp routing-table ipv4 unicast outlabel standby to display outgoing labels of BGP IPv4 unicast routes for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ unicast ] [ vpn-instance vpn-instance-name ] outlabel standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ unicast ] [ vpn-instance vpn-instance-name ] outlabel standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays outgoing labels of BGP IPv4 unicast routes for the public network.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

This command displays outgoing labels of BGP IPv4 unicast routes regardless of whether the unicast keyword is specified or not.

BGP probe commands -- display system internal bgp routing-table ipv4 unicast standby

Use display system internal bgp routing-table ipv4 unicast standby to display BGP IPv4 unicast routing information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ unicast ] [ vpn-instance vpn-instance-name ] [ ip-address [ { mask-length | mask } [ longest-match ] ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ip-address { advertised-routes | received-routes } [ ip-address [ mask-length | mask ] | statistics ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ unicast ] [ vpn-instance vpn-instance-name ] [ ip-address [ { mask-length | mask } [ longest-match ] ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ip-address { advertised-routes | received-routes } [ ip-address [ mask-length | mask ] | statistics ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the BGP IPv4 unicast routing information for the public network.

ip-address: Specifies a destination network address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

longest-match: Specifies longest match mode, which selects the longest matching route through the following steps:

1. ANDs the specified network address with the mask of each route.

2. Matches a route if the AND result is the same as the network address of the route and the mask of the route is shorter than or equal to the specified mask.

3. Selects the route with the longest mask among the matching routes.

as-path-acl as-path-acl-number: Displays BGP IPv4 unicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv4 unicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays routes exactly matching the specified community list. If you do not specify this keyword, the command displays routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer ip-address: Displays BGP IPv4 unicast routing information advertised to or received from the specified peer.

advertised-routes: Displays routing information advertised to the specified peer.

received-routes: Displays routing information received from the specified peer.

statistics: Displays routing statistics.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all BGP IPv4 unicast routes.

If you specify only the ip-address argument, the system ANDs the network address with the mask of a route. If the result matches the network address of the route, this command displays information about the route.

If you specify the ip-address mask or ip-address mask-length argument but do not specify the longest-match keyword, this command displays information about the BGP IPv4 unicast route that matches both the specified destination network address and the mask (or mask length).

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

This command displays BGP IPv4 unicast routing information regardless of whether the unicast keyword is specified or not.

BGP probe commands -- display system internal bgp routing-table ipv6 multicast standby

Use display system internal bgp routing-table ipv6 multicast standby to display BGP IPv6 multicast routing information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast [ ipv6-address prefix-length | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv6-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast [ ipv6-address prefix-length | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv6-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

ipv6-address prefix-length: Specifies the destination network address and prefix length. The value range for the prefix-length argument is 0 to 128. If you do not specify this argument, the command displays brief information about all BGP IPv6 multicast routes.

as-path-acl as-path-acl-number: Displays BGP IPv6 multicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv6 multicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays BGP IPv6 multicast routes exactly matching the specified community list. If you do not specify this keyword, the command displays BGP IPv6 multicast routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer: Displays BGP IPv6 multicast routing information advertised to or received from the specified peer.

ipv6-address: Specifies the peer IPv6 address.

advertised-routes: Displays BGP IPv6 multicast routing information advertised to the specified peer.

received-routes: Displays BGP IPv6 multicast routing information received from the specified peer.

statistics: Displays routing statistics.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp routing-table ipv6 unicast outlabel standby

Use display system internal bgp routing-table ipv6 unicast outlabel standby to display outgoing labels of BGP IPv6 unicast routes for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv6 [ unicast ] outlabel standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv6 [ unicast ] outlabel standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

This command displays outgoing labels of BGP IPv6 unicast routes regardless of whether the unicast keyword is specified or not.

BGP probe commands -- display system internal bgp routing-table ipv6 unicast standby

Use display system internal bgp routing-table ipv6 unicast standby to display BGP IPv6 unicast routing information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv6 [ unicast ] [ vpn-instance vpn-instance-name ] [ ipv6-address prefix-length | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv6-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ] standby slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] routing-table ipv6 [ unicast ] peer ipv4-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv6 [ unicast ] [ vpn-instance vpn-instance-name ] [ ipv6-address prefix-length | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv6-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal bgp [ instance instance-name ] routing-table ipv6 [ unicast ] peer ipv4-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the BGP IPv6 unicast routing information for the public network.

ipv6-address prefix-length: Specifies the destination network address and prefix length. The value range for the prefix-length argument is 0 to 128. If you do not specify this argument, the command displays brief information about all BGP IPv6 unicast routes.

as-path-acl as-path-acl-number: Displays BGP IPv6 unicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv6 unicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays routes exactly matching the specified community list. If you do not specify this keyword, the command displays routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer: Displays BGP IPv6 unicast routing information advertised to or received from the specified peer.

ipv4-address: Specifies the peer IPv4 address.

ipv6-address: Specifies the peer IPv6 address.

advertised-routes: Displays routing information advertised to the specified peer.

received-routes: Displays routing information received from the specified peer.

statistics: Displays routing statistics.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

This command displays BGP IPv6 unicast routing information regardless of whether the unicast keyword is specified or not.

BGP probe commands -- display system internal bgp routing-table verbose

Use display system internal bgp routing-table verbose to display detailed BGP routing information.

Syntax

Centralized devices:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ vpn-instance vpn-instance-name ] ipv4-address { mask-length | mask } verbose

display system internal bgp [ instance instance-name ] routing-table ipv6 [ vpn-instance vpn-instance-name ] ipv6-address prefix-length verbose

display system internal bgp [ instance instance-name ] routing-table vpnv4 ipv4-address { mask-length | mask } verbose

display system internal bgp [ instance instance-name ] routing-table vpnv6 ipv6-address prefix-length verbose

display system internal bgp [ instance instance-name ] routing-table ipv4 mdt ipv4-address verbose

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast ipv4-address { mask-length | mask } verbose

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast ipv6-address prefix-length verbose

display system internal bgp [ instance instance-name ] routing-table ipv4 rtfilter ipv4-address [ origin-as as-number ] route-target verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ vpn-instance vpn-instance-name ] ipv4-address { mask-length | mask } verbose [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 [ vpn-instance vpn-instance-name ] ipv6-address prefix-length verbose [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv4 ipv4-address { mask-length | mask } verbose [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv6 ipv6-address prefix-length verbose [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast ipv4-address { mask-length | mask } verbose [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast ipv6-address prefix-length verbose [ standby slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 rtfilter ipv4-address [ origin-as as-number ] route-target verbose [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table ipv4 [ vpn-instance vpn-instance-name ] ipv4-address { mask-length | mask } verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 [ vpn-instance vpn-instance-name ] ipv6-address prefix-length verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv4 ipv4-address { mask-length | mask } verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table vpnv6 ipv6-address prefix-length verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 multicast ipv4-address { mask-length | mask } verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv6 multicast ipv6-address prefix-length verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal bgp [ instance instance-name ] routing-table ipv4 rtfilter ipv4-address [ origin-as as-number ] route-target verbose [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

ipv4: Displays detailed BGP routing information for IPv4 address family.

ipv6: Displays detailed BGP routing information for IPv6 address family.

vpnv4: Displays detailed BGP routing information for VPNv4 address family.

vpnv6: Displays detailed BGP routing information for VPNv6 address family.

mdt: Displays detailed BGP routing information for MDT address family.

multicast: Displays detailed BGP routing information for multicast address family.

rtfilter: Displays detailed BGP routing information for RT filter address family.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays detailed BGP routing information for the public network.

ipv4-address: Specifies an IPv4 destination network address.

mask-length: Specifies a mask length for the destination network address, in the range of 0 to 32.

mask: Specifies a mask for the destination network address, in dotted decimal notation.

ipv6-address: Specifies an IPv6 destination network address.

prefix-length: Specifies a prefix length for the destination network address, in the range of 0 to 128.

origin-as as-number: Specifies an origin AS by its number.

route-target: Specifies an RT, a string of 3 to 21 characters.

An RT has the following formats:

· 16-bit AS number:32-bit user-defined number. For example, 101:3.

· 32-bit IP address:16-bit user-defined number. For example, 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, where the minimum value of the AS number is 65536. For example, 65536:1.

advertise-info: Displays advertisement information for BGP IPv4 RT filter routes.

standby: Displays detailed BGP routing information for a standby BGP process. If you do not specify a standby BGP process, this command displays detailed BGP routing information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything when you execute it with the standby keyword.

BGP probe commands -- display system internal bgp routing-table vpnv4 outlabel standby

Use display system internal bgp routing-table vpnv4 outlabel standby to display outgoing labels of BGP VPNv4 routes for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table vpnv4 outlabel standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table vpnv4 outlabel standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp routing-table vpnv4 standby

Use display system internal bgp routing-table vpnv4 standby to display BGP VPNv4 routing information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table vpnv4 [ [ route-distinguisher route-distinguisher ] [ ip-address [ { mask-length | mask } [ longest-match ] ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } ] | [ vpn-instance vpn-instance-name ] peer ip-address { advertised-routes | received-routes } [ ip-address [ mask-length | mask ] | statistics ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table vpnv4 [ [ route-distinguisher route-distinguisher ] [ ip-address [ { mask-length | mask } [ longest-match ] ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } ] | [ vpn-instance vpn-instance-name ] peer ip-address { advertised-routes | received-routes } [ ip-address [ mask-length | mask ] | statistics ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

ip-address: Specifies a destination network address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

longest-match: Specifies longest match mode, which selects the longest matching route through the following steps:

1. ANDs the specified network address with the mask of each route.

2. Matches a route if the AND result is the same as the network address of the route and the mask of the route is shorter than or equal to the specified mask.

3. Selects the route with the longest mask among the matching routes.

as-path-acl as-path-acl-number: Displays BGP VPNv4 routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP VPNv4 routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays BGP VPNv4 routes exactly matching the specified community list. If you do not specify this keyword, the command displays BGP VPNv4 routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP VPNv4 routing information for the public network.

peer: Displays BGP VPNv4 routing information advertised to or received from the specified peer.

ip-address: Specifies the peer IP address.

advertised-routes: Displays BGP VPNv4 routing information advertised to the specified peer.

received-routes: Displays BGP VPNv4 routing information received from the specified peer.

statistics: Displays routing statistics.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all BGP VPNv4 routes.

If you specify the ip-address mask or ip-address mask-length argument but do not specify the longest-match keyword, this command displays information about the BGP VPNv4 route that matches both the specified destination network address and the mask (or mask length).

If you specify only the ip-address argument, the system ANDs the network address with the mask of a route. If the result matches the network address of the route, this command displays information about the route.

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp routing-table vpnv6 outlabel standby

Use display system internal bgp routing-table vpnv6 outlabel standby to display outgoing labels of BGP VPNv6 routes for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table vpnv6 outlabel standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table vpnv6 outlabel standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgp routing-table vpnv6 standby

Use display system internal bgp routing-table vpnv6 standby to display BGP VPNv6 routing information for a standby BGP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgp [ instance instance-name ] routing-table vpnv6 [ [ route-distinguisher route-distinguisher ] [ ipv6-address prefix-length | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } ] | peer ipv4-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal bgp [ instance instance-name ] routing-table vpnv6 [ [ route-distinguisher route-distinguisher ] [ ipv6-address prefix-length | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } ] | peer ipv4-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

route-distinguisher route-distinguisher: Specifies a route distinguisher (RD), a string of 3 to 21 characters. You can specify an RD in one of the following formats:

· 16-bit AS number:32-bit user-defined number, such as 101:3.

· 32-bit IP address:16-bit user-defined number, such as 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, such as 65536:1. In this format, the minimum value for the AS number is 65536.

ipv6-address prefix-length: Specifies the destination network address and prefix length. The value range for the prefix-length argument is 0 to 128. If you do not specify this argument, the command displays brief information about all BGP VPNv6 routing information.

as-path-acl as-path-acl-number: Displays BGP VPNv6 routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP VPNv6 routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays BGP VPNv6 routes exactly matching the specified community list. If you do not specify this keyword, the command displays BGP VPNv6 routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer: Displays BGP VPNv6 routing information advertised to or received from the specified peer.

ipv4-address: Specifies the peer IPv4 address.

advertised-routes: Displays BGP VPNv6 routing information advertised to the specified peer.

received-routes: Displays BGP VPNv6 routing information received from the specified peer.

statistics: Displays routing statistics.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

The active BGP process backs up BGP peers and routing information to the standby BGP process only when BGP NSR is enabled. If BGP NSR is disabled, this command does not display anything.

BGP probe commands -- display system internal bgpm log

Use display system internal bgpm log to display log information for a BGP management process.

Syntax

Centralized devices:

display system internal bgpm log [ reverse ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bgpm log [ reverse ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bgpm log [ reverse ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

reverse: Displays log information in reverse chronological order.

standby: Displays BGP log information for a standby BGP process. If you do not specify a standby BGP process, this command displays information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

BGP probe commands -- reset system internal bgp link-state

Use reset system internal bgp link-state to clear statistics about link state messages advertised by an IGP and log information for communication between BGP and IGP.

Syntax

reset system internal bgp [ instance instance-name ] link-state log { control | data }

reset system internal bgp [ instance instance-name ] link-state statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command clears information for the default BGP instance.

log: Clears log information for communication between BGP and IGP.

control: Clears control log information.

data: Clears data log information.

statistics: Clears statistics about link state messages advertised by an IGP.

BGP probe commands -- reset system internal bgp log

Use reset system internal bgp log to clear log information for a BGP process.

Syntax

Centralized devices:

reset system internal bgp [ instance instance-name ] log

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal bgp [ instance instance-name ] log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal bgp [ instance instance-name ] log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command clears log information for the default BGP instance.

standby: Clears BGP log information for a standby BGP process. If you do not specify a standby BGP process, this command clears log information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

BGP probe commands -- reset system internal bgpm log

Use reset system internal bgpm log to clear log information for a BGP management process.

Syntax

Centralized devices:

reset system internal bgpm log

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal bgpm log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal bgpm log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

standby: Clears BGP log information for a standby BGP process. If you do not specify a standby BGP process, this command clears log information for the active BGP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.