SMA probe commands -- display system internal sma-anti-spoof ipv6 address-prefix

Use display system internal sma-anti-spoof ipv6 address-prefix to display IPv6 prefix information.

Syntax

Centralized devices:

display system internal sma-anti-spoof ipv6 address-prefix [ ipv6-address ipv6-prefix-length ]

Centralized IRF devices—Distributed devices—In standalone mode:

display system internal sma-anti-spoof ipv6 address-prefix [ ipv6-address ipv6-prefix-length ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices—In IRF mode:

display system internal sma-anti-spoof ipv6 address-prefix [ ipv6-address ipv6-prefix-length ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address ipv6-prefix-length: Specifies an IPv6 address with a prefix length in the range of 0 to 128.

slot slot-number: Specifies a card by its slot number. If you do not specify a slot, this command displays IPv6 prefix information for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv6 prefix information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays IPv6 prefix information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv6 prefix information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays IPv6 prefix information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

SMA probe commands -- display system internal sma-anti-spoof ipv6 packet-tag

Use display system internal sma-anti-spoof ipv6 packet-tag to display SMA tag information.

Syntax

Centralized devices:

display system internal sma-anti-spoof ipv6 packet-tag [ source-as-number destination-as-number ]

Centralized IRF devices—Distributed devices—In standalone mode:

display system internal sma-anti-spoof ipv6 packet-tag [ source-as-number destination-as-number ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices—In IRF mode:

display system internal sma-anti-spoof ipv6 packet-tag [source-as-number destination-as-number ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

source-as-number destination-as-number: Specifies an AS pair by its source and destination AS numbers. The AS number is in the range of 0 to 4294967295. If you do not specify an AS pair, this command displays SMA tag information for all AS pairs.

slot slot-number: Specifies a card by its slot number. If you do not specify a slot, this command displays SMA tag information for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays SMA tag information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays SMA tag information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays SMA tag information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays SMA tag information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.