Basic IPv6 settings probe commands -- display system internal ipv6 rawip

| NOTE: Support for this command depends on the device model.

Use display system internal ipv6 rawip to display brief information about IPv6 RawIP connections.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 rawip slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 rawip chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IPv6 settings probe commands -- display system internal ipv6 tcp

| NOTE: Support for this command depends on the device model.

Use display system internal ipv6 tcp to display brief information about IPv6 TCP connections.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 tcp slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 tcp chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IPv6 settings probe commands -- display system internal ipv6 tcp port-info

| NOTE: Support for this command depends on the device model.

Use display system internal ipv6 tcp port-info to display non-well-known TCP port usage in IPv6.

Syntax

Centralized devices:

display system internal ipv6 tcp port-info

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 tcp port-info [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 tcp port-info [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays non-well-known TCP port usage for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays non-well-known TCP port usage for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays non-well-known TCP port usage for all member devices if you do not specify a member device. On an IRF 3 system, this command displays usage information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. If you do not specify a card, this command displays non-well-known TCP port usage for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays non-well-known TCP port usage for all cards if you do not specify a card. On an IRF 3 system, this command displays usage information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IPv6 settings probe commands -- display system internal ipv6 tcp-proxy verbose

| NOTE: Support for this command depends on the device model.

Use display system internal ipv6 tcp-proxy verbose to display detailed information about IPv6 TCP proxy.

Syntax

Centralized devices:

display system internal ipv6 tcp-proxy verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 tcp-proxy verbose slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 tcp-proxy verbose chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IPv6 settings probe commands -- display system internal ipv6 udp

| NOTE: Support for this command depends on the device model.

Use display system internal ipv6 udp to display brief information about IPv6 UDP connections.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 udp slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 udp chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IPv6 settings probe commands -- display system internal ipv6 udp port-info

| NOTE: Support for this command depends on the device model.

Use display system internal ipv6 udp port-info to display non-well-known UDP port usage in IPv6.

Syntax

Centralized devices:

display system internal ipv6 udp port-info

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 udp port-info [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 udp port-info [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays non-well-known UDP port usage for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays non-well-known UDP port usage for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays non-well-known UDP port usage for all member devices if you do not specify a member device. On an IRF 3 system, this command displays usage information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. If you do not specify a card, this command displays non-well-known UDP port usage for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays non-well-known UDP port usage for all cards if you do not specify a card. On an IRF 3 system, this command displays usage information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IPv6 settings probe commands -- display system internal tcp-proxy statistics

| NOTE: Support for this command depends on the device model.

Use display system internal tcp-proxy statistics to display TCP proxy statistics about IPv4 and IPv6 TCP connections.

Syntax

Centralized devices:

display system internal tcp-proxy statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal tcp-proxy statistics { all | api | error | fsm | packet } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal tcp-proxy statistics { all | api | error | fsm | packet } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Displays all TCP proxy statistics.

api: Displays statistics about API calls.

error: Displays statistics about error packets.

fsm: Displays statistics about finite state machine (FSM) packets.

packet: Displays statistics about input and output TCP packets.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays TCP proxy statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays TCP proxy statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays TCP proxy statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command displays TCP proxy statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. If you do not specify a card, this command displays TCP proxy statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays TCP proxy statistics for all cards if you do not specify a card. On an IRF 3 system, this command displays TCP proxy statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IPv6 settings probe commands -- reset system internal tcp-proxy statistics

Use reset system internal tcp-proxy statistics to clear TCP proxy statistics for IPv4 and IPv6 connections.

Syntax

reset system internal tcp-proxy statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IPv6 settings probe commands -- tcp-proxy statistics

| NOTE: Support for this command depends on the device model.

Use tcp-proxy statistics to turn on or off the counters for TCP proxy.

Syntax

tcp-proxy statistics { off | on }

Default

Counters are turned off for TCP proxy.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

off: Turns off the counters for TCP proxy.

on: Turns on the counters for TCP proxy.

Usage guidelines

The TCP proxy counters collect information about the numbers of API calls, input and output TCP packets, error packets, and FSM packets.

ND probe commands -- debugging system internal nd

Use debugging system internal nd to enable ND debugging.

Use undo debugging system internal nd to disable ND debugging.

Syntax

debugging system internal nd { notify | sync }

undo debugging system internal nd { notify | sync }

Default

ND debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

notify: Enables ND notification debugging.

sync: Enables ND synchronization debugging.

ND probe commands -- debugging system internal nd sub-features

Use debugging system internal nd sub-features { all | event | packet } to enable ND sub-feature debugging.

Use undo debugging system internal nd sub-features to disable ND sub-feature debugging.

Syntax

debugging system internal nd sub-features { all | event | packet }

undo debugging system internal nd sub-features

Default

ND sub-feature debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of ND sub-feature debugging.

event: Enables ND sub-feature event debugging.

packet: Enables ND sub-feature packet debugging.

ND probe commands -- display system internal nd dad

Use display system internal nd dad to display DAD link information.

Syntax

Centralized devices:

display system internal nd dad

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd dad slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd dad chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd entry

Use display system internal nd entry to display ND entries.

Syntax

Centralized devices:

display system internal nd entry

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd entry slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd entry chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd ifcb

Use display system internal nd ifcb to display ND control block information for an interface.

Syntax

Centralized devices:

display system internal nd ifcb interface interface-type interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd ifcb interface interface-type interface-number slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd ifcb interface interface-type interface-number chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd machash

Use display system internal nd machash to display ND machash entries.

Syntax

Centralized devices:

display system internal nd machash { vlan vlan-id | vsi vsi-name } ipv6-address

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd machash { vlan vlan-id | vsi vsi-name } ipv6-address slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd machash { vlan vlan-id | vsi vsi-name } ipv6-address chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Displays ND machash entries for the specified VLAN.

vsi vsi-name: Displays ND machash entries for the specified VSI. The vsi-name argument specifies an VSI by its name, a case-sensitive string of 1 to 31 characters.

ipv6-address: Displays ND machash entries for the specified IPv6 address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd probe

Use display system internal nd probe to display ND probe link information.

Syntax

Centralized devices:

display system internal nd probe

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd probe slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd probe chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd rbhash

Use display system internal nd rbhash to display information about the rbhash entries on a card.

Syntax

Centralized devices:

display system internal nd rbhash vlan vlan-id ipv6-address

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd rbhash vlan vlan-id ipv6-address slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd rbhash vlan vlan-id ipv6-address chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its ID.

ipv6-address: Specifies an IPv6 address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd reload

Use display system internal nd reload to display ND reload link information.

Syntax

Centralized devices:

display system internal nd reload

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd reload slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd reload chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd rule

Use display system internal nd rule to display ND rule information.

Syntax

Centralized devices:

display system internal nd rule { all | interface interface-type interface-number [ ipv6-address ] }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd rule { all | interface interface-type interface-number [ ipv6-address ] } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd rule { all | interface interface-type interface-number [ ipv6-address ] } chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Displays information about all ND rules.

interface interface-type interface-number: Specifies an interface by its type and number.

ipv6-address: Specifies an IPv6 address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd snooping

Use display system internal nd snooping to display ND snooping entries.

Syntax

Centralized devices:

display system internal nd snooping [ count | global | link-local ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd snooping slot slot-number [ cpu cpu-number ] [ count | global | link-local ]

Distributed devices in IRF mode:

display system internal nd snooping chassis chassis-number slot slot-number [ cpu cpu-number ] [ count | global | link-local ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays the total number of ND snooping entries.

global: Displays ND snooping entries for IPv6 global unicast addresses.

link-local: Displays ND snooping entries for IPv6 link-local addresses.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd static

Use display system internal nd static to display static ND entries.

Syntax

display system internal nd static ipv6-address interface interface-type interface-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Displays static ND entries for a specified IPv6 address.

interface interface-type interface-number: Specifies an interface by its type and number.

ND probe commands -- display system internal nd statistics

Use display system internal nd statistics to display ND statistics.

Syntax

Centralized devices:

display system internal nd statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- display system internal nd suppression xconnect-group verbose

Use display system internal nd suppression xconnect-group verbose to display detailed information about ND suppression entries.

Syntax

Centralized devices:

display system internal nd suppression xconnect-group verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd suppression xconnect-group verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal nd suppression xconnect-group verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about ND suppression entries for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about ND suppression entries for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays detailed information about ND suppression entries for all member devices if you do not specify a member device. On an IRF 3 system, this command displays detailed information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about ND suppression entries for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays detailed information about ND suppression entries for all cards if you do not specify a card. On an IRF 3 system, this command displays detailed information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

ND probe commands -- reset system internal nd statistics

Use reset system internal nd statistics to clear ND statistics.

Syntax

Centralized devices:

reset system internal nd statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal nd statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal nd statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command clears ND statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command clears ND statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command clears ND statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command clears ND statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. If you do not specify a card, this command clears ND statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command clears ND statistics for all cards if you do not specify a card. On an IRF 3 system, this command clears ND statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IPv6 address management probe commands -- display system internal ipv6 address

Use display system internal ipv6 address to display IPv6 address detailed information.

Syntax

Centralized devices:

display system internal ipv6 address [ [ vpn-instance vpn-instance-name ] [ ipv6-address ] | [ interface interface-type interface-number [ gateway | multicast | prefix | unicast ] ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 address [ [ vpn-instance vpn-instance-name ] [ ipv6-address ] | [ interface interface-type interface-number ] ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 address [ [ vpn-instance vpn-instance-name ] [ ipv6-address ] | [ interface interface-type interface-number [ gateway | multicast | prefix | unicast ] ] ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Specifies an IPv6 address.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance to which the IPv6 address belongs.

interface interface-type interface-number: Specifies an interface by its type and number.

gateway: Displays gateway address information for the specified interface.

multicast: Displays multicast address information for the specified interface.

prefix: Displays IPv6 prefix information for the specified interface.

unicast: Displays unicast address information for the specified interface.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv6 address detailed information for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv6 address detailed information for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays IPv6 address detailed information for all member devices if you do not specify a member device. On an IRF 3 system, this command displays detailed information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv6 address detailed information for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays IPv6 address detailed information for all cards if you do not specify a card. On an IRF 3 system, this command displays detailed information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IPv6 Path MTU probe commands -- display system internal ipv6 pathmtu

Use display system internal ipv6 pathmtu to display IPv6 Path MTU information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pathmtu [ vpn-instance vpn-instance-name ] { ipv6-address | { all | dynamic | static } [ count ] } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 pathmtu [ vpn-instance vpn-instance-name ] { ipv6-address | { all | dynamic | static } [ count ] } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the IPv6 Path MTU information for the public network. Support for this option depends on the device model.

all: Displays all Path MTU information for the public network.

dynamic: Displays all dynamic Path MTU information.

static: Displays all static Path MTU information.

count: Displays the total number of Path MTU entries.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv6 Path MTU information for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv6 Path MTU information for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays IPv6 Path MTU information for all member devices if you do not specify a member device. On an IRF 3 system, this command displays IPv6 Path MTU information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv6 Path MTU information for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays IPv6 Path MTU information for all cards if you do not specify a card. On an IRF 3 system, this command displays IPv6 Path MTU information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

FIB6 probe commands -- debugging system internal ipv6 fib prefix

Use debugging system internal ipv6 fib prefix to enable IPv6 FIB prefix debugging.

Use undo debugging system internal ipv6 fib prefix to disable IPv6 FIB prefix debugging.

Syntax

Centralized devices:

debugging system internal ipv6 fib prefix { all | message | hardware }

undo debugging system internal ipv6 fib prefix { all | message | hardware }

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal ipv6 fib prefix { all | message | hardware } slot slot-number [ cpu cpu-number ]

undo debugging system internal ipv6 fib prefix { all | message | hardware } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

debugging system internal ipv6 fib prefix { all | message | hardware } chassis chassis-number slot slot-number [ cpu cpu-number ]

undo debugging system internal ipv6 fib prefix { all | message | hardware } chassis chassis-number slot slot-number [ cpu cpu-number ]

Default

IPv6 FIB prefix debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of IPv6 FIB prefix debugging.

message: Enables IPv6 FIB prefix message debugging. If you specify this keyword, the system displays the IPv6 FIB prefix obtained from the routing table or synchronized from other cards or devices.

hardware: Enables IPv6 FIB prefix hardware debugging. If you specify this keyword, the system displays the FIB6 information issued to the driver, and the returned FIB6 information from the driver.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

FIB6 probe commands -- display system internal ipv6 fib prefix

Use display system internal ipv6 fib prefix to display basic information about IPv6 FIB prefixes.

Syntax

Centralized devices:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 fib prefix [vpn-instance vpn-instance-name ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays basic information about the IPv6 FIB prefix for the public network.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

FIB6 probe commands -- display system internal ipv6 fib prefix entry-status

Use display system internal ipv6 fib prefix entry-status to display IPv6 FIB entries that fail to be set to the driver or that are aging.

Syntax

Centralized devices:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ] entry-status status

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ] entry-status status slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ] entry-status status chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information about IPv6 FIB entries for the public network.

entry-status status: Specifies the status of IPv6 FIB entries. The value of the status argument can be A or F. A indicates aging FIB entries, and F indicates the FIB entries that fail to be set to the driver.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

FIB6 probe commands -- display system internal ipv6 fib prefix ipv6-address

Use display system internal ipv6 fib prefix to display detailed information about the IPv6 FIB prefix for a specific IPv6 address.

Syntax

Centralized devices:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ] ipv6-address [ prefix-length ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ] ipv6-address [ prefix-length ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 fib prefix [ vpn-instance vpn-instance-name ] ipv6-address [ prefix-length ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays detailed information about the IPv6 FIB prefix for the public network.

ipv6-address: Specifies an IPv6 address.

prefix-length: Specifies the length of an IPv6 FIB prefix, in the range of 0 to 128.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.