WT commands -- display wlan wt

Use display wlan wt to display wireless terminator (WT) information and information about the wireless terminator units (WTUs) connected to it.

Syntax

display wlan wt { all | name wt-name }

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

all: Specifies all WTs.

name wt-name: Specifies a WT by its name, a case-insensitive string of 1 to 64 characters. The string can contain letters, digits, underscores (_), left brackets ([), right brackets (]), forward slashes (/), and hyphens (-).

Examples

# Display information about all WTs.

<Sysname> display wlan wt all

WT name : wt1

Model : WT1020

Serial ID : 219801A0SS9156G00072

WTU number : 2

Wireless Terminator Unit:

---------------------------------------------------------

WTU name Port Model Serial ID

---------------------------------------------------------

wtu1 1 WTU430 219801A0SS9156G00185

wtu2 2 WTU430 219801A0SS9156G00133

WT name : wt2

Model : WT1020

Serial ID : 219801A0SS9156G00068

WTU number : 2

Wireless Terminator Unit:

---------------------------------------------------------

WTU name Port Model Serial ID

---------------------------------------------------------

wtu3 3 WTU430 219801A0SS9156G00054

Wtu4 4 WTU430 219801A0SS9156G00167

Table 1 Command output

Fields | Description
WTU number | Number of WTUs that are connected to the WT.
Wireless Terminator Unit | WTU information
Port | Port that connects the WT to a WTU.

WT commands -- shutdown wtu-port

Use shutdown wtu-port to disable PoE for a WTU port.

Use undo shutdown wtu-port to enable PoE for a WTU port.

Syntax

shutdown wtu-port port-number

undo shutdown wtu-port port-number

Default

PoE is enabled for WTU ports.

Views

AP view

Predefined user roles

network-admin

mdc-admin

Parameters

port-number: Specifies the WTU port number. The value range varies by device model.

Usage guidelines

A WT stops power supply to the connected WTU through PoE after you disable PoE for a WTU port of the WT.

This command is configurable only when the AP is a WT.

Examples

# Disable PoE for WTU port 1.

<Sysname> system-view

[Sysname] wlan ap ap1 WT1020

[Sysname-wlan-ap-ap1] shutdown wtu-port 1

WT commands -- wt version

Use wt version to specify the WT version.

Use undo wt version to restore the default.

Syntax

wt version { 1 | 2 }

undo wt version

Default

The WT version is version 2.0.

Views

AP view

Predefined user roles

network-admin

mdc-admin

Parameters

1: Specifies version 1.0.

2: Specifies version 2.0.

Usage guidelines

This command is configurable only when the AP is a WT.

Examples

# Specify version 2.0 as the WT version.

<Sysname> system-view

[Sysname] wlan ap ap1 mode WT1020

[Sysname-wlan-ap-ap1] wt version 2