Fast forwarding probe commands -- display system internal ip fast-forwarding cache verbose

Use display system internal ip fast-forwarding cache verbose to display detailed information about the IPv4 fast forwarding table.

Syntax

Centralized devices:

display system internal ip fast-forwarding cache [ ip-address ] verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip fast-forwarding cache [ ip-address ] verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ip fast-forwarding cache [ ip-address ] verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ip-address: Displays IPv4 fast forwarding entries for the specified IPv4 address.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about the IPv4 fast forwarding table for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about the IPv4 fast forwarding table for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about the IPv4 fast forwarding table for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about the IPv6 fast forwarding table for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about the IPv4 fast forwarding table for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Fast forwarding probe commands -- display system internal ip fast-forwarding service-sequence

Use display system internal ip fast-forwarding service-sequence to display service module registration information in the fast forwarding module.

Syntax

display system internal ip fast-forwarding service-sequence

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Fast forwarding probe commands -- display system internal max-ecmp-num

Use display system internal max-ecmp-num to display the maximum number of IPv4 ECMP routes.

Syntax

Centralized devices:

display system internal max-ecmp-num

Distributed devices in standalone mode:Centralized IRF devices:

display system internal max-ecmp-num [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal max-ecmp-num [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays the maximum number of IPv4 ECMP routes for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays the maximum number of IPv4 ECMP routes for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays the maximum number of IPv4 ECMP routes for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays the maximum number of IPv4 ECMP routes for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays the maximum number of IPv4 ECMP routes for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.