Basic IP routing probe commands -- display system internal ip routing-table

Use display system internal ip routing-table to display routing table information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays routing table information for the public network. Support for this option depends on the device model.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing table information for the public network. Support for this option depends on the device model.

verbose: Displays detailed routing table information, including information about both active and inactive routes. If you do not specify this keyword, the command displays only brief information about active routes.

standby slot slot-number: Displays backup routing table information for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup routing table information for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup routing table information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ip routing-table acl

Use display system internal ip routing-table acl to display information about routes permitted by a basic ACL.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] acl ipv4-acl-number [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] acl ipv4-acl-number [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays routing information for the public network. Support for this option depends on the device model.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

ipv4-acl-number: Specifies a basic ACL by its number in the range of 2000 to 2999.

verbose: Displays detailed information about all routes permitted by the basic ACL. If you do not specify this keyword, the command displays only brief information about active routes permitted by the basic ACL.

standby slot slot-number: Displays backup information about routes permitted by the basic ACL for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup information about routes permitted by the basic ACL for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup information about routes permitted by the basic ACL for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ip routing-table ip-address

Use display system internal ip routing-table ip-address to display information about routes to a specific destination address.

Use display system internal ip routing-table ip-address1 to ip-address2 to display information about routes to a range of destination addresses.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] ip-address [ mask-length | mask ] [ longer-match ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] ip-address1 to ip-address2 [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] ip-address [ mask-length | mask ] [ longer-match ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] ip-address1 to ip-address2 [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays routing information for the public network. Support for this option depends on the device model.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

ip-address: Specifies a destination IP address in dotted decimal notation.

mask-length: Specifies the mask length, an integer in the range of 0 to 32.

mask: Specifies the subnet mask in dotted decimal notation.

longer-match: Displays the route entry with the longest mask.

ip-address1 to ip-address2: Specifies a destination IP address range.

verbose: Displays detailed routing table information, including information about both active and inactive routes. If you do not specify this keyword, the command displays brief information about active routes.

standby slot slot-number: Displays backup information about routes for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup information about routes for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup information about routes for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ip routing-table prefix-list

Use display system internal ip routing-table prefix-list to display routes permitted by an IP prefix list.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] prefix-list prefix-list-name [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] prefix-list prefix-list-name [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays routing information for the public network. Support for this option depends on the device model.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

prefix-list-name: Specifies an IP prefix list by its name, a case-sensitive string of 1 to 63 characters.

verbose: Displays detailed information about all routes permitted by the IP prefix list. If you do not specify this keyword, the command displays brief information about active routes permitted by the IP prefix list.

standby slot slot-number: Displays backup routes permitted by the IP prefix list for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup routes permitted by the IP prefix list for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup routes permitted by the IP prefix list for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ip routing-table protocol

Use display system internal ip routing-table protocol to display information about routes installed by a protocol.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] protocol protocol [ inactive | verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] protocol protocol [ inactive | verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays routing information for the public network. Support for this option depends on the device model.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

protocol: Specifies a routing protocol.

inactive: Displays information about inactive routes. If you do not specify this keyword, the command displays information about both active and inactive routes.

verbose: Displays detailed routing table information. If you do not specify this keyword, the command displays brief routing information.

standby slot slot-number: Displays backup information about routes installed by the protocol for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup information about routes installed by the protocol for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup information about routes installed by the protocol for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ip routing-table statistics

Use display system internal ip routing-table statistics to display IPv4 route statistics.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] statistics standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip routing-table [ topology topo-name | vpn-instance vpn-instance-name ] statistics standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays routing information for the public network. Support for this option depends on the device model.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

standby slot slot-number: Displays backup IPv4 route statistics for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv4 route statistics for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv4 route statistics for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 rib event attribute

Use display system internal ipv6 rib event attribute to display IPv6 RIB attribute events.

Syntax

display system internal ipv6 rib event attribute

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal ipv6 rib event policy

Use display system internal ipv6 rib event policy to display IPv6 RIB policy events.

Syntax

display system internal ipv6 rib event policy

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal ipv6 rib event prefix

Use display system internal ipv6 rib event prefix to display IPv6 RIB prefix events.

Syntax

display system internal ipv6 rib event prefix

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal ipv6 rib event protocol

Use display system internal ipv6 rib event protocol to display IPv6 RIB protocol events.

Syntax

display system internal ipv6 rib event protocol [ vpn-instance vpn-instance-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays the information for the public network. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 rib event statistics

Use display system internal ipv6 rib event statistics to display IPv6 RIB event statistics.

Syntax

display system internal ipv6 rib event statistics [ vpn-instance vpn-instance-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays the statistics for the public network. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 rib instance

Use display system internal ipv6 rib instance to display IPv6 RIB process information.

Syntax

display system internal ipv6 rib instance

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal ipv6 rib log

Use display system internal ipv6 rib log to display IPv6 RIB logs.

Syntax

Centralized devices:

display system internal ipv6 rib log [ reverse ]

display system internal ipv6 rib event log

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 rib log [ reverse ] [ standby slot slot-number [ cpu cpu-number ] ]

display system internal ipv6 rib event log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 rib log [ reverse ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal ipv6 rib event log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

rib: Displays IPv6 RIB logs.

event: Displays logs about IPv6 RIB routing changes.

reverse: Displays logs in reverse chronological order.

standby slot slot-number: Displays backup IPv6 RIB logs for a card. If you do not specify this option, the command displays IPv6 RIB logs. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv6 RIB logs for an IRF member device. If you do not specify this option, the command displays IPv6 RIB logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv6 RIB logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IPv6 RIB logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 rib memory

Use display system internal ipv6 rib memory to display IPv6 RIB memory information.

Syntax

display system internal ipv6 rib memory

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal ipv6 rib nib

Use display system internal ipv6 rib nib to display next hop information in the IPv6 RIB.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 rib nib [ self-originated ] [ nib-id ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal ipv6 rib nib protocol protocol [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 rib nib [ self-originated ] [ nib-id ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal ipv6 rib nib protocol protocol [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

self-originated: Displays information about next hops of self-originated routes in the IPv6 RIB.

nib-id: Specifies a NIB by its ID in the range of 1 to FFFFFFFF.

verbose: Displays detailed next hop information in the IPv6 RIB. If you do not specify this keyword, the command displays brief next hop information in the IPv6 RIB.

protocol protocol: Specifies a protocol by its name.

standby slot slot-number: Displays backup next hop information in the IPv6 RIB for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup next hop information in the IPv6 RIB for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup next hop information in the IPv6 RIB for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 rib nib log

Use display system internal ipv6 rib nib log to display IPv6 next hop logs.

Syntax

Centralized devices:

display system internal ipv6 rib nib log [ reverse ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 rib nib log [ reverse ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 rib nib log [ reverse ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib: Displays IPv6 next hop logs.

reverse: Displays logs in reverse chronological order.

standby slot slot-number: Displays backup IPv6 next hop logs for a card. If you do not specify this option, the command displays IPv6 next hop logs. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv6 next hop logs for an IRF member device. If you do not specify this option, the command displays IPv6 next hop logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv6 next hop logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IPv6 next hop logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 rib prefix

Use display system internal ipv6 rib prefix to display IPv6 RIB prefix information.

Syntax

Centralized devices:

display system internal ipv6 rib prefix ipv6-address prefix-length [ vpn-instance vpn-instance-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 rib prefix ipv6-address prefix-length [ vpn-instance vpn-instance-name ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 rib prefix ipv6-address prefix-length [ vpn-instance vpn-instance-name ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Specifies the destination IPv6 address.

prefix-length: Specifies the prefix length of the destination IPv6 address, in the range of 0 to 128.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays the IPv6 RIB prefix information for the public network. Support for this option depends on the device model.

standby slot slot-number: Displays backup IPv6 RIB prefix information for a card. If you do not specify this option, the command displays IPv6 RIB prefix information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv6 RIB prefix information for an IRF member device. If you do not specify this option, the command displays IPv6 RIB prefix information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv6 RIB prefix information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IPv6 RIB prefix information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 rib summary

Use display system internal ipv6 rib summary to display IPv6 RIB statistics.

Syntax

Centralized devices:

display system internal ipv6 rib summary

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 rib summary [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 rib summary [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

standby slot slot-number: Displays backup IPv6 RIB statistics of a card. If you do not specify this option, the command displays IPv6 RIB statistics. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv6 RIB statistics of an IRF member device. If you do not specify this option, the command displays IPv6 RIB statistics. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv6 RIB statistics of a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IPv6 RIB statistics. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 route-direct interface

Use display system internal ipv6 route-direct interface to display IPv6 interface information.

Syntax

display system internal ipv6 route-direct interface [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ipv6-address prefix-length ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays the IPv6 interface information for the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number.

ipv6-address: Specifies an IPv6 address.

prefix-length: Specifies the prefix length of the IPv6 address, in the range of 0 to 128.

Basic IP routing probe commands -- display system internal ipv6 route-direct log

Use display system internal ipv6 route-direct log to display IPv6 direct route logs.

Syntax

display system internal ipv6 route-direct { event | notify | nib } log [ reverse ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

event: Displays interface event logs.

notify: Displays interface event notification logs.

nib: Displays logs for IPv6 direct route next hops.

reverse: Displays logs in reverse chronological order.

Basic IP routing probe commands -- display system internal ipv6 routing-table

Use display system internal ipv6 routing-table to display IPv6 routing table information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing table information for the public network. Support for this option depends on the device model.

verbose: Displays detailed routing table information, including information about both active and inactive routes. If you do not specify this keyword, the command displays only brief information about active routes.

standby slot slot-number: Displays backup IPv6 routing table information for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv6 routing table information for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv6 routing table information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 routing-table acl

Use display system internal ipv6 routing-table acl to display routing information permitted by an IPv6 basic ACL.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] acl ipv6-acl-number [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] acl ipv6-acl-number [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

ipv6-acl-number: Specifies a basic IPv6 ACL by its number in the range of 2000 to 2999.

verbose: Displays detailed information about all routes permitted by the basic IPv6 ACL. If you do not specify this keyword, the command displays only brief information about active routes permitted by the basic IPv6 ACL.

standby slot slot-number: Displays backup information permitted by the IPv6 basic ACL for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup information permitted by the IPv6 basic ACL for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup information permitted by the IPv6 basic ACL for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 routing-table ipv6-address

Use display system internal ipv6 routing-table ipv6-address to display information about routes to a specific IPv6 destination address.

Use display system internal ipv6 routing-table ipv6-address1 to ipv6-address2 to display information about routes to a range of IPv6 destination addresses.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] ipv6-address [ prefix-length ] [ longer-match ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] ipv6-address1 to ipv6-address2 [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] ipv6-address [ prefix-length ] [ longer-match ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] ipv6-address1 to ipv6-address2 [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

ipv6-address: Specifies a destination IPv6 address.

prefix-length: Specifies the prefix length in the range of 0 to 128.

longer-match: Displays the route entry with the longest prefix.

ipv6-address1 to ipv6-address2: Specifies a destination IPv6 address range.

verbose: Displays detailed routing table information, including information about both active and inactive routes. If you do not specify this keyword, the command displays only brief information about active routes.

standby slot slot-number: Displays backup information about IPv6 routes for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup information about IPv6 routes for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup information about IPv6 routes for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 routing-table prefix-list

Use display system internal ipv6 routing-table prefix-list to display information about IPv6 routes permitted by an IPv6 prefix list.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] prefix-list prefix-list-name [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] prefix-list prefix-list-name [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

prefix-list-name: Specifies an IPv6 prefix list by its name, a case-sensitive string of 1 to 63 characters.

verbose: Displays detailed information about all IPv6 routes permitted by the IPv6 prefix list. If you do not specify this keyword, the command displays brief information about active IPv6 routes permitted by the IPv6 prefix list.

standby slot slot-number: Displays backup information about IPv6 routes permitted by the IPv6 prefix list for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup information about IPv6 routes permitted by the IPv6 prefix list for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup information about IPv6 routes permitted by the IPv6 prefix list for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 routing-table protocol

Use display system internal ipv6 routing-table protocol to display information about IPv6 routes installed by a protocol.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] protocol protocol [ inactive | verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] protocol protocol [ inactive | verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

protocol: Specifies a routing protocol.

inactive: Displays information about inactive routes. If you do not specify this keyword, the command displays information about both active and inactive routes.

verbose: Displays detailed routing table information. If you do not specify this keyword, the command displays brief routing information.

standby slot slot-number: Displays backup information about IPv6 routes installed by the protocol for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup information about IPv6 routes installed by the protocol for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup information about IPv6 routes installed by the protocol for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal ipv6 routing-table statistics

Use display system internal ipv6 routing-table statistics to display IPv6 route statistics.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] statistics standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 routing-table [ vpn-instance vpn-instance-name ] statistics standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays routing information for the public network. Support for this option depends on the device model.

standby slot slot-number: Displays backup IPv6 route statistics for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv6 route statistics for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv6 route statistics for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal rib event attribute

Use display system internal rib event attribute to display IPv4 RIB attribute events.

Syntax

display system internal rib event attribute

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal rib event policy

Use display system internal rib event policy to display IPv4 RIB policy events.

Syntax

display system internal rib event policy

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal rib event prefix

Use display system internal rib event prefix to display IPv4 RIB prefix events.

Syntax

display system internal rib event prefix

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal rib event protocol

Use display system internal rib event protocol to display IPv4 RIB protocol events.

Syntax

display system internal rib event protocol [ vpn-instance vpn-instance-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays the information for the public network. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal rib event statistics

Use display system internal rib event statistics to display RIB event statistics.

Syntax

display system internal rib event statistics [ vpn-instance vpn-instance-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays the statistics for the public network. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal rib ftn

Use display system internal rib ftn to display FTN entries and FTN statistics.

Syntax

display system internal rib ftn [ index ] [ statistics ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

index: Specifies an FTN entry by its index, a hexadecimal number in the range of 8000000 to ffffffff. The highest digit of the index value is fixed at 1. If you do not specify this argument, the command displays all FTN entries.

statistics: Displays FTN statistics.

Basic IP routing probe commands -- display system internal rib ftn summary

Use display system internal rib ftn summary to display FTN running information.

Syntax

display system internal rib ftn summary

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal rib instance

Use display system internal rib instance to display RIB process information.

Syntax

display system internal rib instance

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal rib log

Use display system internal rib log to display RIB logs.

Syntax

Centralized devices:

display system internal rib log [ reverse ]

display system internal rib event log

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rib log [ reverse ] [ standby slot slot-number [ cpu cpu-number ] ]

display system internal rib event log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal rib log [ reverse ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

display system internal rib event log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

rib: Displays RIB logs.

event: Displays logs about RIB routing changes.

reverse: Displays logs in reverse chronological order.

standby slot slot-number: Displays backup RIB logs for a card. If you do not specify this option, the command displays RIB logs. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup RIB logs for an IRF member device. If you do not specify this option, the command displays RIB logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup RIB logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays RIB logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal rib memory

Use display system internal rib memory to display RIB memory information.

Syntax

display system internal rib memory

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic IP routing probe commands -- display system internal rib nib

Use display system internal rib nib to display next hop information in the RIB.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rib nib [ self-originated ] [ nib-id ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

display system internal rib nib protocol protocol [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rib nib [ self-originated ] [ nib-id ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal rib nib protocol protocol [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

self-originated: Displays information about next hops of self-originated routes in the RIB.

nib-id: Specifies a NIB by its ID in the range of 1 to FFFFFFFF.

verbose: Displays detailed next hop information in the RIB. If you do not specify this keyword, the command displays brief next hop information in the RIB.

protocol protocol: Specifies a protocol by its name.

standby slot slot-number: Displays backup next hop information in the RIB for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup next hop information in the RIB for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup next hop information in the RIB for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal rib nib log

Use display system internal rib nib log to display next hop logs.

Syntax

Centralized devices:

display system internal rib nib log [ reverse ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rib nib log [ reverse ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal rib nib log [ reverse ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib: Displays next hop logs.

reverse: Displays logs in reverse chronological order.

standby slot slot-number: Displays backup next hop logs for a card. If you do not specify this option, the command displays next hop logs. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup next hop logs for an IRF member device. If you do not specify this option, the command displays next hop logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup next hop logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays next hop logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal rib prefix

Use display system internal rib prefix to display RIB prefix information.

Syntax

Centralized devices:

display system internal rib prefix ip-address mask-length [ vpn-instance vpn-instance-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rib prefix ip-address mask-length [ vpn-instance vpn-instance-name ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal rib prefix ip-address mask-length [ vpn-instance vpn-instance-name ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ip-address: Specifies the destination IP address.

mask-length: Specifies the mask length of the IP address, in the range of 0 to 32.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays RIB prefix information for the public network. Support for this option depends on the device model.

standby slot slot-number: Displays backup RIB prefix information for a card. If you do not specify this option, the command displays RIB prefix information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup RIB prefix information for an IRF member device. If you do not specify this option, the command displays RIB prefix information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup RIB prefix information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays RIB prefix information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal rib summary

Use display system internal rib summary to display RIB statistics.

Syntax

Centralized devices:

display system internal rib summary

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rib summary [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal rib summary [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

standby slot slot-number: Displays backup RIB statistics of a card. If you do not specify this option, the command displays RIB statistics. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup RIB statistics of an IRF member device. If you do not specify this option, the command displays RIB statistics. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup RIB statistics of a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays RIB statistics. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- display system internal route-direct interface

Use display system internal route-direct interface to display interface information.

Syntax

display system internal route-direct interface [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ip-address { mask-length | mask } ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the interface information for the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number.

ip-address: Specifies an IP address in dotted decimal notation.

mask-length: Specifies the mask length, an integer in the range of 0 to 32.

mask: Specifies the subnet mask in dotted decimal notation.

Basic IP routing probe commands -- display system internal route-direct log

Use display system internal route-direct log to display direct route logs.

Syntax

display system internal route-direct { event | notify | nib } log [ reverse ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

event: Displays interface event logs.

notify: Displays interface event notification logs.

nib: Displays logs for direct routes next hops.

reverse: Displays logs in reverse chronological order.

Basic IP routing probe commands -- reset system internal ip routing-table statistics protocol

Use reset system internal ip routing-table statistics protocol to clear IPv4 route statistics.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ip routing-table statistics protocol [ vpn-instance vpn-instance-name ] { protocol | all } standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal ip routing-table statistics protocol [ vpn-instance vpn-instance-name ] { protocol | all } standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command clears IPv4 route statistics for the public network.

protocol: Clears statistics about IPv4 routes installed by a protocol.

all: Clears all IPv4 route statistics.

standby slot slot-number: Clears backup IPv4 route statistics for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup IPv4 route statistics for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup IPv4 route statistics for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal ipv6 rib log

Use reset system internal ipv6 rib log to clear IPv6 RIB logs.

Syntax

Centralized devices:

reset system internal ipv6 rib [ event ] log

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ipv6 rib [ event ] log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal ipv6 rib [ event ] log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

event: Clears logs about IPv6 RIB route changes.

standby slot slot-number: Clears backup IPv6 RIB logs for a card. If you do not specify this option, the command clears IPv6 RIB logs. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup IPv6 RIB logs for an IRF member device. If you do not specify this option, the command clears IPv6 RIB logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup IPv6 RIB logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command clears IPv6 RIB logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal ipv6 rib nib log

Use reset system internal ipv6 rib nib log to clear IPv6 next hop logs.

Syntax

Centralized devices:

reset system internal ipv6 rib nib log

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ipv6 rib nib log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal ipv6 rib nib log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

standby slot slot-number: Clears backup IPv6 next hop logs for a card. If you do not specify this option, the command clears IPv6 next hop logs. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup IPv6 next hop logs for an IRF member device. If you do not specify this option, the command clears IPv6 next hop logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup IPv6 next hop logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command clears IPv6 next hop logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal ipv6 rib summary

Use reset system internal ipv6 rib summary to clear IPv6 RIB statistics.

Syntax

Centralized devices:

reset system internal ipv6 rib summary

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ipv6 rib summary [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal ipv6 rib summary [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

standby slot slot-number: Clears backup IPv6 RIB statistics of a card. If you do not specify this option, the command clears IPv6 RIB statistics. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup IPv6 RIB statistics of an IRF member device. If you do not specify this option, the command clears IPv6 RIB statistics. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup IPv6 RIB statistics of a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command clears IPv6 RIB statistics. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal ipv6 route-direct log

Use reset system internal ipv6 route-direct log to clear IPv6 direct route logs.

Syntax

reset system internal ipv6 route-direct { event | notify | nib } log

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

event: Clears interface event logs.

notify: Clears interface event notification logs.

nib: Clears logs for IPv6 direct route next hops.

Basic IP routing probe commands -- reset system internal ipv6 routing-table statistics protocol

Use reset system internal ipv6 routing-table statistics protocol to clear IPv6 route statistics.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ipv6 routing-table statistics protocol [ vpn-instance vpn-instance-name ] { protocol | all } standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal ipv6 routing-table statistics protocol [ vpn-instance vpn-instance-name ] { protocol | all } standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command clears IPv4 route statistics for the public network.

protocol: Clears statistics about IPv6 routes installed by a protocol.

all: Clears all IPv6 route statistics.

standby slot slot-number: Clears backup IPv6 route statistics for a card. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup IPv6 route statistics for an IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup IPv6 route statistics for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal rib log

Use reset system internal rib log to clear RIB logs.

Syntax

Centralized devices:

reset system internal rib [ event ] log

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal rib [ event ] log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal rib [ event ] log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

event: Clears logs about RIB route changes.

standby slot slot-number: Clears backup RIB logs for a card. If you do not specify this option, the command clears RIB logs. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup RIB logs for an IRF member device. If you do not specify this option, the command clears RIB logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup RIB logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command clears RIB logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal rib nib log

Use reset system internal rib nib log to clear next hop logs.

Syntax

Centralized devices:

reset system internal rib nib log

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal rib nib log [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal rib nib log [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

standby slot slot-number: Clears backup next hop logs for a card. If you do not specify this option, the command clears next hop logs. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup next hop logs for an IRF member device. If you do not specify this option, the command clears next hop logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup next hop logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command clears next hop logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal rib summary

Use reset system internal rib summary to clear RIB statistics.

Syntax

Centralized devices:

reset system internal rib summary

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal rib summary [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal rib summary [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

standby slot slot-number: Clears backup RIB statistics of a card. If you do not specify this option, the command clears RIB statistics. (Distributed devices in standalone mode.)

standby slot slot-number: Clears backup RIB statistics of an IRF member device. If you do not specify this option, the command clears RIB statistics. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Clears backup RIB statistics of a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command clears RIB statistics. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Basic IP routing probe commands -- reset system internal route-direct log

Use reset system internal route-direct log to clear direct route logs.

Syntax

reset system internal route-direct { event | notify | nib } log

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

event: Clears interface event logs.

notify: Clears interface event notification logs.

nib: Clears logs for direct route next hops.