L2PT probe commands -- display system internal l2protocol tunnel-group

Use display system internal l2protocol tunnel-group to display L2PT tunnel group information.

Syntax

Centralized devices:

display system internal l2protocol tunnel-group

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2protocol tunnel-group slot slot-number

Distributed devices in IRF mode:

display system internal l2protocol tunnel-group chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID, and the slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)