Tunneling probe commands -- display system internal tunnel data

Use display system internal tunnel data to display kernel data for a tunnel interface.

Syntax

Centralized devices:

display system internal tunnel data interface tunnel number [ cpu cpu-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal tunnel data interface tunnel number [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal tunnel data interface tunnel number [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface tunnel number: Specifies a tunnel interface by interface number. The specified tunnel interface must already exist.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays data for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays data for the master device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays data for the global active MPU. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.