WLAN RRM probe commands -- rrm calibrate-power step

Use rrm calibrate-power step to set the power adjustment step.

Use undo rrm calibrate-power step to restore the default.

Syntax

rrm calibrate-power step { down | up } value

undo rrm calibrate-power step { down | up }

Default

The power adjustment step is 3 dBm.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

down: Specifies a power decrement step.

up: Specifies a power increment step.

value: Specifies a power adjustment step in the range of 1 to 8 dBm.