Ethernet link aggregation probe commands -- debugging system internal link-aggregation soft-forward

Use debugging system internal link-aggregation soft-forward to enable software-based forwarding debugging for aggregate interfaces.

Use undo debugging system internal link-aggregation soft-forward to disable software-based forwarding debugging for aggregate interfaces.

Syntax

Centralized devices:

debugging system internal link-aggregation soft-forward [ interface { blade-aggregation | bridge-aggregation | route-aggregation | schannel-bundle } [ interface-number ] ]

undo debugging system internal link-aggregation soft-forward [ interface { blade-aggregation | bridge-aggregation | route-aggregation | schannel-bundle } [ interface-number ] ]

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal link-aggregation soft-forward slot slot-number [ interface { blade-aggregation | bridge-aggregation | route-aggregation | schannel-bundle } [ interface-number ] ]

undo debugging system internal link-aggregation soft-forward slot slot-number [ interface { blade-aggregation | bridge-aggregation | route-aggregation | schannel-bundle } [ interface-number ] ]

Distributed devices in IRF mode:

debugging system internal link-aggregation soft-forward chassis chassis-number slot slot-number [ interface { blade-aggregation | bridge-aggregation | route-aggregation | schannel-bundle } [ interface-number ] ]

undo debugging system internal link-aggregation soft-forward chassis chassis-number slot slot-number [ interface { blade-aggregation | bridge-aggregation | route-aggregation | schannel-bundle } [ interface-number ] ]

Default

Software-based forwarding debugging is disabled for aggregate interfaces.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

blade-aggregation: Specifies Blade aggregate interfaces. Support for this keyword depends on the device model.

bridge-aggregation: Specifies Layer 2 aggregate interfaces. Support for this keyword depends on the device model.

route-aggregation: Specifies Layer 3 aggregate interfaces. Support for this keyword depends on the device model.

schannel-bundle: Specifies S-channel bundle interfaces. Support for this keyword depends on the device model.

interface-number: Specifies an interface number. The specified interface must already exist.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

Ethernet link aggregation probe commands -- display system internal link-aggregation global

Use display system internal link-aggregation global to display the global information about the Ethernet link aggregation module.

Syntax

Centralized devices:

display system internal link-aggregation global

Distributed devices in standalone mode:Centralized IRF devices:

display system internal link-aggregation slot slot-number global

Distributed devices in IRF mode:

display system internal link-aggregation chassis chassis-number slot slot-number global

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

Ethernet link aggregation probe commands -- display system internal link-aggregation interface

Use display system internal link-aggregation interface to display aggregate interface information.

Syntax

Centralized devices:

display system internal link-aggregation interface { bridge-aggregation | route-aggregation } interface-number [ kernel | statistics [ ipv4 | ipv6 ] ]

display system internal link-aggregation interface interface-type interface-number [ kernel | lacp | lacppdu | statistics [ ipv4 | ipv6 ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal link-aggregation slot slot-number interface { bridge-aggregation | route-aggregation } interface-number [ kernel | statistics [ ipv4 | ipv6 ] ]

display system internal link-aggregation slot slot-number interface interface-type interface-number [ kernel | lacp | lacppdu | statistics [ ipv4 | ipv6 ] ]

Distributed devices in IRF mode:

display system internal link-aggregation chassis chassis-number slot slot-number interface { bridge-aggregation | route-aggregation } interface-number [ kernel | statistics [ ipv4 | ipv6 ] ]

display system internal link-aggregation chassis chassis-number slot slot-number interface interface-type interface-number [ kernel | lacp | lacppdu | statistics [ ipv4 | ipv6 ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

bridge-aggregation: Displays information about Layer 2 aggregate interfaces.

route-aggregation: Displays information about Layer 3 aggregate interfaces. Support for this keyword depends on the device model.

interface-number: Specifies an existing aggregate interface number. The value range for the interface-number argument varies by device model.

interface-type interface-number: Specifies the interface type and interface number. The value range for the interface-type interface-number argument varies by device model.

kernel: Displays kernel information.

statistics: Displays statistic information.

ipv4: Displays IPv4 packet statistics.

ipv6: Displays IPv6 packet statistics.

lacp: Displays dynamic aggregation information.

lacppdu: Displays statistics for LACPDUs.

slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

Usage guidelines

If you do not specify any of the kernel, lacp, lacppdu, and statistics keywords, the command displays the interface information in the main thread.

If you specify the statistics keyword without specifying the ipv4 or ipv6 keyword, the command displays statistics about all packets.

Part of the information that is displayed overlaps because the information is saved in separate threads. You can use the overlapping information for problem location and analysis.