AP management probe commands -- display system internal wlan backup-ap

| NOTE: Support for this command depends on the device model.

Use display system internal wlan backup-ap to display AP backup information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal wlan backup-ap [ slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify this option, the command displays AP backup information for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify this option, the command displays AP backup information for the master device. (Centralized IRF devices.)

Usage guidelines

(Distributed devices in standalone mode.) An AC backs up AP information for all online APs on all cards. If a card fails, APs associated with the card will connect to the card that has the lowest work load.

(Centralized IRF devices.) An AC backs up AP information for all online APs on all member devices. If a member fails, APs associated with the member will connect to the member that has the lowest work load.

AP management probe commands -- display system internal wlan kernel-ap

Use display system internal wlan kernel-ap to display AP kernel information.

Syntax

display system internal wlan kernel-ap { all | name ap-name } [ chassis chassis-number slot slot-number cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all APs.

name ap-name: Specifies an AP by its name, a case-insensitive string of 1 to 64 characters. The string can contain letters, digits, underscores (_), left brackets ([), right brackets (]), forward slashes (/), and hyphens (-).

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If you do not specify the chassis chassis-number slot slot-number cpu cpu-number option, this command displays AP kernel information for the global active MPU.

AP management probe commands -- display system internal wlan link-info

Use display system internal wlan link-info to display link information.

Syntax

display system internal wlan link-info [ chassis chassis-number slot slot-number cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If you do not specify the chassis chassis-number slot slot-number cpu cpu-number option, this command displays link information for the global active MPU.