VSRP probe commands -- IPoE VSRP probe commands -- display system internal ip subscriber cache statistics

Use display system internal ip subscriber cache statistics to display statistics about cached IPv4 IPoE user information.

Syntax

Centralized devices:

display system internal ip subscriber cache statistics [ vsrp-instance vsrp-instance-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip subscriber cache statistics [ vsrp-instance vsrp-instance-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ip subscriber cache statistics [ vsrp-instance vsrp-instance-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vsrp-instance vsrp-instance-name: Specifies a VSRP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, this command displays statistics about cached IPv4 IPoE user information for all VSRP instances.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays statistics about cached IPv4 IPoE user information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays statistics about cached IPv4 IPoE user information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays statistics about cached IPv4 IPoE user information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays statistics about cached IPv4 IPoE user information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays statistics about cached IPv4 IPoE user information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VSRP probe commands -- IPoE VSRP probe commands -- display system internal ipv6 subscriber cache statistics

Use display system internal ipv6 subscriber cache statistics to display statistics about cached IPv6 IPoE user information.

Syntax

Centralized devices:

display system internal ipv6 subscriber cache statistics [ vsrp-instance vsrp-instance-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 subscriber cache statistics [ vsrp-instance vsrp-instance-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 subscriber cache statistics [ vsrp-instance vsrp-instance-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vsrp-instance vsrp-instance-name: Specifies a VSRP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, this command displays statistics about cached IPv6 IPoE user information for all VSRP instances.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays statistics about cached IPv6 IPoE user information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays statistics about cached IPv6 IPoE user information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays statistics about cached IPv6 IPoE user information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays statistics about cached IPv6 IPoE user information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays statistics about cached IPv6 IPoE user information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VSRP probe commands -- PPPoE VSRP probe commands -- display system internal ppp sync-session

Use display system internal ppp sync-session to display the PPP sessions or PPPoE sessions to be associated by PPP on the backup.

Syntax

display system internal ppp sync-session [ vsrp-instance vsrp-instance-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vsrp-instance vsrp-instance-name: Specifies a VSRP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, this command displays PPP or PPPoE sessions to be associated by PPP in all VSRP instances.

Usage guidelines

PPPoE sessions and PPP sessions are synchronized independently from the master to the backup. Then PPP associates the PPPoE sessions with the corresponding PPP sessions on the backup.

· If the PPPoE sessions are synchronized to the backup prior to the PPP sessions, PPP stores the PPPoE sessions to be associated. And it performs the association when the PPP sessions are synchronized.

· If the PPP sessions are synchronized to the backup prior to the PPPoE sessions, PPP stores the PPP sessions to be associated. And it performs the association when the PPPoE sessions are synchronized.