Flow manager probe commands -- debugging system internal flow-manager

| NOTE: Support for this command depends on the device model.

Use debugging system internal flow-manager to enable flow manager debugging.

Use undo debugging system internal flow-manager to disable flow manager debugging.

Syntax

Centralized devices:

debugging system internal flow-manager [ acl { ipv4-acl-number | ipv6 ipv6-acl-number } | remote-address { ipv4-address | ipv6 ipv6-address } ]

undo debugging system internal flow-manager

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal flow-manager [ acl { ipv4-acl-number | ipv6 ipv6-acl-number } | remote-address { ipv4-address | ipv6 ipv6-address } ] [ slot slot-number cpu cpu-number ]

undo debugging system internal flow-manager [ slot slot-number cpu cpu-number ]

Distributed devices in IRF mode:

debugging system internal flow-manager [ acl { ipv4-acl-number | ipv6 ipv6-acl-number } | remote-address { ipv4-address | ipv6 ipv6-address } ] [ chassis chassis-number slot slot-number cpu cpu-number ]

undo debugging system internal flow-manager [ chassis chassis-number slot slot-number cpu cpu-number ]

Default

Flow manager debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

acl: Filters debugging information by using an ACL.

ipv4-acl-number: Specifies an IPv4 ACL by its number in the range of 3000 to 3999.

ipv6 ipv6-acl-number: Specifies an IPv6 ACL by its number in the range of 3000 to 3999.

remote-address: Filters debugging information by a remote IP address.

ipv4-address: Specifies a remote IPv4 address, in dotted decimal notation.

ipv6 ipv6-address: Specifies a remote IPv6 address.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command enables flow manager debugging for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command enables flow manager debugging for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command enables flow manager debugging for all member devices if you do not specify a member device. On an IRF 3 system, this command enables flow manager debugging for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command enables flow manager debugging for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command enables flow manager debugging for all cards if you do not specify a card. On an IRF 3 system, this command enables flow manager debugging for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Flow manager probe commands -- display system internal flow-manager failover-group

| NOTE: Support for this command depends on the device model.

Use display system internal flow-manager failover-group to display failover group information for the flow manager.

Syntax

Centralized devices:

display system internal flow-manager failover-group

Distributed devices in standalone mode:Centralized IRF devices:

display system internal flow-manager failover-group [ slot slot-number cpu cpu-number ]

Distributed devices in IRF mode:

display system internal flow-manager failover-group [ chassis chassis-number slot slot-number cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays failover group information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays failover group information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays failover group information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays failover group information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays failover group information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.