RLINK probe commands -- debugging system internal rlink packet

| NOTE: Support for this command depends on the device model.

Use debugging system internal rlink packet to enable RLINK packet debugging.

Use undo debugging system internal rlink packet to disable RLINK packet debugging.

Syntax

debugging system internal rlink packet

undo debugging system internal rlink packet

Default

RLINK packet debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

RLINK probe commands -- debugging system internal rlink pcb

| NOTE: Support for this command depends on the device model.

Use debugging system internal rlink pcb to enable RLINK PCB debugging.

Use undo debugging system internal rlink pcb to disable RLINK PCB debugging.

Syntax

debugging system internal rlink pcb

undo debugging system internal rlink pcb

Default

RLINK PCB debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

RLINK probe commands -- display system internal rlink pcb

| NOTE: Support for this command depends on the device model.

Use display system internal rlink pcb to display detailed RLINK PCB information.

Syntax

display system internal rlink pcb

Views

Probe view

Predefined user roles

network-admin

mdc-admin

RLINK probe commands -- display system internal rlink port statistics

| NOTE: Support for this command depends on the device model.

Use display system internal rlink port statistics to display RLINK port statistics.

Syntax

Centralized devices:

display system internal rlink port port-number statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rlink port port-number statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal rlink port port-number statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

port port-number: Specifies a port number in the range of 100 to 65535.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays information about all member devices if you do not specify a member device. On an IRF 3 system, this command displays information about all member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays information about all cards if you do not specify a card. On an IRF 3 system, this command displays information about all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

RLINK probe commands -- display system internal rlink statistics

| NOTE: Support for this command depends on the device model.

Use display system internal rlink statistics to display RLINK statistics.

Syntax

Centralized devices:

display system internal rlink statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rlink statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal rlink statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays information about all member devices if you do not specify a member device. On an IRF 3 system, this command displays information about all member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays information about all cards if you do not specify a card. On an IRF 3 system, this command displays information about all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.