MLD snooping commands -- display ipv6 l2-multicast fast-forwarding cache

Use display ipv6 l2-multicast fast-forwarding cache to display Layer 2 IPv6 multicast fast forwarding entries.

Syntax

Centralized devices:

display ipv6 l2-multicast fast-forwarding cache [ vlan vlan-id ] [ ipv6-source-address | ipv6-group-address ] *

Distributed devices in standalone mode:Centralized IRF devices:

display ipv6 l2-multicast fast-forwarding cache [ vlan vlan-id ] [ ipv6-source-address | ipv6-group-address ] * [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display ipv6 l2-multicast fast-forwarding cache [ vlan vlan-id ] [ ipv6-source-address | ipv6-group-address ] * [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

ipv6-source-address: Specifies an IPv6 multicast source address. If you do not specify an IPv6 multicast source, this command displays Layer 2 IPv6 multicast forwarding entries for all IPv6 multicast sources.

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F. If you do not specify an IPv6 multicast group, this command displays Layer 2 IPv6 multicast forwarding entries for all IPv6 multicast groups.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays Layer 2 IPv6 multicast fast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays Layer 2 IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays Layer 2 IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays Layer 2 IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays Layer 2 IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display Layer 2 IPv6 multicast fast forwarding entries.

<Sysname> display ipv6 l2-multicast fast-forwarding cache

Total 1 entries, 1 matched

(1::6, FF1E::2)

Status : Enable VLAN : 1

Source port : 9876 Destination port: 5432

Protocol : 17 Flag : 0x2

Ingress port: GigabitEthernet1/0/2

List of 1 egress ports:

GigabitEthernet1/0/3

Status: Enable Flag: 0x10

Table 1 Command output

Field | Description
Total 1 entries, 1 matched | Total number of (S, G) entries in the Layer 2 IPv6 multicast fast forwarding table, and the total number of matching entries.
(1::6, FF1E::2) | (S, G) entry in the Layer 2 IPv6 multicast fast forwarding table.
Protocol | Protocol number.
VLAN | VLAN ID.
Flag | Flag for the (S, G) entry or the outgoing port. This field displays one flag or the sum of multiple flags. In this example, the value 0x2 means that the entry has only one flag 0x2. The following flags are available for an entry: · 0x1—The entry is created because of packets passed through between cards. · 0x2—The entry is added by multicast forwarding. The following flags are available for an outgoing interface: · 0x1—The port is added to the entry because of packets passed through between cards. · 0x2—The port is added to an existing entry. · 0x10—The port is associated with the entry. · 0x20—The port is to be deleted.
Status | Status of the (S, G) entry or the outgoing port: · Enabled—Available. · Disabled—Unavailable.
Ingress port | Incoming port of the (S, G) entry.
List of 1 egress ports | List of outgoing ports of the (S, G) entry.

Related commands

reset ipv6 l2-multicast fast-forwarding cache all

MLD snooping commands -- display ipv6 l2-multicast ip

Use display ipv6 l2-multicast ip to display information about Layer 2 IPv6 multicast groups.

Syntax

Centralized devices:

display ipv6 l2-multicast ip [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display ipv6 l2-multicast ip [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display ipv6 l2-multicast ip [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

group ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. If you do not specify an IPv6 multicast group, this command displays information about all Layer 2 IPv6 multicast groups.

source ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays information about Layer 2 IPv6 multicast groups for all IPv6 multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays information about Layer 2 IPv6 multicast groups for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays information about Layer 2 IPv6 multicast groups for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about Layer 2 IP multicast groups for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about Layer 2 IP multicast groups for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information about Layer 2 IP multicast groups for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about Layer 2 IP multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays information about Layer 2 IP multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display information about Layer 2 IPv6 multicast groups for VLAN 2.

<Sysname> display ipv6 l2-multicast ip vlan 2

Total 1 entries.

VLAN 2: Total 1 entries.

(::, FF1E::101)

Attribute: static, success

Host ports (1 in total):

GE1/0/1 (S, SUC)

# Display information about Layer 2 IPv6 multicast groups for VSI aaa.

<Sysname> display ipv6 l2-multicast ip vsi aaa

Total 1 entries.

VSI aaa: Total 1 entries.

(::, FF1E::101)

Attribute: dynamic, success

Host ports (3 in total):

GE1/0/3 (Link ID 0) (D, SUC)

NPW (Link ID 8) (D, SUC)

UPW (Link ID 9) (D, SUC)

# Display information about Layer 2 IPv6 multicast groups for VSI bbb.

<Sysname> display ipv6 l2-multicast ip vsi bbb

Total 1 entries.

VSI bbb: Total 1 entries.

(::, FF1E::101)

Attribute: dynamic, success

Host ports (2 in total):

GE1/0/3 (Link ID 0) (D, SUC)

Tun0 (VXLAN ID 0) (D, SUC)

Table 2 Command output

Field | Description
Total 1 entries | Total number of Layer 2 IPv6 multicast groups.
VLAN 2: Total 1 entries | Total number of Layer 2 IPv6 multicast groups in VLAN 2.
VSI aaa: Total 1 entries | Total number of Layer 2 IPv6 multicast groups in VSI aaa.
(::, FF1E::101) | (S, G) entry, where a double colon (::) in the S position means all IPv6 multicast sources.
Attribute | Entry attribute: · dynamic—The entry is created by a dynamic protocol. · static—The entry is created by a static protocol. · pim—The entry is created by IPv6 PIM. · kernel—The entry is obtained from the kernel. · success—Processing has succeeded. · fail—Processing has failed.
Host ports (1 in total) | Member ports and total number of member ports.
(S, SUC) | Port attribute: · D—Dynamic port. · S—Static port. · P—IPv6 PIM port. · K—Port obtained from the kernel. · R—Port learned from (*, *) entries. · W—Port learned from (*, G) entries. · SUC—Processing has succeeded. · F—Processing has failed. · BC—In a VLAN, the port is a TRILL port that floods IPv6 multicast data after the topology changes. In a VSI, the port is a multicast tunnel port for a multicast-mode VXLAN.
GE1/0/3 (Link ID 0) | AC and its link ID.
NPW (Link ID 8) | N-PW and its link ID.
UPW (Link ID 9) | U-PW and its link ID.
Tun0 (VXLAN ID 0) | VXLAN tunnel and its VXLAN ID.

MLD snooping commands -- display ipv6 l2-multicast ip forwarding

Use display ipv6 l2-multicast ip forwarding to display Layer 2 IPv6 multicast IP forwarding entries.

Syntax

Centralized devices:

display ipv6 l2-multicast ip forwarding [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display ipv6 l2-multicast ip forwarding [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display ipv6 l2-multicast ip forwarding [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

group ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. If you do not specify an IPv6 multicast group, this command displays Layer 2 IPv6 multicast IP forwarding entries for all IPv6 multicast groups.

source ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays Layer 2 IPv6 multicast IP forwarding entries for all IPv6 multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays Layer 2 IPv6 multicast IP forwarding entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays Layer 2 IPv6 multicast IP forwarding entries for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays the Layer 2 IPv6 multicast IP forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays Layer 2 IPv6 multicast IP forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays Layer 2 IPv6 multicast IP forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays Layer 2 IPv6 multicast IP forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays Layer 2 IPv6 multicast IP forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display Layer 2 IPv6 multicast IP forwarding entries for VLAN 2.

<Sysname> display ipv6 l2-multicast ip forwarding vlan 2

Total 1 entries.

VLAN 2: Total 1 entries.

(::, FF1E::101)

Host ports (3 in total):

GigabitEthernet1/0/1

GigabitEthernet1/0/2

GigabitEthernet1/0/3

# Display Layer 2 IPv6 multicast IP forwarding entries for VSI aaa.

<Sysname> display ipv6 l2-multicast ip forwarding vsi aaa

Total 1 entries.

VSI aaa: Total 1 entries.

(::, FF1E::101)

Host ports (3 in total):

GigabitEthernet1/0/3 (Link ID 0)

NPW (Link ID 8)

UPW (Link ID 9)

# Display Layer 2 IPv6 multicast IP forwarding entries for VSI bbb.

<Sysname> display ipv6 l2-multicast ip forwarding vsi bbb

Total 1 entries.

VSI bbb: Total 1 entries.

(::, FF1E::101)

Host ports (2 in total):

GigabitEthernet1/0/3 (Link ID 0)

Tunnel0 (VXLAN ID 0)

Table 3 Command output

Field | Description
Total 1 entries | Total number of Layer 2 IPv6 multicast IP forwarding entries.
VLAN 2: Total 1 entries | Total number of Layer 2 IPv6 multicast IP forwarding entries in VLAN 2.
VSI aaa: Total 1 entries | Total number of Layer 2 IPv6 multicast IP forwarding entries in VSI aaa.
(::, FF1E::101) | (S, G) entry, where a double colon (::) in the S position means all IPv6 multicast sources.
Host ports (3 in total) | Member ports and total number of member ports.
GigabitEthernet1/0/3 (Link ID 0) | AC and its link ID.
NPW (Link ID 8) | N-PW and its link ID.
UPW (Link ID 9) | U-PW and its link ID.
Tunnel0 (VXLAN ID 0) | VXLAN tunnel and its VXLAN ID.

MLD snooping commands -- display ipv6 l2-multicast mac

Use display ipv6 l2-multicast mac to display information about Layer 2 IPv6 multicast MAC multicast groups.

Syntax

Centralized devices:

display ipv6 l2-multicast mac [ mac-address ] [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display ipv6 l2-multicast mac [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display ipv6 l2-multicast mac [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

mac-address: Specifies an IPv6 multicast MAC address. If you do not specify an IPv6 multicast MAC address, this command displays information about all Layer 2 IPv6 multicast MAC multicast groups.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays information about Layer 2 IPv6 multicast MAC multicast groups for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays information about Layer 2 IPv6 multicast MAC multicast groups for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about the Layer 2 IPv6 multicast MAC multicast groups for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about Layer 2 IPv6 multicast MAC multicast groups for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information about Layer 2 IPv6 multicast MAC multicast groups for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about Layer 2 IPv6 multicast MAC multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays information about Layer 2 IPv6 multicast MAC multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display information about Layer 2 IPv6 multicast MAC multicast groups for VLAN 2.

<Sysname> display ipv6 l2-multicast mac vlan 2

Total 1 entries.

VLAN 2: Total 1 entries.

MAC group address: 3333-0000-0101

Attribute: success

Host ports (1 in total):

GE1/0/1

# Display information about Layer 2 IPv6 MAC multicast groups for VSI aaa.

<Sysname> display ipv6 l2-multicast mac vsi aaa

Total 1 MAC entries.

VSI aaa: Total 1 entries.

MAC group address: 0100-5e01-0101

Attribute: success

Host ports (3 in total):

GE1/0/3 ( Link ID 0)

NPW (Link ID 8)

UPW (Link ID 9)

# Display information about Layer 2 IPv6 MAC multicast groups for VSI bbb.

<Sysname> display ipv6 l2-multicast mac vsi bbb

Total 1 entries.

VSI bbb: Total 1 entries.

MAC group address: 0100-5e01-0101

Attribute: success

Host ports (2 in total):

GE1/0/3 ( Link ID 0)

Tun0 (VXLAN ID 0)

Table 4 Command output

Field | Description
Total 1 entries | Total number of Layer 2 IPv6 MAC multicast groups.
VLAN 2: Total 1 entries | Total number of Layer 2 IPv6 MAC multicast groups in VLAN 2.
VSI aaa: Total 1 entries | Total number of Layer 2 IPv6 MAC multicast groups in VSI aaa.
MAC group address | IPv6 address of the Layer 2 IPv6 MAC multicast group.
Attribute | Entry attribute: · success—Processing has succeeded. · fail—Processing has failed.
Host ports (1 in total) | Member ports and total number of member ports.
GE1/0/3 ( Link ID 0) | AC and its link ID.
NPW (Link ID 8) | N-PW and its link ID.
UPW (Link ID 9) | U-PW and its link ID.
Tun0 (VXLAN ID 0) | VXLAN tunnel and its VXLAN ID.

MLD snooping commands -- display ipv6 l2-multicast mac forwarding

Use display ipv6 l2-multicast mac forwarding to display Layer 2 IPv6 multicast MAC forwarding entries.

Syntax

Centralized devices:

display ipv6 l2-multicast mac forwarding [ mac-address ] [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display ipv6 l2-multicast mac forwarding [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display ipv6 l2-multicast mac forwarding [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

mac-address: Specifies an IPv6 MAC multicast group by its IPv6 MAC address. If you do not specify an IPv6 MAC multicast group, this command displays Layer 2 IPv6 multicast MAC forwarding entries for all IPv6 MAC multicast groups.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays Layer 2 IPv6 multicast MAC forwarding entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays Layer 2 IPv6 multicast MAC forwarding entries for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays Layer 2 IPv6 multicast MAC forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays Layer 2 IPv6 multicast MAC forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays Layer 2 IPv6 multicast MAC forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays Layer 2 IPv6 multicast MAC forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays Layer 2 IPv6 multicast MAC forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display Layer 2 IPv6 multicast MAC forwarding entries for VLAN 2.

<Sysname> display ipv6 l2-multicast mac forwarding vlan 2

Total 1 entries.

VLAN 2: Total 1 entries.

MAC group address: 3333-0000-0101

Host ports (3 in total):

GigabitEthernet1/0/1

GigabitEthernet1/0/2

GigabitEthernet1/0/3

# Display Layer 2 IPv6 multicast MAC forwarding entries for VSI aaa.

<Sysname> display ipv6 l2-multicast mac forwarding vsi aaa

Total 1 entries.

VSI aaa: Total 1 entries.

MAC group address: 0100-5e01-0101

Host ports (3 in total):

GigabitEthernet1/0/3 (Link ID 0)

NPW (Link ID 8)

UPW (Link ID 9)

# Display Layer 2 IPv6 multicast MAC forwarding entries for VSI bbb.

<Sysname> display ipv6 l2-multicast mac forwarding vsi bbb

Total 1 entries.

VSI bbb: Total 1 entries.

MAC group address: 0100-5e01-0101

Host ports (2 in total):

GigabitEthernet1/0/3 (Link ID 0)

Tunnel0 (VXLAN ID 0)

Table 5 Command output

Field | Description
Total 1 MAC entries | Total number of Layer 2 IPv6 multicast MAC forwarding entries.
VLAN 2: Total 1 entries | Total number of Layer 2 IPv6 multicast MAC forwarding entries in VLAN 2.
VSI aaa: Total 1 entries | Total number of Layer 2 IPv6 multicast MAC forwarding entries in VSI aaa.
MAC group address | Address of the IPv6 MAC multicast group.
Host ports (3 in total) | Member ports, and the total number of member ports.
GigabitEthernet1/0/3 (Link ID 0) | AC and its link ID.
NPW (Link ID 8) | N-PW and its link ID.
UPW (Link ID 9) | U-PW and its link ID.
Tunnel0 (VXLAN ID 0) | VXLAN tunnel and its VXLAN ID.

MLD snooping commands -- display mld-snooping

Use display mld-snooping to display MLD snooping status.

Syntax

display mld-snooping [ global | vlan vlan-id | vsi vsi-name ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

global: Displays the global MLD snooping status.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters.

Usage guidelines

If you do not specify any parameters, this command displays the global MLD snooping status and the MLD snooping status in all VLANs and VSIs.

Examples

# Display the global MLD snooping status and the MLD snooping status for all VLANs and VSIs.

<Sysname> display mld-snooping

MLD snooping information: Global

Global-enable: Enabled

Drop-unknown: Disabled

Host-aging-time: 260s

Router-aging-time: 260s

Max-response-time: 10s

Last-listener-query-interval: 1s

Report-aggregation: Enabled

Host-tracking: Disabled

Dot1p-priority: --

MLD snooping information: VLAN 1

MLD snooping: Enabled

Drop-unknown: Disabled

Version: 1

Host-aging-time: 260s

Router-aging-time: 260s

Max-response-time: 10s

Last-listener-query-interval: 1s

Querier: Disabled

Query-interval: 125s

General-query source IP: FE80::2FF:FFFF:FE00:1

Special-query source IP: FE80::2FF:FFFF:FE00:1

Report source IP: FE80::2FF:FFFF:FE00:2

Done source IP: FE80::2FF:FFFF:FE00:3

Host-tracking: Disabled

Dot1p-priority: 2

Proxy: Disabled

MLD snooping information: VLAN 10

MLD snooping: Enabled

Drop-unknown: Enabled

Version: 1

Host-aging-time: 260s

Router-aging-time: 260s

Max-response-time: 10s

Last-listener-query-interval: 1s

Querier: Disabled

Query-interval: 125s

General-query source IP: FE80::2FF:FFFF:FE00:1

Special-query source IP: FE80::2FF:FFFF:FE00:1

Report source IP: FE80::2FF:FFFF:FE00:2

Done source IP: FE80::2FF:FFFF:FE00:3

Host-tracking: Disabled

Dot1p-priority: --

Proxy: Disabled

MLD snooping information: VSI aaa

MLD snooping: Enabled

Drop-unknown: Enabled

Version: 1

Host-aging-time: 260s

Router-aging-time: 260s

Max-response-time: 10s

Last-listener-query-interval: 1s

Querier: Disabled

Query-interval: 125s

General-query source IP: FE80::2FF:FFFF:FE00:1

Special-query source IP: FE80::2FF:FFFF:FE00:1

Table 6 Command output

Field | Description
Global-enable | Global MLD snooping status: · Enabled. · Disabled.
MLD snooping | MLD snooping status in a VLAN or VSI: · Enabled. · Disabled. · Globally enabled. · Inactive—MLD snooping configuration does not take effect.
Drop-unknown | Status of dropping unknown IPv6 multicast data: · Enabled. · Disabled. · Globally enabled.
Version | MLD snooping version.
Host-aging-time | Aging timer for the dynamic member port.
Router-aging-time | Aging timer for the dynamic router port.
Max-response-time | Maximum time for responding to MLD general queries.
Last-listener-query-interval | Interval for sending MLD multicast-address-specific queries.
Report-aggregation | Status of MLD report suppression: · Enabled. · Disabled.
Dot1p-priority | 802.1p priority for MLD messages. This field displays two hyphens (--) if the 802.1p priority is not configured.
Querier | Status of MLD snooping querier: · Enabled. · Disabled.
Query-interval | Interval for sending MLD general queries.
General-query source IP | Source IPv6 address of MLD general queries.
Special-query source IP | Source IPv6 address of MLD multicast-address-specific queries.
Report source IP | Source IPv6 address of MLD reports.
Done source IP | Source IPv6 address of MLD done messages.
Host-tracking | ‌ Status of host tracking: · Enabled. · Disabled. · Globally enabled.
Proxy | ‌ Status of MLD snooping proxying: · Enabled. · Disabled.

MLD snooping commands -- display mld-snooping group

Use display mld-snooping group to display information about dynamic MLD snooping group entries.

Syntax

Centralized devices:

display mld-snooping group [ ipv6-group-address | ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ interface interface-type interface-number | verbose ]

Distributed devices in standalone mode:Centralized IRF devices:

display mld-snooping group [ ipv6-group-address | ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ interface interface-type interface-number | [ verbose ] [ slot slot-number [ cpu cpu-number ] ] ]

Distributed devices in IRF mode:

display mld-snooping group [ ipv6-group-address | ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ interface interface-type interface-number | [ verbose ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F. If you do not specify an IPv6 multicast group, this command displays information about all dynamic MLD snooping group entries.

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays information about dynamic MLD snooping group entries for all IPv6 multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays information about dynamic MLD snooping group entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays information about dynamic MLD snooping group entries for all VSIs.

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays brief information about dynamic MLD snooping group entries for all interfaces.

verbose: Displays detailed information about dynamic MLD snooping group entries. If you do not specify this keyword, the command displays brief information about dynamic MLD snooping group entries.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about dynamic MLD snooping group entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about dynamic MLD snooping group entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information about dynamic MLD snooping group entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about dynamic MLD snooping group entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays information about dynamic MLD snooping group entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display brief information about dynamic MLD snooping group entries for GigabitEthernet 1/0/1.

<Sysname> display mld-snooping group interface gigabitethernet 1/0/1

Total 1 entries.

GE1/0/1:

VLAN 2: Total 1 entries.

(::,FF1E::101) (00:03:23)

# Display detailed information about dynamic MLD snooping group entries for VLAN 2.

<Sysname> display mld-snooping group vlan 2 verbose

Total 1 entries.

VLAN 2: Total 1 entries.

(::,FF1E::101)

Attribute: local port

FSM information: dummy

Host slots (0 in total):

Host ports (1 in total):

GE1/0/2 (00:03:23)

# Display brief information about dynamic MLD snooping group entries for VSI aaa.

<Sysname> display mld-snooping group vsi aaa

Total 1 entries.

VSI aaa: Total 1 entries.

(::,FF1E::101)

Host ports (1 in total):

GE1/0/3 (Link ID 1) (00:03:35)

NPW (Link ID 8) (00:02:35)

UPW (Link ID 9) (00:01:35)

# Display detailed information about dynamic MLD snooping group entries for VSI bbb.

<Sysname> display mld-snooping group vsi bbb verbose

Total 1 entries.

VSI bbb: Total 1 entries.

(::,FF1E::101)

Attribute: global port

FSM information: dummy

Host slots (0 in total):

Host ports (2 in total):

GE1/0/3 (Link ID 0) (00:03:35)

VLAN pairs (1 in total):

Outer VLAN 5 Inner VLAN 2 (00:03:35)

Tun0 (VXLAN ID 0) (00:03:35)

VLAN pairs (1 in total):

Outer VLAN 5 Inner VLAN 2 (00:03:35)

Table 7 Command output

Field | Description
Total 1 entries | Total number of dynamic MLD snooping group entries.
VLAN 2: Total 1 entries | Total number of dynamic MLD snooping group entries in VLAN 2.
VSI aaa: Total 1 entries | Total number of dynamic MLD snooping group entries in VSI aaa.
(::, FF1E::101) | (S, G) entry, where a double colon (::) in the S position means all IPv6 multicast sources.
Attribute | Entry attribute: · global port—The entry has a global port. · local port—The entry has a port that resides on the card for which the information is displayed. · slot—The entry has ports that reside on other cards, but not on the card for which the information is displayed.
FSM information | Finite state machine information of the entry: · delete—The entry attributes have been deleted. · dummy—The entry is a new temporary entry. · no info—The entry does not exist. · normal—The entry is a correct entry.
Host slots (0 in total) | (Centralized devices.) This field is not supported. (Distributed devices in standalone mode.) Slot numbers and total number of the cards that have member ports, except for the specified card or the MPU when no card is specified. (Centralized IRF devices.) Member IDs and total number of the member devices that have member ports, except for the specified member device or the master device when no member device is specified. (Distributed devices in IRF mode.) Chassis numbers, slot numbers, and total number of the cards that have member ports, except for the specified card or the global active MPU when no card is specified.
Host ports (1 in total) | Member ports and total number of member ports.
(00:03:23) | Remaining aging time for the dynamic member port. This field is always displayed for a global port (such as Layer 2 aggregate interfaces, ACs, N-PWs, and U-PWs). (Centralized devices.) For a non-global port, this field is always displayed. (Distributed devices in standalone mode.) For a non-global port, this field is displayed when one of the following conditions exists: · The port is on the specified card. · The port is on the MPU and no card is specified. (Centralized IRF devices.) For a non-global port, this field is displayed when one of the following conditions exists: · The port is on the specified member device. · The port is on the master device and no member device is specified. (Distributed devices in IRF mode.) For a non-global port, this field is displayed when one of the following conditions exists: · The port is on the specified card. · The port is on the global active MPU and no card is specified.
GE1/0/3 (Link ID 0) | AC and its link ID.
NPW (Link ID 8) | N-PW and its link ID.
UPW (Link ID 9) | U-PW and its link ID.
Tun0 (VXLAN ID 0) | VXLAN tunnel and its VXLAN ID.
VLAN pairs (1 in total) | VLAN pairs and total number of VLAN pairs.
Outer VLAN 5 Inner VLAN 2 | Outer VLAN ID and inner VLAN ID.

Related commands

reset mld-snooping group

MLD snooping commands -- display mld-snooping host-tracking

Use display mld-snooping host-tracking to display host tracking information.

Syntax

Centralized devices:

display mld-snooping host-tracking vlan vlan-id group ipv6-group-address [ source ipv6-source-address ]

Distributed devices in standalone mode:Centralized IRF devices:

display mld-snooping host-tracking vlan vlan-id group ipv6-group-address [ source ipv6-source-address ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display mld-snooping host-tracking vlan vlan-id group ipv6-group-address [ source ipv6-source-address ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

group ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. The value range for the ipv6-group-address argument is FFxy::/16, where "x" and "y" represent any hexadecimal numbers in the range of 0 to F.

source ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this commands displays host tracking information for all IPv6 multicast sources.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays host tracking information for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays host tracking information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays host tracking information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays host tracking information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays host tracking information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display tracking information for hosts that have joined IPv6 multicast group FF1E::2 in VLAN 2.

<Sysname> display mld-snooping host-tracking vlan 2 group FF1E::2

VLAN 2

(1::6, FF1E::2)

Port: GE1/0/1

Host Uptime Expires

1::2 00:02:20 00:00:40

1::3 00:02:21 00:00:39

Table 8 Command output

Field | Description
VLAN | VLAN ID.
(1::6, FF1E::2) | (S, G) entry, where 0::0 in the S position means any IPv6 multicast sources.
Port | Member port.
Host | IPv6 address of the host.
Uptime | Length of time elapsed since the host joined the IPv6 multicast group.
Expires | Remaining timeout time for the host. The host timeout time is the same as the aging timer of the port. The timer is reset when the port receives an MLD report from the host. This field displays timeout if the host times out.

Related commands

host-tracking (MLD-snooping view)

mld-snooping enable

mld-snooping host-tracking

MLD snooping commands -- display mld-snooping router-port

Use display mld-snooping router-port to display dynamic router port information.

Syntax

Centralized devices:

display mld-snooping router-port [ vlan vlan-id | vsi vsi-name ] [ verbose ]

Distributed devices in standalone mode:Centralized IRF devices:

display mld-snooping router-port [ vlan vlan-id | vsi vsi-name ] [ verbose ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display mld-snooping router-port [ vlan vlan-id | vsi vsi-name ] [ verbose ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

verbose: Displays detailed information about dynamic router ports. If you do not specify this keyword, the command displays brief information about dynamic router ports.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays dynamic router port information for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays dynamic router port information for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays dynamic router port information for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays dynamic router port information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays dynamic router port information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays dynamic router port information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays dynamic router port information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display brief information about dynamic router ports for VLAN 2.

<Sysname> display mld-snooping router-port vlan 2

VLAN 2:

Router ports (2 in total):

GE1/0/1 (00:01:30)

GE1/0/2 (00:00:23)

# Display detailed information about dynamic router ports for VSI aaa.

<Sysname> display mld-snooping router-port vsi aaa verbose

VSI aaa:

Router slots (0 in total):

Router ports (3 in total):

GE1/0/3 (Link ID 0) (00:03:35)

VLAN pairs (1 in total):

Outer VLAN 5 Inner VLAN 2 (00:03:35)

NPW (Link ID 8) (00:03:35)

VLAN pairs (1 in total):

Outer VLAN 5 Inner VLAN 2 (00:03:35)

UPW (Link ID 9) (00:03:35)

VLAN pairs (1 in total):

Outer VLAN 5 Inner VLAN 2 (00:03:35)

# Display detailed information about dynamic router ports for VSI bbb.

<Sysname> display mld-snooping router-port vsi bbb verbose

VSI bbb:

Router slots (0 in total):

Router ports (2 in total):

GE1/0/3 (Link ID 0) (00:03:35)

VLAN pairs (1 in total):

Outer VLAN 5 Inner VLAN 2 (00:03:35)

Tun0 (VXLAN ID 0) (00:03:35)

VLAN pairs (1 in total)

Outer VLAN 5 Inner VLAN 2 (00:03:35)

Table 9 Command output

Field | Description
VLAN 2 | VLAN ID.
VSI aaa | VSI name.
Router slots (0 in total) | (Centralized devices.) This field is not supported. (Distributed devices in standalone mode.) Slot numbers and total number of the cards that have dynamic router ports, except for the specified card or the MPU when no card is specified. (Centralized IRF devices.) Member IDs and total number of the member devices that have dynamic router ports, except for the specified member device or the master device when no member device is specified. (Distributed devices in IRF mode.) Chassis numbers, slot numbers, and total number of the cards that have dynamic router ports, except for the specified card or the global active MPU when no card is specified.
Router ports (2 in total) | Dynamic router ports and total number of dynamic router ports.
(00:01:30) | Remaining aging time for the dynamic router port. This field is always displayed for a global port (including Layer 2 aggregate interfaces). (Centralized devices.) For a non-global port, this field is always displayed. (Distributed devices in standalone mode.) For a non-global port, this field is displayed when one of the following conditions exists: · The port is on the specified card. · The port is on the MPU and no card is specified. (Centralized IRF devices.) For a non-global port, this field is displayed when one of the following conditions exists: · The port is on the specified member device. · The port is on the master device and no member device is specified. (Distributed devices in IRF mode.) For a non-global port, this field is displayed when one of the following conditions exists: · The port is on the specified card. · The port is on the global active MPU and no card is specified.
GE1/0/3 (Link ID 0) | AC and its link ID.
NPW (Link ID 8) | N-PW and its link ID.
UPW (Link ID 9) | U-PW and its link ID.
Tun0 (VXLAN ID 0) | Name of the VXLAN tunnel and the VXLAN ID.
VLAN pairs (1 in total) | VLAN pairs and total number of VLAN pairs.
Outer VLAN 5 Inner VLAN 2 | Outer VLAN ID and inner VLAN ID.

Related commands

reset mld-snooping router-port

MLD snooping commands -- display mld-snooping static-group

Use display mld-snooping static-group to display information about static MLD snooping group entries.

Syntax

Centralized devices:

display mld-snooping static-group [ ipv6-group-address | ipv6-source-address ] * [ vlan vlan-id ] [ verbose ]

Distributed devices in standalone mode:Centralized IRF devices:

display mld-snooping static-group [ ipv6-group-address | ipv6-source-address ] * [ vlan vlan-id ] [ verbose ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display mld-snooping static-group [ ipv6-group-address | ipv6-source-address ] * [ vlan vlan-id ] [ verbose ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F. If you do not specify an IPv6 multicast group, this command displays information about static MLD snooping group entries for all IPv6 multicast groups.

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays information about static MLD snooping group entries for all IPv6 multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays information about static MLD snooping group entries for all VLANs.

verbose: Displays detailed information. If you do not specify this keyword, the command displays brief information.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about static MLD snooping group entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about static MLD snooping group entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information about static MLD snooping group entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about static MLD snooping group entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays information about static MLD snooping group entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display detailed information about static MLD snooping group entries for VLAN 2.

<Sysname> display mld-snooping static-group vlan 2 verbose

Total 1 entries.

VLAN 2: Total 1 entries.

(::,FF1E::101)

Attribute: local port

FSM information: dummy

Host slots (0 in total):

Host ports (1 in total):

GE1/0/2

Table 10 Command output

Field | Description
Total 1 entries | Total number of static MLD snooping group entries.
VLAN 2: Total 1 entries | Total number of static MLD snooping group entries in VLAN 2.
(::, FF1E::101) | (S, G) entry, where a double colon (::) in the S position means all IPv6 multicast sources.
Attribute | Entry attribute: · global port—The entry has a global port. · local port—The entry has a port that resides on the card for which the information is displayed. · slot—The entry has ports that reside on other cards, but not on the card for which the information is displayed.
FSM information | Finite state machine information of the entry: · delete—The entry attributes have been deleted. · dummy—The entry is a new temporary entry. · no info—The entry does not exist. · normal—The entry is a correct entry.
Host slots (0 in total) | (Centralized devices.) This field is not supported. (Distributed devices in standalone mode.) Slot numbers and total number of the cards that have member ports, except for the specified card or the MPU when no card is specified. (Centralized IRF devices.) Member IDs and total number of the member devices that have member ports, except for the specified member device or the master device when no member device is specified. (Distributed devices in IRF mode.) Chassis numbers, slot numbers, and total number of the cards that have member ports, except for the specified card or the global active MPU when no card is specified.
Host ports (1 in total) | Member ports and total number of member ports.

MLD snooping commands -- display mld-snooping static-router-port

Use display mld-snooping static-router-port to display static router port information.

Syntax

Centralized devices:

display mld-snooping static-router-port [ vlan vlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display mld-snooping static-router-port [ vlan vlan-id ] [ verbose ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display mld-snooping static-router-port [ vlan vlan-id ] [ verbose ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

verbose: Displays detailed information about static router ports. If you do not specify this keyword, the command displays brief information about static router ports.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays static router port information for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays static router port information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays static router port information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays static router port information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays static router port information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display brief information about static router ports for VLAN 2.

<Sysname> display mld-snooping static-router-port vlan 2

VLAN 2:

Router ports (2 in total):

GE1/0/1

GE1/0/2

# Display detailed information about static router ports for VLAN 2.

<Sysname> display mld-snooping static-router-port vlan 2 verbose

VLAN 2:

Router slots (0 in total):

Router ports (2 in total):

GE1/0/1

GE1/0/2

Table 11 Command output

Field | Description
VLAN 2 | VLAN ID.
Router slots (0 in total) | (Centralized devices.) This field is not supported. (Distributed devices in standalone mode.) Slot numbers and total number of the cards that have static router ports, except for the specified card or the MPU when no card is specified. (Centralized IRF devices.) Member IDs and total number of the member devices that have static router ports, except for the specified member device or the master device when no member device is specified. (Distributed devices in IRF mode.) Chassis numbers, slot numbers, and total number of the cards that have static router ports, except for the specified card or the global active MPU when no card is specified.
Router ports (2 in total) | Static router ports and total number of static router ports.

MLD snooping commands -- display mld-snooping statistics

Use display mld-snooping statistics to display statistics for the MLD messages and IPv6 PIM hello messages learned through MLD snooping.

Syntax

display mld-snooping statistics

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Examples

# Display statistics for the MLD messages and IPv6 PIM hello messages learned through MLD snooping.

<Sysname> display mld-snooping statistics

Received MLD general queries: 0

Received MLDv1 specific queries: 0

Received MLDv1 reports: 0

Received MLD dones: 0

Sent MLDv1 specific queries: 0

Received MLDv2 reports: 0

Received MLDv2 reports with right and wrong records: 0

Received MLDv2 specific queries: 0

Received MLDv2 specific sg queries: 0

Sent MLDv2 specific queries: 0

Sent MLDv2 specific sg queries: 0

Received IPv6 PIM hello: 0

Received error MLD messages: 0

Table 12 Command output

Field | Description
general queries | Number of MLD general queries.
specific queries | Number of MLD multicast-address-specific queries.
reports | Number of MLD reports.
dones | Number of MLD done messages.
reports with right and wrong records | Number of MLD reports with correct and incorrect records.
specific sg queries | Number of MLD multicast-address-and-source-specific queries.
IPv6 PIM hello | Number of IPv6 PIM hello messages.
error MLD messages | Number of MLD messages with errors.

Related commands

reset mld-snooping statistics

MLD snooping commands -- dot1p-priority (MLD-snooping view)

Use dot1p-priority to set the 802.1p priority for MLD messages globally.

Use undo dot1p-priority to restore the default.

Syntax

dot1p-priority priority

undo dot1p-priority

Default

The 802.1p priority for MLD messages varies by device model.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

priority: Specifies an 802.1p priority for MLD messages, in the range of 0 to 7. The greater the value, the higher the priority.

Usage guidelines

You can set the 802.1p priority globally for all VLANs and VSIs in MLD-snooping view or for a VLAN in VLAN view. For a VLAN, the VLAN-specific configuration takes priority over the global configuration.

Examples

# Set the 802.1p priority for MLD messages to 3 globally.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] dot1p-priority 3

Related commands

mld-snooping dot1p-priority

MLD snooping commands -- drop-unknown (MLD-snooping view)

Use drop-unknown to enable dropping unknown IPv6 multicast data packets globally.

Use undo drop-unknown to disable dropping unknown IPv6 multicast data packets globally.

Syntax

drop-unknown

undo drop-unknown

Default

Dropping unknown IPv6 multicast data packets is disabled, and unknown IPv6 multicast data packets are flooded.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You can enable this feature globally for all VLANs and VSIs in MLD-snooping view, for a VSI in VSI view, or for a VLAN in VLAN view.

The mld-snooping drop-unknown command and the drop-unknown command in MLD-snooping view are mutually exclusive. You cannot configure them on the same device.

Examples

# Enable dropping unknown IPv6 multicast data packets globally.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] drop-unknown

Related commands

mld-snooping drop-unknown

MLD snooping commands -- enable (MLD-snooping view)

Use enable to enable MLD snooping for VLANs.

Use undo enable to disable MLD snooping for VLANs.

Syntax

enable vlan vlan-list

undo enable vlan vlan-list

Default

The MLD snooping status in a VLAN is consistent with the global MLD snooping status.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094.

Usage guidelines

You must enable the MLD snooping feature by using the mld-snooping command before you enable MLD snooping for VLANs.

You can enable MLD snooping for multiple VLANs by using this command in MLD-snooping view or for a VLAN by using the mld-snooping enable command in VLAN view. The configuration in VLAN view has the same priority as the configuration in MLD-snooping view, and the most recent configuration takes effect.

Examples

# Enable the MLD snooping feature, and then enable MLD snooping for VLAN 2 through VLAN 10.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] enable vlan 2 to 10

Related commands

mld-snooping

mld-snooping enable

MLD snooping commands -- entry-limit (MLD-snooping view)

Use entry-limit to globally set the maximum number of MLD snooping forwarding entries, including dynamic entries and static entries.

Use undo entry-limit to restore the default.

Syntax

entry-limit limit

undo entry-limit

Default

The maximum number of MLD snooping forwarding entries is 4294967295.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

limit: Specifies the maximum number of MLD snooping forwarding entries, in the range of 0 to 4294967295.

Examples

# Set the global maximum number of MLD snooping forwarding entries to 512.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] entry-limit 512

MLD snooping commands -- fast-leave (MLD-snooping view)

Use fast-leave to enable fast-leave processing globally.

Use undo fast-leave to disable fast-leave processing globally.

Syntax

fast-leave [ vlan vlan-list ]

undo fast-leave [ vlan vlan-list ]

Default

Fast-leave processing is disabled.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you do not specify a VLAN, this command takes effect for all VLANs and VSIs.

Usage guidelines

The fast-leave processing feature enables the device to immediately remove a port from the forwarding entry for an IPv6 multicast group when the port receives a done message.

You can enable fast-leave processing globally for all ports in MLD-snooping view or for a port in interface view. For a port, the port-specific configuration takes priority over the global configuration.

Examples

# Globally enable MLD snooping fast-leave processing for VLAN 2.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] fast-leave vlan 2

Related commands

mld-snooping fast-leave

MLD snooping commands -- global-enable (MLD-snooping view)

Use global-enable to enable MLD snooping globally.

Use undo global-enable to disable MLD snooping globally.

Syntax

global-enable

undo global-enable

Default

MLD snooping is disabled globally.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

To configure other MLD snooping features for VLANs or VSIs, you must enable MLD snooping for the specific VLANs or VSIs even though MLD snooping is enabled globally.

Examples

# Enable MLD snooping globally.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] global-enable

Related commands

enable (MLD-snooping view)

mld-snooping

mld-snooping disable

mld-snooping enable

MLD snooping commands -- group-policy (MLD-snooping view)

Use group-policy to globally configure an IPv6 multicast group policy to control the IPv6 multicast groups that hosts can join.

Use undo group-policy to globally delete IPv6 multicast group policies.

Syntax

group-policy ipv6-acl-number [ vlan vlan-list ]

undo group-policy [ vlan vlan-list ]

Default

No IPv6 multicast group policies exist. Hosts can join any IPv6 multicast groups.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-acl-number: Specifies an IPv6 basic or advanced ACL by its number in the range of 2000 to 3999. Hosts can join only IPv6 multicast groups that the ACL permits. If the ACL does not exist or does not have valid rules, hosts cannot join IPv6 multicast groups.

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you do not specify a VLAN, this command takes effect for all VLANs and VSIs.

Usage guidelines

An IPv6 multicast group policy filters MLD reports to control the IPv6 multicast groups that hosts can join.

This command does not take effect on static member ports, because static member ports do not send MLD reports.

You can configure an IPv6 multicast group policy globally for all ports in MLD-snooping view or for a port in interface view. For a port, the port-specific configuration takes priority over the global configuration.

When you configure a rule in the IPv6 ACL, follow these restrictions and guidelines:

· For the rule to take effect, do not specify the vpn-instance vpn-instance option.

· In a basic ACL, the source source-address source-prefix option specifies an IPv6 multicast group address.

· In an advanced ACL, the source source-address source-prefix option specifies an IPv6 multicast source address. The destination dest-address dest-prefix option specifies an IPv6 multicast group address.

To match MLDv1 reports and MLDv2 IS_EX and MLDv2 TO_EX reports that do not carry IPv6 multicast source addresses, set the source source-address source-prefix option to 0::0.

· Among the other optional parameters, only the fragment keyword and the time-range time-range-name option take effect.

You can configure different ACLs for all ports in different VLANs. If you configure multiple ACLs for all ports in the same VLAN, the most recent configuration takes effect.

Examples

# Configure an IPv6 multicast group policy for VLAN 2 so that hosts in VLAN 2 can join only IPv6 multicast group FF03::101.

<Sysname> system-view

[Sysname] acl ipv6 basic 2000

[Sysname-acl-ipv6-basic-2000] rule permit source ff03::101 128

[Sysname-acl-ipv6-basic-2000] quit

[Sysname] mld-snooping

[Sysname-mld-snooping] group-policy 2000 vlan 2

Related commands

mld-snooping group-policy

MLD snooping commands -- host-aging-time (MLD-snooping view)

Use host-aging-time to set the aging timer for dynamic member ports globally.

Use undo host-aging-time to restore the default.

Syntax

host-aging-time seconds

undo host-aging-time

Default

The aging timer for dynamic member ports is 260 seconds.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies an aging timer for dynamic member ports, in the range of 1 to 8097894 seconds.

Usage guidelines

You can set the timer globally for all VLANs and VSIs in MLD-snooping view, for a VSI in VSI view, or for a VLAN in VLAN view. For a VSI, the VSI-specific configuration takes priority over the global configuration. For a VLAN, the VLAN-specific configuration takes priority over the global configuration.

To avoid mistakenly deleting IPv6 multicast group members, set the aging timer for dynamic member ports to be greater than the value calculated by using the following formula:

[ MLD general query interval ] + [ maximum response time for MLD general queries ]

As a best practice, set the aging timer of dynamic member ports to the value calculated by using the following formula:

[ MLD general query interval ] ?2 + [ maximum response time for MLD general queries ]

Examples

# Set the global aging timer for dynamic member ports to 300 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] host-aging-time 300

Related commands

mld-snooping host-aging-time

MLD snooping commands -- host-tracking (MLD-snooping view)

Use host-tracking to enable host tracking globally.

Use undo host-tracking to disable host tracking globally.

Syntax

host-tracking

undo host-tracking

Default

Host tracking is disabled.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You can enable host tracking globally for all VLANs in MLD-snooping view or for a VLAN in VLAN view. For a VLAN, the global configuration has the same priority as the VLAN-specific configuration.

Examples

# Enable host tracking globally.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] host-tracking

Related commands

display mld-snooping host-tracking

mld-snooping host-tracking

MLD snooping commands -- last-listener-query-interval (MLD-snooping view)

Use last-listener-query-interval to set the MLD last listener query interval globally.

Use undo last-listener-query-interval to restore the default.

Syntax

last-listener-query-interval interval

undo last-listener-query-interval

Default

The MLD last listener query interval is 1 second.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

interval: Specifies an MLD last listener query interval in the range of 1 to 25 seconds.

Usage guidelines

You can set the interval for a VLAN in VLAN view, for a VSI in VSI view, or globally for all VLANs and VSIs in MLD-snooping view. For a VLAN, the VLAN-specific configuration takes priority over the global configuration. For a VSI, the VSI-specific configuration takes priority over the global configuration.

Examples

# Set the global MLD last listener query interval to 3 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] last-listener-query-interval 3

Related commands

mld-snooping last-listener-query-interval

MLD snooping commands -- max-response-time (MLD-snooping view)

Use max-response-time to set the maximum response time for MLD general queries globally.

Use undo max-response-time to restore the default.

Syntax

max-response-time seconds

undo max-response-time

Default

The maximum response time for MLD general queries is 10 seconds.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the maximum response time for MLD general queries, in the range of 1 to 3174 seconds.

Usage guidelines

You can set the time globally for all VLANs and VSIs in MLD-snooping view, for a VSI in VSI view, or for a VLAN in VLAN view. For a VSI, the VSI-specific configuration takes priority over the global configuration. For a VLAN, the VLAN-specific configuration takes priority over the global configuration.

To avoid mistakenly deleting IPv6 multicast group members, set the maximum response time for MLD general queries to be less than the MLD general query interval.

Examples

# Set the global maximum response time for MLD general queries to 5 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] max-response-time 5

Related commands

mld-snooping max-response-time

mld-snooping query-interval

MLD snooping commands -- mld-snooping

Use mld-snooping to enable the MLD snooping feature and enter MLD-snooping view.

Use undo mld-snooping to disable the MLD snooping feature.

Syntax

mld-snooping

undo mld-snooping

Default

The MLD snooping feature is disabled.

Views

System view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

If you disable the MLD snooping feature, MLD snooping is disabled in all VLANs and VSIs.

Examples

# Enable the MLD snooping feature and enter MLD-snooping view.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping]

Related commands

enable (MLD-snooping view)

mld-snooping enable

mld-snooping disable

MLD snooping commands -- mld-snooping access-policy

Use mld-snooping access-policy to configure an MLD snooping access control policy.

Use undo mld-snooping access-policy to delete an MLD snooping access control policy.

Syntax

mld-snooping access-policy ipv6-acl-number

undo mld-snooping access-policy { ipv6-acl-number | all }

Default

No MLD snooping access control policies exist. IPv6 multicast users can join or leave any IPv6 multicast groups.

Views

User profile view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-acl-number: Specifies an IPv6 basic or advanced ACL by its number, in the range of 2000 to 3999. IPv6 multicast users can join only the IPv6 multicast groups that the ACL permits. If the ACL does not exist or does not have valid rules, IPv6 multicast users cannot join or leave any IPv6 multicast groups.

all: Specifies all MLD snooping access control policies.

Usage guidelines

You can repeat this command to configure multiple MLD snooping access control policies. An IPv6 multicast user can join or leave an IPv6 multicast group if its MLD report or done message is permitted by one of the MLD snooping access control policies.

When you configure a rule in the IPv6 ACL, follow these restrictions and guidelines:

· For the rule to take effect, do not specify the vpn-instance vpn-instance option.

· In a basic ACL, the source source-address source-prefix option specifies an IPv6 multicast group address.

· In an advanced ACL, the source source-address source-prefix option specifies an IPv6 multicast source address. The destination dest-address dest-prefix option specifies an IPv6 multicast group address.

To match the following MLD messages, set the source source-address source-prefix option to 0::0:

?span style='font:7.0pt "Times New Roman"'> MLDv1 report and done messages.

?span style='font:7.0pt "Times New Roman"'> MLDv2 IS_EX and MLDv2 TO_EX reports that do not carry IPv6 multicast source addresses.

· Among the other optional parameters, only the fragment keyword and the time-range time-range-name option take effect.

Examples

# In user profile abc, configure an MLD snooping access control policy to allow IPv6 multicast users to join or leave only IPv6 multicast group FF03::101.

<Sysname> system-view

[Sysname] acl ipv6 basic 2001

[Sysname-acl6-basic-2001] rule permit source ff03::101 16

[Sysname-acl6-basic-2001] quit

[Sysname] user-profile abc

[Sysname-user-profile-abc] mld-snooping access-policy 2001

MLD snooping commands -- mld-snooping cvid-forward

Use mld-snooping cvid-forward to enable inner VLAN ID-based forwarding on a port.

Use undo mld-snooping cvid-forward to restore the default.

Syntax

mld-snooping cvid-forward

undo mld-snooping cvid-forward

Default

Inner VLAN ID-based forwarding is disabled on a port. The port performs outer VLAN ID-based forwarding.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This command enables the device to create and maintain MLD snooping forwarding entries based on the inner VLAN ID of the received double-tagged MLD packets.

This command takes effect only on MLD packets tagged with double VLAN IDs.

Examples

# Enable inner VLAN ID-based forwarding on GigabitEthernet 1/0/1.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping cvid-forward

MLD snooping commands -- mld-snooping done source-ip

Use mld-snooping done source-ip to configure the source IPv6 address for MLD done messages.

Use undo mld-snooping done source-ip to restore the default.

Syntax

mld-snooping done source-ip ipv6-address

undo mld-snooping done source-ip

Default

In a VLAN, the source IPv6 address of MLD done messages is the IPv6 link-local address of the current VLAN interface. If the current VLAN interface does not have an IPv6 link-local address, the source IPv6 address is FE80::02FF:FFFF:FE00:0001.

In a VSI, the source IPv6 address of MLD done messages is the IPv6 link-local address of the gateway interface for the VSI. If the gateway interface does not have an IPv6 link-local address, the source IPv6 address is FE80::02FF:FFFF:FE00:0001.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Specifies the source IPv6 address for MLD done messages.

Usage guidelines

You must enable MLD snooping for a VLAN before you execute this command.

Examples

# In VLAN 2, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address of MLD done messages.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping done source-ip fe80:0:0:1::1

# In VSI aaa, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address of MLD done messages.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping done source-ip fe80:0:0:1::1

Related commands

enable (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping dot1p-priority

Use mld-snooping dot1p-priority to set the 802.1p priority for MLD messages in a VLAN.

Use undo mld-snooping dot1p-priority to restore the default.

Syntax

mld-snooping dot1p-priority priority

undo mld-snooping dot1p-priority

Default

The 802.1p priority for MLD messages varies by device model.

Views

VLAN view

Predefined user roles

network-admin

mdc-admin

Parameters

priority: Specifies an 802.1p priority for MLD messages, in the range of 0 to 7. The greater the value, the higher the priority.

Usage guidelines

You must enable MLD snooping for a VLAN before you execute this command.

You can set the 802.1p priority for a VLAN in VLAN view or globally for all VLANs in MLD-snooping view. For a VLAN, the VLAN-specific configuration takes priority over the global configuration.

Examples

# In VLAN 2, enable MLD snooping, and set the 802.1p priority for MLD messages to 3.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping dot1p-priority 3

Related commands

dot1p-priority (MLD-snooping view)

enable (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping drop-unknown

Use mld-snooping drop-unknown to enable dropping unknown IPv6 multicast data packets for a VLAN or VSI.

Use undo mld-snooping drop-unknown to disable dropping unknown IPv6 multicast data packets for a VLAN or VSI.

Syntax

mld-snooping drop-unknown

undo mld-snooping drop-unknown

Default

Dropping unknown IPv6 multicast data packets is disabled. Unknown IPv6 multicast data packets are flooded.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command.

You can enable this feature for a VLAN in VLAN view, for a VSI in VSI view, or globally for all VLANs and VSIs in MLD-snooping view.

The mld-snooping drop-unknown command and the drop-unknown command in MLD-snooping view are mutually exclusive. You cannot configure them on the same device.

Examples

# In VLAN 2, enable MLD snooping, and enable dropping unknown IPv6 multicast data packets.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping drop-unknown

# In VSI aaa, enable MLD snooping, and enable dropping unknown IPv6 multicast data packets.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping drop-unknown

Related commands

drop-unknown (MLD-snooping view)

enable (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping { enable | disable }

Use mld-snooping enable to enable MLD snooping for a VLAN or VSI.

Use mld-snooping disable to disable MLD snooping for a VLAN or VSI.

Use undo mld-snooping to restore the MLD snooping status in a VLAN or VSI to the global MLD snooping status.

Syntax

mld-snooping { disable | enable }

undo mld-snooping

Default

The MLD snooping status in a VLAN or VSI is consistent with the global MLD snooping status.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You must enable the MLD snooping feature by using the mld-snooping command before you enable MLD snooping for a VLAN or VSI.

You can enable MLD snooping for a VLAN by using this command in VLAN view or for multiple VLANs by using the enable command. The configuration in VLAN view has the same priority as the configuration in MLD-snooping view, and the most recent configuration takes effect.

Examples

# Enable the MLD snooping feature, and then enable MLD snooping for VLAN 2.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

# Disable MLD snooping for VLAN 2.

<Sysname> system-view

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping disable

# Enable the MLD snooping feature, and then enable MLD snooping for VSI aaa.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

# Disable MLD snooping for VSI aaa.

<Sysname> system-view

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping disable

Related commands

enable (MLD-snooping view)

mld-snooping

MLD snooping commands -- mld-snooping fast-leave

Use mld-snooping fast-leave to enable fast-leave processing on a port.

Use undo mld-snooping fast-leave to disable fast-leave processing on a port.

Syntax

mld-snooping fast-leave [ vlan vlan-list ]

undo mld-snooping fast-leave [ vlan vlan-list ]

Default

Fast-leave processing is disabled on a port.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you do not specify a VLAN, this command takes effect on all VLANs.

Usage guidelines

The fast-leave processing feature enables the device to immediately remove a port from the forwarding entry for an IPv6 multicast group when the port receives a done message.

You can enable fast-leave processing for a port in interface view or globally for all ports in MLD-snooping view. For a port, the port-specific configuration takes priority over the global configuration.

Examples

# Enable fast-leave processing for VLAN 2 on GigabitEthernet 1/0/1.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping fast-leave vlan 2

Related commands

fast-leave (MLD-snooping view)

MLD snooping commands -- mld-snooping general-query source-ip

Use mld-snooping general-query source-ip to configure the source IPv6 address for MLD general queries.

Use undo mld-snooping general-query source-ip to restore the default.

Syntax

mld-snooping general-query source-ip ipv6-address

undo mld-snooping general-query source-ip

Default

In a VLAN, the source IPv6 address for MLD general queries is the IPv6 link-local address of the current VLAN interface. If the current VLAN interface does not have an IPv6 link-local address, the source IPv6 address is FE80::02FF:FFFF:FE00:0001.

In a VSI, the source IPv6 address for MLD general queries is the IPv6 link-local address of the gateway interface for the VSI. If the gateway interface does not have an IPv6 link-local address, the source IPv6 address is FE80::02FF:FFFF:FE00:0001.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Specifies the source IPv6 address for MLD general queries.

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command.

Examples

# In VLAN 2, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address for MLD general queries.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping general-query source-ip fe80:0:0:1::1

# In VSI aaa, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address for MLD general queries.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping general-query source-ip fe80:0:0:1::1

Related commands

enable (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping group-limit

Use mld-snooping group-limit to set the maximum number of IPv6 multicast groups that a port can join.

Use undo mld-snooping group-limit to remove the limit on the maximum number of IPv6 multicast groups that a port can join.

Syntax

mld-snooping group-limit limit [ vlan vlan-list ]

undo mld-snooping group-limit [ vlan vlan-list ]

Default

No limit is placed on the maximum number of IPv6 multicast groups that a port can join.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

limit: Specifies the maximum number of multicast groups that a port can join, in the range of 0 to 4294967295.

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you do not specify a VLAN, this command takes effect for all VLANs.

Usage guidelines

This command takes effect only on the IPv6 multicast groups that a port joins dynamically.

Examples

# On GigabitEthernet 1/0/1, set the maximum number to 10 for IPv6 multicast groups that the port can join in VLAN 2.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping group-limit 10 vlan 2

MLD snooping commands -- mld-snooping group-policy

Use mld-snooping group-policy to configure an IPv6 multicast group policy on a port to control the IPv6 multicast groups that hosts attached to the port can join.

Use undo mld-snooping group-policy to delete IPv6 multicast group policies on a port.

Syntax

mld-snooping group-policy ipv6-acl-number [ vlan vlan-list ]

undo mld-snooping group-policy [ vlan vlan-list ]

Default

No IPv6 multicast group policies exist. Hosts attached to the port can join any IPv6 multicast groups.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-acl-number: Specifies an IPv6 basic or advanced ACL number in the range of 2000 to 3999. Hosts can join only the IPv6 multicast groups that the ACL permits. If the ACL does not exist or does not have valid rules, hosts cannot join IPv6 multicast groups.

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you do not specify a VLAN, this command takes effect on all VLANs.

Usage guidelines

An IPv6 multicast group policy filters MLD reports to control the IPv6 multicast groups that hosts can join.

This command does not take effect on static member ports, because static member ports do not send MLD reports.

You can configure an IPv6 multicast group policy for a port in interface view or globally for all ports in MLD-snooping view. For a port, the port-specific configuration takes priority over the global configuration.

When you configure a rule in the IPv6 ACL, follow these restrictions and guidelines:

· For the rule to take effect, do not specify the vpn-instance vpn-instance option.

· In a basic ACL, the source source-address source-prefix option specifies an IPv6 multicast group address.

· In an advanced ACL, the source source-address source-prefix option specifies an IPv6 multicast source address. The destination dest-address dest-prefix option specifies an IPv6 multicast group address.

To match MLDv1 reports and MLD IS_EX and MLDv2 TO_EX reports that do not carry IPv6 multicast source addresses, set the source source-address source-prefix option to 0::0.

· Among the other optional parameters, only the fragment keyword and the time-range time-range-name option take effect.

You can configure different ACLs for different VLANs on a port. If you configure multiple ACLs for the same VLANs on a port, the most recent configuration takes effect.

Examples

# On GigabitEthernet 1/0/1, configure an IPv6 multicast group policy for VLAN 2 so that hosts attached to the port in VLAN 2 can join only the group FF03::101.

<Sysname> system-view

[Sysname] acl ipv6 basic 2000

[Sysname-acl-ipv6-basic-2000] rule permit source ff03::101 128

[Sysname-acl-ipv6-basic-2000] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping group-policy 2000 vlan 2

Related commands

group-policy (MLD-snooping view)

MLD snooping commands -- mld-snooping host-aging-time

Use mld-snooping host-aging-time to set the aging timer for dynamic member ports in a VLAN or VSI.

Use undo mld-snooping host-aging-time to restore the default.

Syntax

mld-snooping host-aging-time seconds

undo mld-snooping host-aging-time

Default

The aging timer for dynamic member ports is 260 seconds.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies an aging timer for dynamic member ports, in the range of 1 to 8097894 seconds.

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command.

You can set the timer for a VLAN in VLAN view, for a VSI in VSI view, or globally for all VLANs and VSIs in MLD-snooping view. For a VLAN, the VLAN-specific configuration takes priority over the global configuration. For a VSI, the VSI-specific configuration takes priority over the global configuration.

To avoid mistakenly deleting IPv6 multicast group members, set the aging timer for dynamic member ports to be greater than the value calculated by using the following formula:

[ MLD general query interval ] + [ maximum response time for MLD general queries ]

As a best practice, set the aging timer of dynamic member ports to the value calculated by using the following formula:

[ MLD general query interval ] ?2 + [ maximum response time for MLD general queries ]

Examples

# In VLAN 2, enable MLD snooping, and set the aging timer for dynamic member ports in the VLAN to 300 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping host-aging-time 300

# In VSI aaa, enable MLD snooping, and set the aging timer for dynamic member ports in the VSI to 300 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping host-aging-time 300

Related commands

enable (MLD-snooping view)

host-aging-time (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping host-join

Use mld-snooping host-join to configure a port as a simulated member host for an IPv6 multicast group or an IPv6 multicast source and group.

Use undo mld-snooping host-join to remove the configuration of a simulated member host for an IPv6 multicast group.

Syntax

mld-snooping host-join ipv6-group-address [ source-ip ipv6-source-address ] vlan vlan-id

undo mld-snooping host-join { ipv6-group-address [ source-ip ipv6-source-address ] vlan vlan-id | all }

Default

A port is not a simulated member host of any IPv6 multicast groups or any IPv6 multicast sources and groups.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F.

source-ip ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you specify an IPv6 multicast source, this command configures the port as a simulated member host for an IPv6 multicast source and group. If you do not specify an IPv6 multicast source, this command configures the port as a simulated member host for an IPv6 multicast group. This option takes effect on MLDv2 snooping devices.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

all: Specifies all IPv6 multicast groups and all IPv6 multicast sources and groups.

Usage guidelines

The version of MLD running on a simulated member host is the same as the version of MLD snooping running on the port. The port ages out in the same way as a dynamic member port.

Examples

# Configure GigabitEthernet 1/0/1 as a simulated member host for the IPv6 multicast group (*, FF3E::101) in VLAN 2.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping host-join ff3e::101 vlan 2

MLD snooping commands -- mld-snooping host-tracking

Use mld-snooping host-tracking to enable host tracking for a VLAN.

Use undo mld-snooping host-tracking to disable host tracking for a VLAN.

Syntax

mld-snooping host-tracking

undo mld-snooping host-tracking

Default

Host tracking is disabled.

Views

VLAN view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You must enable MLD snooping for a VLAN before you execute this command for the VLAN.

You can enable host tracking for a VLAN in VLAN view or globally for all VLANs in MLD-snooping view. For a VLAN, the VLAN-specific configuration has the same priority as the global configuration.

Examples

# In VLAN 2, enable MLD snooping, and then enable host tracking.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping host-tracking

Related commands

display mld-snooping host-tracking

host-tracking (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping last-listener-query-interval

Use mld-snooping last-listener-query-interval to set the MLD last listener query interval for a VLAN or VSI.

Use undo mld-snooping last-listener-query-interval to restore the default.

Syntax

mld-snooping last-listener-query-interval interval

undo mld-snooping last-listener-query-interval

Default

The MLD last listener query interval is 1 second.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

interval: Specifies an MLD last listener query interval in the range of 1 to 25 seconds.

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command.

You can set the interval for a VLAN in VLAN view, for a VSI in VSI view, or globally for all VLANs and VSIs in MLD-snooping view. For a VLAN, the VLAN-specific configuration takes priority over the global configuration. For a VSI, the VSI-specific configuration takes priority over the global configuration.

Examples

# In VLAN 2, enable MLD snooping, and set the MLD last listener query interval to 3 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping last-listener-query-interval 3

# In VSI aaa, enable MLD snooping, and set the MLD last listener query interval to 3 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping last-listener-query-interval 3

Related commands

enable (MLD-snooping view)

last-listener-query-interval (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping max-response-time

Use mld-snooping max-response-time to set the maximum response time for MLD general queries in a VLAN or VSI.

Use undo mld-snooping max-response-time to restore the default.

Syntax

mld-snooping max-response-time seconds

undo mld-snooping max-response-time

Default

The maximum response time for MLD general queries is 10 seconds.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the maximum response time for MLD general queries, in the range of 1 to 3174 seconds.

Usage guidelines

You must enable MLD snooping for a VLAN before you execute this command.

You can set the time for a VLAN in VLAN view, for a VSI in VSI view, or globally for all VLANs and VSIs in MLD-snooping view. For a VLAN, the VLAN-specific configuration takes priority over the global configuration. For a VSI, the VSI-specific configuration takes priority over the global configuration.

To avoid mistakenly deleting IPv6 multicast group members, set the maximum response time for MLD general queries to be less than the MLD general query interval.

Examples

# In VLAN 2, enable MLD snooping, and set the maximum response time for MLD general queries to 5 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping max-response-time 5

# In VSI aaa, enable MLD snooping, and set the maximum response time for MLD general queries to 5 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping max-response-time 5

Related commands

enable (MLD-snooping view)

max-response-time (MLD-snooping view)

mld-snooping enable

mld-snooping query-interval

MLD snooping commands -- mld-snooping overflow-replace

Use mld-snooping overflow-replace to enable the IPv6 multicast group replacement feature on a port.

Use undo mld-snooping overflow-replace to disable the multicast group replacement feature on a port.

Syntax

mld-snooping overflow-replace [ vlan vlan-list ]

undo mld-snooping overflow-replace [ vlan vlan-list ]

Default

The IPv6 multicast group replacement feature is disabled.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you do not specify a VLAN, this command takes effect on all VLANs.

Usage guidelines

This command takes effect only on the IPv6 multicast groups that a port joins dynamically.

You can enable the IPv6 multicast group replacement feature for a port in interface view or globally for all ports in MLD-snooping view. For a port, the port-specific configuration takes priority over the global configuration.

Examples

# On GigabitEthernet 1/0/1, enable the IPv6 multicast group replacement feature for VLAN 2.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping overflow-replace vlan 2

Related commands

overflow-replace (MLD-snooping view)

MLD snooping commands -- mld-snooping proxy enable

Use mld-snooping proxy enable to enable MLD snooping proxying for a VLAN.

Use undo mld-snooping proxy enable to disable MLD snooping proxying for a VLAN.

Syntax

mld-snooping proxy enable

undo mld-snooping proxy enable

Views

VLAN view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You must enable MLD snooping for a VLAN before you execute this command.

This command does not take effect on a VLAN that is a sub-VLAN of an IPv6 multicast VLAN.

Examples

# In VLAN 2, enable MLD snooping, and enable MLD snooping proxying.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping proxy enable

Related commands

enable (MLD-snooping view)

mld-snooping enable

subvlan (IPv6 multicast-VLAN view)

MLD snooping commands -- mld-snooping querier

Use mld-snooping querier to enable the MLD snooping querier.

Use undo mld-snooping querier to disable the MLD snooping querier.

Syntax

mld-snooping querier

undo mld-snooping querier

Default

The MLD snooping querier is disabled.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command.

For a sub-VLAN of an IPv6 multicast VLAN, this command takes effect only after you remove the VLAN from the IPv6 multicast VLAN.

Examples

# In VLAN 2, enable MLD snooping, and enable the MLD snooping querier.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping querier

# In VSI aaa, enable MLD snooping, and enable the MLD snooping querier.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping querier

Related commands

enable (MLD-snooping view)

mld-snooping enable

subvlan (IPv6 multicast-VLAN view)

MLD snooping commands -- mld-snooping query-interval

Use mld-snooping query-interval to set the MLD general query interval for a VLAN or VSI.

Use undo mld-snooping query-interval to restore the default.

Syntax

mld-snooping query-interval interval

undo mld-snooping query-interval

Default

The MLD general query interval is 125 seconds.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

interval: Specifies an MLD general query interval, in the range of 2 to 31744 seconds.

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command for the VLAN.

To avoid mistakenly deleting IPv6 multicast group members, set the MLD general query interval to be greater than the maximum response time for MLD general queries.

Examples

# In VLAN 2, enable MLD snooping, and set the MLD general query interval to 20 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping query-interval 20

# In VSI aaa, enable MLD snooping, and set the MLD general query interval to 20 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping query-interval 20

Related commands

enable (MLD-snooping view)

max-response-time

mld-snooping enable

mld-snooping max-response-time

mld-snooping querier

MLD snooping commands -- mld-snooping report source-ip

Use mld-snooping report source-ip to configure the source IPv6 address for MLD reports.

Use undo mld-snooping report source-ip to restore the default.

Syntax

mld-snooping report source-ip ipv6-address

undo mld-snooping report source-ip

Default

In a VLAN, the source IPv6 address for MLD reports is the IPv6 link-local address of the current VLAN interface. If the current VLAN interface does not have an IPv6 link-local address, the source IPv6 address is FE80::02FF:FFFF:FE00:0001.

In a VSI, the source IPv6 address for MLD reports is the IPv6 link-local address of the gateway interface for the VSI. If the gateway interface does not have an IPv6 link-local address, the source IPv6 address is FE80::02FF:FFFF:FE00:0001.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Specifies the source IPv6 address for MLD reports.

Usage guidelines

You must enable MLD snooping for a VLAN before you execute this command.

Examples

# In VLAN 2, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address for MLD reports.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping report source-ip fe80:0:0:1::1

# In VSI aaa, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address for MLD reports.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping report source-ip fe80:0:0:1::1

Related commands

enable (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping router-aging-time

Use mld-snooping router-aging-time to set the aging timer for dynamic router ports in a VLAN or VSI.

Use undo mld-snooping router-aging-time to restore the default.

Syntax

mld-snooping router-aging-time seconds

undo mld-snooping router-aging-time

Default

The aging timer for dynamic router ports is 260 seconds.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies an aging timer for dynamic router ports, in the range of 1 to 8097894 seconds.

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command.

You can set the timer for a VLAN in VLAN view, for a VSI in VSI view, or globally for all VLANs and VSIs in MLD-snooping view. For a VLAN, the VLAN-specific configuration takes priority over the global configuration. For a VSI, the VSI-specific configuration takes priority over the global configuration.

Examples

# In VLAN 2, enable MLD snooping, and set the aging timer for dynamic router ports in the VLAN to 100 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping router-aging-time 100

# In VSI aaa, enable MLD snooping, and set the aging timer for dynamic router ports in the VSI to 100 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping router-aging-time 100

Related commands

enable (MLD-snooping view)

mld-snooping enable

router-aging-time (MLD-snooping view)

MLD snooping commands -- mld-snooping router-port-deny

Use mld-snooping router-port-deny to disable a port from becoming a dynamic router port.

Use undo mld-snooping router-port-deny to allow a port to become a dynamic router port.

Syntax

mld-snooping router-port-deny [ vlan vlan-list ]

undo mld-snooping router-port-deny [ vlan vlan-list ]

Default

A port is allowed to become a dynamic router port.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you specify VLANs, this command takes effect only when the port belongs to the specified VLANs. If you do not specify a VLAN, this command takes effect on all VLANs.

Examples

# Disable GigabitEthernet 1/0/1 from becoming a dynamic router port in VLAN 2.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping router-port-deny vlan 2

MLD snooping commands -- mld-snooping source-deny

Use mld-snooping source-deny to enable IPv6 multicast source port filtering on a port to discard all IPv6 multicast data packets.

Use undo mld-snooping source-deny to disable IPv6 multicast source port filtering on a port.

Syntax

mld-snooping source-deny

undo mld-snooping source-deny

Default

IPv6 multicast source port filtering is disabled.

Views

Layer 2 Ethernet interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You can enable this feature for a port in interface view or for the specified ports in MLD-snooping view. For a port, the configuration in interface view has the same priority as the configuration in MLD-snooping view, and the most recent configuration takes effect.

Examples

# Enable source port filtering for IPv6 multicast data on GigabitEthernet 1/0/1.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping source-deny

Related commands

source-deny (MLD-snooping view)

MLD snooping commands -- mld-snooping special-query source-ip

Use mld-snooping special-query source-ip to configure the source IPv6 address for MLD multicast-address-specific queries.

Use undo mld-snooping special-query source-ip to restore the default.

Syntax

mld-snooping special-query source-ip ipv6-address

undo mld-snooping special-query source-ip

Default

In a VLAN, the source IPv6 address of MLD multicast-address-specific queries is one of the following:

· The source address of MLD general queries if the MLD snooping querier of the VLAN has received MLD general queries.

· The IPv6 link-local address of the current VLAN interface if the MLD snooping querier does not receive an MLD general query.

· FE80::02FF:FFFF:FE00:0001 if the MLD snooping querier does not receive an MLD general query and the current VLAN interface does not have an IPv6 link-local address.

In a VSI, the source IPv6 address of MLD multicast-address-specific queries is one of the following:

· The source address of MLD general queries if the MLD snooping querier of the VSI has received MLD general queries.

· The IPv6 link-local address of the gateway interface for the VSI if the MLD snooping querier does not receive an MLD general query.

· FE80::02FF:FFFF:FE00:0001 if the gateway interface does not have an IPv6 link-local address.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Specifies the source IPv6 address for MLD multicast-address-specific queries.

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you execute this command.

Examples

# In VLAN 2, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address of MLD multicast-address-specific queries.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping special-query source-ip fe80:0:0:1::1

# In VSI aaa, enable MLD snooping, and specify FE80:0:0:1::1 as the source IPv6 address of MLD multicast-address-specific queries.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping special-query source-ip fe80:0:0:1::1

Related commands

enable (MLD-snooping view)

mld-snooping enable

MLD snooping commands -- mld-snooping static-group

Use mld-snooping static-group to configure a port as a static member port of an IPv6 multicast group or an IPv6 multicast source and group.

Use undo mld-snooping static-group to delete the configuration of static member ports.

Syntax

mld-snooping static-group ipv6-group-address [ source-ip ipv6-source-address ] vlan vlan-id

undo mld-snooping static-group { ipv6-group-address [ source-ip ipv6-source-address ] vlan vlan-id | all }

Default

A port is not a static member port of IPv6 multicast groups.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F.

source-ip ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you specify an IPv6 multicast source, this command configures the port as a static member port of an IPv6 multicast source and group. If you do not specify an IPv6 multicast source, this command configures the port as a static member port of an IPv6 multicast group. This option takes effect on MLDv2 snooping devices.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

all: Specifies all IPv6 multicast groups and all IPv6 multicast sources and groups.

Examples

# Configure GigabitEthernet 1/0/1 as a static member port for the IPv6 multicast group (*, FF3E::101) in VLAN 2.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping static-group ff3e::101 vlan 2

MLD snooping commands -- mld-snooping static-router-port

Use mld-snooping static-router-port to configure a port as a static router port.

Use undo mld-snooping static-router-port to remove the configuration of static router ports.

Syntax

mld-snooping static-router-port vlan vlan-id

undo mld-snooping static-router-port { all | vlan vlan-id }

Default

A port is not a static router port.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all VLANs.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

Examples

# Configure GigabitEthernet 1/0/1 as a static router port in VLAN 2.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mld-snooping static-router-port vlan 2

MLD snooping commands -- mld-snooping version

Use mld-snooping version to specify an MLD snooping version for a VLAN or VSI.

Use undo mld-snooping version to restore the default.

Syntax

mld-snooping version version-number

undo mld-snooping version

Default

The MLD snooping version in a VLAN or VSI is 1.

Views

VLAN view

VSI view

Predefined user roles

network-admin

mdc-admin

Parameters

version-number: Specifies an MLD snooping version, 1 or 2.

Usage guidelines

You must enable MLD snooping for a VLAN or VSI before you configure this command.

You can specify the version for a VLAN in VLAN view or for the specified VLANs in MLD-snooping view. The VLAN-specific configuration has the same priority as the configuration in MLD-snooping view, and the most recent configuration takes effect.

Examples

# In VLAN 2, enable MLD snooping, and specify MLD snooping version 2.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 2

[Sysname-vlan2] mld-snooping enable

[Sysname-vlan2] mld-snooping version 2

# In VSI aaa, enable MLD snooping, and specify MLD snooping version 2.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vsi aaa

[Sysname-vsi-aaa] mld-snooping enable

[Sysname-vsi-aaa] mld-snooping version 2

Related commands

enable (MLD-snooping view)

mld-snooping enable

version (MLD-snooping view)

MLD snooping commands -- overflow-replace (MLD-snooping view)

Use overflow-replace to enable the IPv6 multicast group replacement feature globally.

Use undo overflow-replace to disable the IPv6 multicast group replacement feature globally.

Syntax

overflow-replace [ vlan vlan-list ]

undo overflow-replace [ vlan vlan-list ]

Default

The IPv6 multicast group replacement feature is disabled.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094. If you do not specify a VLAN, this command takes effect on all VLANs.

Usage guidelines

This command takes effect only on the IPv6 multicast groups that a port joins dynamically.

You can enable IPv6 multicast group replacement globally for all ports in MLD-snooping view or for a port in interface view. For a port, the port-specific configuration takes priority over the global configuration.

Examples

# Globally enable the IPv6 multicast group replacement feature for VLAN 2.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] overflow-replace vlan 2

Related commands

mld-snooping overflow-replace

MLD snooping commands -- report-aggregation (MLD-snooping view)

Use report-aggregation to enable MLD report suppression.

Use undo report-aggregation to disable MLD report suppression.

Syntax

report-aggregation

undo report-aggregation

Default

MLD report suppression is enabled.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Examples

# Disable MLD report suppression.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] undo report-aggregation

MLD snooping commands -- reset ipv6 l2-multicast fast-forwarding cache

Use reset ipv6 l2-multicast fast-forwarding cache to clear Layer 2 IPv6 multicast fast forwarding entries.

Syntax

Centralized devices:

reset ipv6 l2-multicast fast-forwarding cache [ vlan vlan-id ] { { ipv6-source-address | ipv6-group-address } * | all }

Distributed devices in standalone mode:Centralized IRF devices:

reset ipv6 l2-multicast fast-forwarding cache [ vlan vlan-id ] { { ipv6-source-address | ipv6-group-address } * | all } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset ipv6 l2-multicast fast-forwarding cache [ vlan vlan-id ] { { ipv6-source-address | ipv6-group-address } * | all } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

ipv6-source-address: Specifies an IPv6 multicast source address.

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command clears Layer 2 IPv6 multicast fast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command clears Layer 2 IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command clears Layer 2 IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command clears Layer 2 IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command clears Layer 2 IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

all: Specifies all Layer 2 IPv6 multicast fast forwarding entries.

Examples

# Clear all Layer 2 IPv6 multicast fast forwarding entries.

<Sysname> reset ipv6 l2-multicast fast-forwarding cache all

# Clear the Layer 2 IPv6 multicast fast forwarding entry for the IPv6 group (*, FF1E::2).

<Sysname> reset ipv6 l2-multicast fast-forwarding cache FF1E::2

Related commands

display ipv6 l2-multicast fast-forwarding cache

MLD snooping commands -- reset mld-snooping group

Use reset mld-snooping group to clear information about dynamic MLD snooping group entries.

Syntax

reset mld-snooping group { ipv6-group-address [ ipv6-source-address ] | all } [ vlan vlan-id | vsi vsi-name ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F.

ipv6-source-address: Specifies an IPv6 multicast source address. If you do not specify an IPv6 multicast source, this command clears information about dynamic MLD snooping group entries for all IPv6 multicast sources.

all: Specifies all IPv6 multicast groups.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command clears information about dynamic MLD snooping group entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command clears information about dynamic MLD snooping group entries for all VSIs.

Examples

# Clear information about all dynamic MLD snooping group entries.

<Sysname> reset mld-snooping group all

Related commands

display mld-snooping group

MLD snooping commands -- reset mld-snooping router-port

Use reset mld-snooping router-port to clear dynamic router port information.

Syntax

reset mld-snooping router-port { all | vlan vlan-id | vsi vsi-name }

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all dynamic router ports.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command clears dynamic router port information for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command clears dynamic router port information for all VSIs.

Examples

# Clear information about all dynamic router ports.

<Sysname> reset mld-snooping router-port all

Related commands

display mld-snooping router-port

MLD snooping commands -- reset mld-snooping statistics

Use reset mld-snooping statistics to clear statistics for MLD messages and IPv6 PIM hello messages learned through MLD snooping.

Syntax

reset mld-snooping statistics

Views

User view

Predefined user roles

network-admin

mdc-admin

Examples

# Clear statistics for all MLD messages and IPv6 PIM hello messages learned through MLD snooping.

<Sysname> reset mld-snooping statistics

Related commands

display mld-snooping statistics

MLD snooping commands -- router-aging-time (MLD-snooping view)

Use router-aging-time to set the aging timer for dynamic router ports globally.

Use undo router-aging-time to restore the default.

Syntax

router-aging-time seconds

undo router-aging-time

Default

The aging timer for dynamic router ports is 260 seconds.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies an aging timer for dynamic router ports, in the range of 1 to 8097894 seconds.

Usage guidelines

You can set the timer globally for all VLANs and VSIs in MLD-snooping view, for a VSI in VSI view, or for a VLAN in VLAN view. For a VSI, the VSI-specific configuration takes priority over the global configuration. For a VLAN, the VLAN-specific configuration takes priority over the global configuration.

Examples

# Set the global aging timer for dynamic router ports to 100 seconds.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] router-aging-time 100

Related commands

mld-snooping router-aging-time

MLD snooping commands -- source-deny (MLD-snooping view)

Use source-deny to enable IPv6 multicast source port filtering on ports to discard all IPv6 multicast data packets.

Use undo source-deny to disable IPv6 multicast source port filtering on ports.

Syntax

source-deny port interface-list

undo source-deny port interface-list

Default

IPv6 multicast source port filtering is disabled.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

port interface-list: Specifies a space-separated list of port items. Each item specifies a port by its port type and number or a range of ports in the form of start-interface-type interface-number to end-interface-type interface-number.

Usage guidelines

You can enable this feature for the specified ports in MLD-snooping view or for a port in interface view. For a port, the configuration in MLD-snooping view has the same priority as the configuration in interface view, and the most recent configuration takes effect.

Examples

# Enable source port filtering for IPv6 multicast data on ports GigabitEthernet 1/0/1 through GigabitEthernet 1/0/4.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] source-deny port gigabitethernet 1/0/1 to gigabitethernet 1/0/4

Related commands

mld-snooping source-deny

MLD snooping commands -- version (MLD-snooping view)

Use version to specify an MLD snooping version for VLANs.

Use undo version to restore the default.

Syntax

version version-number vlan vlan-list

undo version vlan vlan-list

Default

The MLD snooping version in a VLAN is 1.

Views

MLD-snooping view

Predefined user roles

network-admin

mdc-admin

Parameters

version-number: Specifies an MLD snooping version, 1 or 2.

vlan vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The VLAN ID is in the range of 1 to 4094.

Usage guidelines

You must enable MLD snooping for the specified VLANs before you execute this command.

You can specify the version for the specified VLANs in MLD-snooping view or for a VLAN in VLAN view. The VLAN-specific configuration has the same priority as the configuration in MLD-snooping view, and the most recent configuration takes effect.

Examples

# Enable MLD snooping for VLAN 2 through VLAN 10, and specify MLD snooping version 2 for these VLANs.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] enable vlan 2 to 10

[Sysname-mld-snooping] version 2 vlan 2 to 10

Related commands

enable (MLD-snooping view)

mld-snooping enable

mld-snooping version