IPv6 IS-IS probe commands -- display system internal isis import-route ipv6

Use display system internal isis import-route ipv6 to display routes redistributed by IPv6 IS-IS.

Syntax

Centralized devices:

display system internal isis import-route ipv6 [ process-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis import-route ipv6 [ process-id ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal isis import-route ipv6 [ process-id ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 635535. If you do not specify this argument, the command displays routes redistributed by all IS-IS processes.

standby slot slot-number: Displays backup routes redistributed by IPv6 IS-IS for a card. If you do not specify this option, the command displays routes redistributed by IPv6 IS-IS. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup routes redistributed by IPv6 IS-IS for an IRF member device. If you do not specify this option, the command displays routes redistributed by IPv6 IS-IS. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup routes redistributed by IPv6 IS-IS for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays routes redistributed by IPv6 IS-IS. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IPv6 IS-IS probe commands -- display system internal isis interface ipv6

Use display system internal isis interface ipv6 to display IPv6 IS-IS interface information.

Syntax

display system internal isis interface ipv6 [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ipv6-address prefix-length ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays interface information for the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number.

ipv6-address: Specifies an IPv6 address.

prefix-length: Specifies the prefix length, an integer in the range of 0 to 128.

IPv6 IS-IS probe commands -- display system internal isis nib ipv6

Use display system internal isis nib ipv6 to display IPv6 IS-IS next hop information.

Syntax

display system internal isis nib ipv6 [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib-id: Specifies a next hop by its ID, a hexadecimal number in the range of 1 to ffffffff. If you do not specify this argument, the command displays information about all next hops.

verbose: Displays detailed IPv6 IS-IS next hop information. If you do not specify this keyword, the command displays brief IPv6 IS-IS next hop information.

IPv6 IS-IS probe commands -- display system internal isis prefix ipv6

Use display system internal isis prefix ipv6 to display IPv6 IS-IS prefix information.

Syntax

Centralized devices:

display system internal isis prefix ipv6 [ [ level-1 | level-2 ] | [ prefix prefix-length ] ] * [ process-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis prefix ipv6 [ [ level-1 | level-2 ] | [ prefix prefix-length ] ] * [ process-id ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal isis prefix ipv6 [ [ level-1 | level-2 ] | [ prefix prefix-length ] ] * [ process-id ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

level-1: Displays IS-IS Level 1 prefix information. If you do not specify this keyword, the command displays both Level 1 and Level 2 prefix information.

level-2: Displays IS-IS Level 2 prefix information. If you do not specify this keyword, the command displays both Level 1 and Level 2 prefix information.

prefix prefix-length: Specifies a prefix and the prefix length.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 635535. If you do not specify this argument, the command displays prefix information for all IS-IS processes.

standby slot slot-number: Displays backup IPv6 IS-IS prefix information for a card. If you do not specify this option, the command displays IPv6 IS-IS prefix information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IPv6 IS-IS prefix information for an IRF member device. If you do not specify this option, the command displays IPv6 IS-IS prefix information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IPv6 IS-IS prefix information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IPv6 IS-IS prefix information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.