2.11 probe commands -- display system internal dot11 characteristics

| NOTE: Support for this command depends on the device model.

Use display system internal dot11 characteristics to display detected 802.11 characteristics information.

Syntax

Centralized devices:

display system internal dot11 characteristics { bss bssid | interface wlan-radio interface-number }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal dot11 characteristics { bss bssid | interface wlan-radio interface-number } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal dot11 characteristics { bss bssid | interface wlan-radio interface-number } chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

bss bssid: Displays the 802.11 characteristics information detected on a BSS in both inbound and outbound directions.

interface wlan-radio interface-number: Displays the 802.11 characteristics information detected on the specified interface.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

2.11 probe commands -- display system internal dot11 verbose

| NOTE: Support for this command depends on the device model.

Use display system internal dot11 verbose to display detailed 802.11 socket information.

Syntax

Centralized devices:

display system internal dot11 verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal dot11 slot slot-number [ cpu cpu-number ] verbose

Distributed devices in IRF mode:

display system internal dot11 chassis chassis-number slot slot-number [ cpu cpu-number ] verbose

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.