IPv6 static routing commands -- delete ipv6 static-routes all

Use delete ipv6 static-routes all to delete all IPv6 static routes.

Syntax

delete ipv6 [ vpn-instance vpn-instance-name ] static-routes all

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command deletes all IPv6 static routes for the public network.

Usage guidelines

When you use this command, the system will prompt you to confirm the operation before deleting all the IPv6 static routes.

Examples

# Delete all IPv6 static routes.

<Sysname> system-view

[Sysname] delete ipv6 static-routes all

This will erase all IPv6 static routes and their configurations, you must reconfigure all static routes.

Are you sure?[Y/N]:y

Related commands

ipv6 route-static

IPv6 static routing commands -- display ipv6 route-static nib

Use display ipv6 route-static nib to display IPv6 static route next hop information.

Syntax

display ipv6 route-static nib [ nib-id ] [ verbose ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

nib-id: Specifies a NIB by its ID, a hexadecimal string in the range of 1 to ffffffff.

verbose: Displays detailed IPv6 static route next hop information. If you do not specify this keyword, the command displays brief IPv6 static route next hop information.

Examples

# Display brief IPv6 static route next hop information.

<Sysname> display ipv6 route-static nib

Total number of nexthop(s): 35

NibID: 0x21000000 Sequence: 0

Type: 0x41 Flushed: Yes

UserKey0: 0x0 VrfNthp: 0

UserKey1: 0x0 Nexthop: 2::3

IFIndex: 0x0 LocalAddr: ::

TopoNthp: Invalid

NibID: 0x21000001 Sequence: 1

Type: 0x41 Flushed: Yes

UserKey0: 0x0 VrfNthp: 0

UserKey1: 0x0 Nexthop: 3::4

IFIndex: 0x0 LocalAddr: ::

TopoNthp: Invalid

...

Table 1 Command output

Field | Description
NibID | ID of the NIB.
Sequence | Sequence number of the NIB.
Type | Type of the NIB.
Flushed | Indicates whether the route with the NIB has been flushed to the FIB.
UserKey0 | Reserved data 1.
UserKey1 | Reserved data 2.
VrfNthp | ‌ Index of the VPN instance to which the next hop belongs. This field displays 0 if the next hop is on an IPv6 network.
Nexthop | Next hop address.
IFIndex | Interface index
LocalAddr | Local interface address.
TopoNthp | ‌ Index of the topology that contains the next hop. This field displays Invalid if the next hop is on an IPv6 network, because the router does not support multiple topologies.

# Display detailed IPv6 static route next hop information. (Applicable to routers.)

<Sysname> display ipv6 route-static nib verbose

Total number of nexthop(s): 35

NibID: 0x21000000 Sequence: 0

Type: 0x41 Flushed: Yes

UserKey0: 0x0 VrfNthp: 0

UserKey1: 0x0 Nexthop: 2::3

IFIndex: 0x0 LocalAddr: ::

TopoNthp: Invalid

RefCnt: 1 FlushRefCnt: 0

Flag: 0x12 Version: 1

1 nexthop(s):

PrefixIndex: 0 OrigNexthop: 2::3

RelyDepth: 2 RealNexthop: ::

Interface: NULL0 LocalAddr: ::

TunnelCnt: 0 Vrf: default-vrf

TunnelID: N/A Topology:

Weight: 0

NibID: 0x21000001 Sequence: 1

Type: 0x41 Flushed: Yes

UserKey0: 0x0 VrfNthp: 0

UserKey1: 0x0 Nexthop: 3::4

IFIndex: 0x0 LocalAddr: ::

TopoNthp: Invalid

RefCnt: 1 FlushRefCnt: 0

Flag: 0x12 Version: 1

1 nexthop(s):

PrefixIndex: 0 OrigNexthop: 3::4

RelyDepth: 1 RealNexthop: ::

Interface: GE1/0/1 LocalAddr: ::

TunnelCnt: 0 Vrf: default-vrf

TunnelID: N/A Topology:

Weight: 0

...

# Display detailed IPv6 static route next hop information. (Applicable to switches.)

<Sysname> display ipv6 route-static nib verbose

Total number of nexthop(s): 35

NibID: 0x21000000 Sequence: 0

Type: 0x41 Flushed: Yes

UserKey0: 0x0 VrfNthp: 0

UserKey1: 0x0 Nexthop: 2::3

IFIndex: 0x0 LocalAddr: ::

TopoNthp: Invalid

RefCnt: 1 FlushRefCnt: 0

Flag: 0x12 Version: 1

1 nexthop(s):

PrefixIndex: 0 OrigNexthop: 2::3

RelyDepth: 2 RealNexthop: ::

Interface: NULL0 LocalAddr: ::

TunnelCnt: 0 Vrf: default-vrf

TunnelID: N/A Topology:

Weight: 0

NibID: 0x21000001 Sequence: 1

Type: 0x41 Flushed: Yes

UserKey0: 0x0 VrfNthp: 0

UserKey1: 0x0 Nexthop: 3::4

IFIndex: 0x0 LocalAddr: ::

TopoNthp: Invalid

RefCnt: 1 FlushRefCnt: 0

Flag: 0x12 Version: 1

1 nexthop(s):

PrefixIndex: 0 OrigNexthop: 3::4

RelyDepth: 1 RealNexthop: ::

Interface: Vlan11 LocalAddr: ::

TunnelCnt: 0 Vrf: default-vrf

TunnelID: N/A Topology:

Weight: 0

...

Table 2 Command output

Field | Description
x nexthop(s) | Number of next hops.
PrefixIndex | Prefix index of the next hop for an ECMP route.
Vrf | ‌ VPN instance name. For an IPv6 network, this field displays default-vrf.
OrigNexthop | Original next hop.
RealNexthop | Real next hop.
Interface | Output interface.
localAddr | Local interface address.
RelyDepth | Recursion depth.
TunnelCnt | ‌ Number of tunnels after route recursion.
TunnelID | ‌ ID of the tunnel after route recursion.
Topology | ‌ Topology name. This field is blank for IPv6, because IPv6 does not support multiple topologies.
Weight | ECMP route weight. This field displays 0 for non-ECMP routes.
RefCnt | Reference count of the next hop.
FlushRefCnt | Reference count of the next hop that is flushed to the FIB.
Flag | Flag of the next hop.
Version | Version of the next hop.

IPv6 static routing commands -- display ipv6 route-static routing-table

Use display ipv6 route-static routing-table to display IPv6 static routing table information.

Syntax

display ipv6 route-static routing-table [ vpn-instance vpn-instance-name ] [ ipv6-address prefix-length ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays IPv6 static routing table information for the public network.

ipv6-address: Specifies the destination IPv6 address.

prefix-length: Specifies the prefix length in the range of 0 to 128.

Examples

# Display IPv6 static routing table information. (Applicable to routers.)

<Sysname> display ipv6 route-static routing-table

Total number of routes: 5

Status: * - valid

*Destination: 1::1/128

NibID: 0x21000000 NextHop: 2::2

MainNibID: N/A BkNextHop: N/A

BkNibID: N/A Interface: GigabitEthernet1/0/1

TableID: 0xa BkInterface: N/A

Flag: 0x80d0a BfdSrcIp: N/A

DbIndex: 0x3 BfdIfIndex: 0x0

Type: Normal BfdVrfIndex: 0

TrackIndex: 0xffffffff Label: NULL

Preference: 60 vrfIndexDst: 0

BfdMode: N/A vrfIndexNH: 0

Permanent: 0 Tag: 0

*Destination: 1::1234/128

NibID: 0x21000000 NextHop: 2::2

MainNibID: N/A BkNextHop: N/A

BkNibID: N/A Interface: NULL0

TableID: 0xa BkInterface: N/A

Flag: 0x80d0a BfdSrcIp: N/A

DbIndex: 0x1 BfdIfIndex: 0x0

Type: Normal BfdVrfIndex: 0

TrackIndex: 0xffffffff Label: NULL

Preference: 60 vrfIndexDst: 0

BfdMode: N/A vrfIndexNH: 0

Permanent: 0 Tag: 0

...

# Display IPv6 static routing table information. (Applicable to switches.)

<Sysname> display ipv6 route-static routing-table

Total number of routes: 5

Status: * - valid

*Destination: 1::1/128

NibID: 0x21000000 NextHop: 2::2

MainNibID: N/A BkNextHop: N/A

BkNibID: N/A Interface: Vlan-interface11

TableID: 0xa BkInterface: N/A

Flag: 0x80d0a BfdSrcIp: N/A

DbIndex: 0x3 BfdIfIndex: 0x0

Type: Normal BfdVrfIndex: 0

TrackIndex: 0xffffffff Label: NULL

Preference: 60 vrfIndexDst: 0

BfdMode: N/A vrfIndexNH: 0

Permanent: 0 Tag: 0

*Destination: 1::1234/128

NibID: 0x21000000 NextHop: 2::2

MainNibID: N/A BkNextHop: N/A

BkNibID: N/A Interface: NULL0

TableID: 0xa BkInterface: N/A

Flag: 0x80d0a BfdSrcIp: N/A

DbIndex: 0x1 BfdIfIndex: 0x0

Type: Normal BfdVrfIndex: 0

TrackIndex: 0xffffffff Label: NULL

Preference: 60 vrfIndexDst: 0

BfdMode: N/A vrfIndexNH: 0

Permanent: 0 Tag: 0

...

Table 3 Command output

Field | Description
Destination | Destination address/prefix.
NibID | ID of the NIB.
MainNibID | ID of the primary next hop for static route FRR.
BkNibID | ID of the backup next hop for static route FRR.
NextHop | Next hop address.
BkNextHop | Backup next hop address.
Interface | Output interface of the route.
BkInterface | Backup output interface.
TableID | ID of the table to which the route belongs.
DbIndex | Index of the database to which the route belongs.
Type | Route type: · Normal. · DHCP. · NAT.
BfdSrcIp | Source IPv6 address of the indirect BFD session.
BfdIfIndex | Index of the interface where BFD is enabled.
BfdVrfIndex | ‌ Index of the VPN instance where BFD is enabled. This field displays 0 if BFD is enabled for an IPv6 network.
BfdMode | BFD session mode: · N/A—No BFD session is configured. · Ctrl—Control packet mode. · Echo—Echo packet mode.
TrackIndex | NQA Track index.
vrfIndexDst | ‌ Index of the VPN instance to which the destination belongs. For an IPv6 network, this field displays 0.
vrfIndexNH | ‌ Index of the VPN instance to which the next hop belongs. For an IPv6 network, this field displays 0.
Permanent | Permanent static route flag. 1 indicates a permanent static route.

IPv6 static routing commands -- ipv6 route-static

Use ipv6 route-static to configure an IPv6 static route.

Use undo ipv6 route-static to remove an IPv6 static route.

Syntax

ipv6 route-static ipv6-address prefix-length { interface-type interface-number [ next-hop-address ] [ bfd { control-packet | echo-packet } [ bfd-source ipv6-address ] | permanent ] | [ vpn-instance d-vpn-instance-name ] next-hop-address [ bfd control-packet bfd-source ipv6-address | permanent ] } [ preference preference ] [ tag tag-value ] [ description text ]

undo ipv6 route-static ipv6-address prefix-length [ interface-type interface-number [ next-hop-address ] | [ vpn-instance d-vpn-instance-name ] next-hop-address ] [ preference preference ]

ipv6 route-static vpn-instance s-vpn-instance-name ipv6-address prefix-length { interface-type interface-number [ next-hop-address ] [ bfd { control-packet | echo-packet } [ bfd-source ipv6-address ] | permanent ] | next-hop-address [ public ] [ bfd control-packet bfd-source ipv6-address | permanent ] | vpn-instance d-vpn-instance-name next-hop-address [ bfd control-packet bfd-source ipv6-address | permanent ] } [ preference preference ] [ tag tag-value ] [ description text ]

undo ipv6 route-static vpn-instance s-vpn-instance-name ipv6-address prefix-length [ interface-type interface-number [ next-hop-address ] | next-hop-address [ public ] | vpn-instance d-vpn-instance-name next-hop-address ] [ preference preference ]

Default

No IPv6 static route is configured.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address prefix-length: Specifies the IPv6 address and prefix length.

interface-type interface-number: Specifies an output interface by its type and number. If the output interface is an NBMA interface or broadcast interface and not a point-to-point (P2P) interface, the next hop address must be specified.

next-hop-address: Specifies the next hop IPv6 address.

bfd: Enables BFD to detect reachability of the static route's next hop.

control-packet: Specifies the BFD control mode.

bfd-source ipv6-address: Specifies the source IPv6 address of BFD packets.

echo-packet: Specifies the BFD echo mode.

permanent: Specifies the IPv6 route as a permanent IPv6 static route. If the output interface is down, the permanent IPv6 static route is still active.

public: Indicates the next hop is on the public network.

vpn-instance d-vpn-instance-name: Specifies a destination MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If a destination VPN is specified, packets will search for the output interface based on the specified next hop (IPv6 address) for the static route.

preference preference: Specifies a preference for IPv6 static routes, in the range of 1 to 255. The default is 60.

tag tag-value: Sets a tag for marking the static route, in the range of 1 to 4294967295. The default is 0. Tags of routes are used for route control in routing policies. For more information about routing policies, see Layer 3—IP Routing Configuration Guide.

description text: Configures a description for the IPv6 static route, which consists of 1 to 60 characters, including special characters such as the space, but excluding the question mark (?).

vpn-instance s-vpn-instance-name: Specifies a source MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. Each VPN has its own routing table, and the configured static route is installed in the routing tables of the specified VPNs.

Usage guidelines

An IPv6 static route that has the destination address configured as ::/0 (a prefix length of 0) is the default IPv6 route. If the destination address of an IPv6 packet does not match any entry in the routing table, this default route is used to forward the packet.

Follow these guidelines to configure the output interface, next hop address, or both for a static route:

· If the output interface is a broadcast interface or an NBMA interface, the next hop address must be specified.

· If the output interface is a P2P interface, you can specify only the output interface. You do not need to change the configuration of the route even if the peer address is changed.

Follow these guidelines when you configure BFD for IPv6 static routes:

· If you specify the source IPv6 address of BFD packets, you must specify the IPv6 address as the next hop IPv6 address on the peer device.

· If you specify a non-P2P output interface and a direct next hop, specify the bfd-source ipv6-address option as a best practice. Make sure the source IPv6 address of BFD packets meets the following requirements:

?span style='font:7.0pt "Times New Roman"'> The address is the same as the IPv6 address of the output interface.

?span style='font:7.0pt "Times New Roman"'> The address is on the same network segment as the next hop IPv6 address of the same type.

For example, if the next hop IPv6 address is a link-local address, the source IPv6 address of BFD packets must also be a link-local address.

Follow these guidelines when you configure a static route:

· Enabling BFD for a flapping route could worsen the route flapping situation. Therefore, use it with caution. For more information about BFD, see High Availability Configuration Guide.

· The next hop IPv6 address of echo packets must be a global unicast address.

· Do not specify the permanent keyword together with the bfd keyword.

Examples

# Configure an IPv6 static route, with the destination address 1:1:2::/64 and next hop 1:1:3::1.

<Sysname> system-view

[Sysname] ipv6 route-static 1:1:2:: 64 1:1:3::1

Related commands

display ipv6 routing-table protocol

IPv6 static routing commands -- ipv6 route-static default-preference

Use ipv6 route-static default-preference to set a default preference for IPv6 static routes.

Use undo ipv6 route-static default-preference to restore the default.

Syntax

ipv6 route-static default-preference default-preference

undo ipv6 route-static default-preference

Default

The default preference of IPv6 static routes is 60.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

default-preference: Specifies a default preference for IPv6 static routes, in the range of 1 to 255.

Usage guidelines

If no preference is specified for an IPv6 static route, the default preference applies.

When the default preference is reconfigured, it applies only to newly added IPv6 static routes.

Examples

# Set a default preference of 120 for IPv6 static routes.

<Sysname> system-view

[Sysname] ipv6 route-static default-preference 120

Related commands

display ipv6 routing-table protocol