RIPng probe commands -- display system internal ripng database standby

Use display system internal ripng database standby to display backup information about active routes in the database for a RIPng process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ripng process-id database standby [ ipv6-address prefix-length ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ripng process-id database standby [ ipv6-address prefix-length ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a RIPng process by its ID in the range of 1 to 65535.

ipv6-address: Specifies an IPv6 address.

prefix-length: Specifies the prefix length in the range of 0 to 128.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIPng probe commands -- display system internal ripng graceful-restart event-log

Use display system internal ripng graceful-restart event-log to display RIPng GR log information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ripng graceful-restart event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ripng graceful-restart event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIPng probe commands -- display system internal ripng interface

Use display system internal ripng interface to display RIPng interface information.

Syntax

display system internal ripng interface [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ipv6-address prefix-length ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays information about the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number.

ipv6-address: Specifies an IPv6 address.

mask-length: Specifies the prefix length in the range of 0 to 128.

RIPng probe commands -- display system internal ripng interface standby

Use display system internal ripng interface standby to display backup interface information for a RIPng process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ripng process-id interface standby [ interface-type interface-number ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ripng process-id interface standby [ interface-type interface-number ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a RIPng process by its ID in the range of 1 to 65535.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays backup information about all interfaces for the RIPng process.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIPng probe commands -- display system internal ripng neighbor standby

Use display system internal ripng neighbor standby to display backup neighbor information for a RIPng process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ripng process-id neighbor standby [ interface-type interface-number ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ripng process-id neighbor standby [ interface-type interface-number ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a RIPng process by its ID in the range of 1 to 65535.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays backup neighbor information for all interfaces.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIPng probe commands -- display system internal ripng nib

Use display system internal ripng nib to display next hop information of RIPng routes.

Syntax

display system internal ripng nib [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib-id: Specifies a next hop by its ID in the range of 1 to FFFFFFFF. If you do not specify this argument, the command displays information about all next hops.

verbose: Displays the detailed next hop information.

RIPng probe commands -- display system internal ripng nib log

Use display system internal ripng nib log to display logs of next hops for RIPng routes.

Syntax

display system internal ripng nib log

Views

Probe view

Predefined user roles

network-admin

mdc-admin

RIPng probe commands -- display system internal ripng non-stop-routing event-log

Use display system internal ripng non-stop-routing event-log to display RIPng NSR log information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ripng non-stop-routing event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ripng non-stop-routing event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIPng probe commands -- display system internal ripng route standby

Use display system internal ripng route standby to display backup routing information for a RIPng process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ripng process-id route standby [ ipv6-address prefix-length [ verbose ] | peer ipv6-address | statistics ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ripng process-id route standby [ ipv6-address prefix-length [ verbose ] | peer ipv6-address | statistics ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a RIPng process by its ID in the range of 1 to 65535.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIPng probe commands -- display system internal ripng status

Use display system internal ripng status to display global RIPng status information.

Syntax

display system internal ripng status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

RIPng probe commands -- reset system internal ripng graceful-restart event-log

Use reset system internal ripng graceful-restart event-log to clear RIPng GR log information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ripng graceful-restart event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal ripng graceful-restart event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIPng probe commands -- reset system internal ripng non-stop-routing event-log

Use reset system internal ripng non-stop-routing event-log to clear RIPng NSR log information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ripng non-stop-routing event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal ripng non-stop-routing event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents its IRF member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.