Device management probe commands -- cellular-diag enable type filter

| NOTE: Support for this command depends on the device model.

Use cellular-diag enable type filter to enable offline 3G/4G diagnosing for the Comware 7 system.

Use undo cellular-diag enable to disable both online 3G/4G diagnosing and offline 3G/4G diagnosing for the Comware 7 system.

Syntax

cellular-diag enable type filter filter-file-name { local file-url | remote tftp-server-address tftp-file-name } cellular interface-number

undo cellular-diag enable

Default

Offline 3G/4G diagnosing is disabled for the Comware 7 system.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

filter-file-name: Specifies the name of the file that defines the diagnostic information filtering rules.

local file-url: Saves diagnostic information to a local file. The file-url argument specifies the file name.

remote tftp-server-address: Saves diagnostic information to a TFTP server. The tftp-server-address argument specifies the IP address of the TFTP server.

tftp-file-name: Specifies the name of the file for saving diagnostic information on the TFTP server.

cellular interface-number: Specifies a cellular interface by its number.

Device management probe commands -- cellular-diag enable type virtual-com

| NOTE: Support for this command depends on the device model.

Use cellular-diag enable type virtual-com to enable online 3G/4G diagnosing for the Comware 7 system.

Use undo cellular-diag enable to disable both online and offline 3G/4G diagnosing for the Comware 7 system.

Syntax

cellular-diag enable type virtual-com port-number cellular interface-number

undo cellular-diag enable

Default

Online 3G/4G diagnosing is disabled for the Comware 7 system.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

port number: Specifies the online diagnosing service port number on a PC, in the range of 1024 to 65535. Make sure the online diagnosing software is running on the PC.

cellular interface-number: Specifies a cellular interface by its number.

Device management probe commands -- debugging transceiver

Use debugging transceiver to enable or disable debugging for transceiver features.

Syntax

debugging transceiver { mibcache | moduleinfo | read_write_retry } { disable | enable } interface [ interface-type interface-number ]

Default

Debugging is disabled for all transceiver features.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

mibcache: Specifies debugging for the transceiver MIB node information retrieving feature. In debugging mode, upper-layer modules must obtain data from the transceiver and calculate MIB node values. In non-debugging mode, the system periodically retrieves data from the transceiver in the background to calculate MIB node values, and saves the values in memory. Upper-layer modules use the values saved in memory.

moduleinfo: Specifies debugging for the transceiver parameters retrieving feature. In debugging mode, upper-layer modules must obtain transceiver information from the transceiver. In non-debugging mode, the system retrieves transceiver information from a transceiver when it detects a transceiver, and saves the information in memory. Upper-layer modules use the information saved in memory.

read_write_retry: Specifies debugging for the auto read and write feature. In non-debugging mode, the system automatically reads or writes transceiver information again upon detecting checksum errors in transceiver information. In debugging mode, the system does not read or write transceiver information again, even if the transceiver information has checksum errors.

disable: Enables debugging.

enable: Disables debugging.

interface [ interface-type interface-number ]: Specifies an interface by its type and number. If you do not specify the interface-type interface-number option, the command enables or disables debugging for internal transceiver features on all interfaces.

Device management probe commands -- display hardware internal physical cellular

| NOTE: Support for this command depends on the device model.

Use display hardware internal physical cellular to display the 3G/4G diagnostic information for the Comware 7 system.

Syntax

display hardware internal physical cellular interface-number diag_info

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface number: Specifies a cellular interface by its number.

Device management probe commands -- display hardware internal transceiver register interface

| NOTE: Support for this command depends on the device model.

Use display hardware internal transceiver register interface to display the content of a register area on a transceiver module.

Syntax

display hardware internal transceiver register interface interface-type interface-number device device-index address start-address length region-length

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

device device-index: Specifies the index of an internal register in hexadecimal notation. The value range is 0 to ff.

address start-address: Specifies the offset of the register area to the beginning of the register, in hexadecimal notation. The value range is 0 to ffff.

length region-length: Specifies the length of the register area in bytes. The value range is 1 to 256.

Device management probe commands -- display system internal dbm

Use display system internal dbm to display database information.

Syntax

Centralized devices:

display system internal dbm { all | name dbname [ key keyname ] }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal dbm { all | name dbname [ key keyname ] } [ slot slot-number ]

Distributed devices in IRF mode:

display system internal dbm { all | name dbname [ key keyname ] } [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all databases.

name dbname: Specifies a database name.

key keyname: Specifies the name of the key for the database.

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays database information for the master. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or a PEX, this command displays database information for the master. (Centralized IRF devices.) (IRF 3 capable.)

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays database information for the active MPU. (Distributed devices in standalone mode.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays database information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card, this command displays database information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

Device management probe commands -- display system internal process state

Use display system internal process state to display service operating status information.

Syntax

Centralized devices:

display system internal process state

Distributed devices in standalone mode:Centralized IRF devices:

display system internal process state [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal process state [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Device management probe commands -- display transceiver information

Use display transceiver information to display detailed transceiver information.

Syntax

display transceiver information interface [ interface-type interface-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface [ interface-type interface-number ]: Specifies an interface by its type and number. If you do not specify this option, the command displays detailed information about transceivers on all interfaces.

Device management probe commands -- display transceiver moduleinfo

Use display transceiver moduleinfo to display core transceiver data structure information used in the software.

Syntax

display transceiver moduleinfo interface [ interface-type interface-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface [ interface-type interface-number ]: Specifies an interface by its type and number. If you do not specify the interface-type interface-number option, the command displays information about transceivers on all interfaces.

Device management probe commands -- display transceiver register

Use display transceiver register to display transceiver register information.

Syntax

display transceiver register interface [ interface-type interface-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface [ interface-type interface-number ]: Specifies an interface by its type and number. If you do not specify the interface-type interface-number option, the command displays information about transceivers on all interfaces.