CFD probe commands -- debugging system internal cfd

Use debugging system internal cfd to enable CFD debugging.

Use undo debugging system internal cfd to disable CFD debugging.

Syntax

debugging system internal cfd { error | hardware }

undo debugging system internal cfd { error | hardware }

Default

CFD debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

error: Debugging for CFD errors.

hardware: Debugging for CFD hardware.

CFD probe commands -- display system internal cfd hardware

Use display system internal cfd hardware to display CFD hardware information.

Syntax

Centralized devices:

display system internal cfd hardware level level-value [ vlan vlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal cfd hardware slot slot-number level level-value [ vlan vlan-id ]

Distributed devices in IRF mode:

display system internal cfd hardware chassis chassis-number slot slot-number level level-value [ vlan vlan-id ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Displays CFD hardware information on a card. The slot-number argument represents the number of the slot that holds the card. (Distributed devices in standalone mode.)

slot slot-number: Displays CFD hardware information on an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Displays CFD hardware information on a card in an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the number of the slot that holds the card. (Distributed devices in IRF mode.)

level level-value: Specifies an MD level in the range of 0 to 7.

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094. If no VLAN is specified, the command displays CFD hardware information without VLAN attributes.

CFD probe commands -- display system internal cfd mep

Use display system internal cfd mep to display MEP information.

Syntax

Centralized devices:

display system internal cfd mep mep-id service-instance instance-id

Distributed devices in standalone mode:Centralized IRF devices:

display system internal cfd mep mep-id service-instance instance-id slot slot-number

Distributed devices in IRF mode:

display system internal cfd mep mep-id service-instance instance-id chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

mep-id: Specifies a MEP by its ID in the range of 1 to 8191.

service-instance instance-id: Specifies a service instance by its ID in the range of 1 to 32767.

slot slot-number: Displays MEP information on a card. The slot-number argument represents the number of the slot that holds the card. (Distributed devices in standalone mode.)

slot slot-number: Displays MEP information on an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Displays MEP information on a card in an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the number of the slot that holds the card. (Distributed devices in IRF mode.)