MTR probe commands -- debugging system internal ip topology

Use debugging system internal ip topology to enable topology debugging.

Use undo debugging system internal ip topology to disable topology debugging.

Syntax

Centralized devices:

debugging system internal ip topology

undo debugging system internal ip topology

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal ip topology [ slot slot-number [ cpu cpu-number ] ]

undo debugging system internal ip topology [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

debugging system internal ip topology [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

undo debugging system internal ip topology [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Default

Topology debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the number of the slot that holds the card. If you do not specify this option, the command enables topology debugging for the global active MPU. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

MTR probe commands -- display system internal ip topology

Use display system internal ip topology to display topology information.

Syntax

Centralized devices:

display system internal ip topology [ topology-name | statistics ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip topology [ topology-name | statistics ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ip topology [ topology-name | statistics ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

topology-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this argument, the command displays information about all topologies.

statistics: Displays topology statistics.

slot slot-number: Specifies a card by its slot number. If you do not specify this option, the command displays topology information on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. If you do not specify this option, the command displays topology information on the master device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the number of the slot that holds the card. If you do not specify this option, the command displays topology information on the global active MPU. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

MTR probe commands -- display system internal ip topology inactive

Use display system internal ip topology inactive to display inactive topology information.

Syntax

display system internal ip topology inactive

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

You can use this command to display information about topologies that are being deleted.