RIP probe commands -- display system internal rip database standby

Use display system internal rip database standby to display backup active route information in the database for a RIP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rip process-id database standby [ ip-address { mask-length | mask } ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rip process-id database standby [ ip-address { mask-length | mask } ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a RIP process by its ID in the range of 1 to 65535.

ip-address: Specifies the destination IP address, in dotted decimal notation.

mask: Specifies the subnet mask, in dotted decimal notation.

mask-length: Specifies the mask length in the range of 0 to 32.

standby slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIP probe commands -- display system internal rip graceful-restart event-log

Use display system internal rip graceful-restart event-log to display RIP GR event logs.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rip graceful-restart event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rip graceful-restart event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIP probe commands -- display system internal rip interface

Use display system internal rip interface to display RIP interface information.

Syntax

display system internal rip interface [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ip-address { mask | mask-length } ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, the command displays information about the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number.

ip-address: Specifies an IP address, in dotted decimal notation.

mask: Specifies the subnet mask, in dotted decimal notation.

mask-length: Specifies the mask length in the range of 0 to 32.

RIP probe commands -- display system internal rip interface standby

Use display system internal rip interface standby to display backup interface information for a RIP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rip process-id interface standby [ interface-type interface-number ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rip process-id interface standby [ interface-type interface-number ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

process-id: Specifies a RIP process by its ID in the range of 1 to 65535.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays information about all RIP interfaces.

standby slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIP probe commands -- display system internal rip neighbor standby

Use display system internal rip neighbor standby to display backup neighbor information for a RIP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rip process-id neighbor standby [ interface-type interface-number ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rip process-id neighbor standby [ interface-type interface-number ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a RIP process by its ID in the range of 1 to 65535.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays information about all RIP interfaces.

standby slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIP probe commands -- display system internal rip nib

Use display system internal rip nib to display next hop information of RIP routes.

Syntax

display system internal rip nib [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib-id: Specifies a next hop by its ID, a hexadecimal number in the range of 1 to ffffffff. If you do not specify a next hop, the command displays information about all next hops.

verbose: Displays the detailed next hop information.

RIP probe commands -- display system internal rip nib log

Use display system internal rip nib log to display logs of next hops for RIP routes.

Syntax

display system internal rip nib log

Views

Probe view

Predefined user roles

network-admin

mdc-admin

RIP probe commands -- display system internal rip non-stop-routing event-log

Use display system internal rip non-stop-routing event-log to display RIP NSR event logs.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rip non-stop-routing event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rip non-stop-routing event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIP probe commands -- display system internal rip route standby

Use display system internal rip route standby to display backup routing information for a RIP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rip process-id route standby [ ip-address { mask-length | mask } [ verbose ] | peer ip-address | statistics ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rip process-id route standby [ ip-address { mask-length | mask } [ verbose ] | peer ip-address | statistics ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a RIP process by its ID in the range of 1 to 65535.

ip-address: Specifies the destination IP address, in dotted decimal notation.

mask: Specifies the subnet mask, in dotted decimal notation.

mask-length: Specifies the mask length in the range of 0 to 32.

verbose: Displays all routing information for the specified destination IP address. If you do not specify this keyword, the command displays only information about optimal routes with the specified destination IP address.

peer ip-address: Displays routing information learned from the specified neighbor.

statistics: Displays route statistics, including the total number of routes and number of routes learned from each neighbor.

standby slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIP probe commands -- display system internal rip status

Use display system internal rip status to display global RIP status information.

Syntax

display system internal rip status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

RIP probe commands -- reset system internal rip graceful-restart event-log

Use reset system internal rip graceful-restart event-log to clear the RIP GR event logs.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal rip graceful-restart event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal rip graceful-restart event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

RIP probe commands -- reset system internal rip non-stop-routing event-log

Use reset system internal rip non-stop-routing event-log to clear the RIP NSR event logs.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal rip non-stop-routing event-log slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal rip non-stop-routing event-log chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card of an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.