WLAN mesh commands -- akm mode sae

Use akm mode sae to set the authentication and key management mode to simultaneous authentication of equals (SAE).

Use undo akm mode to restore the default.

Syntax

akm mode sae

undo akm mode

Default

The authentication and key management mode is not set.

Views

Mesh profile view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Make sure the mesh profile is disabled before you configure or remove its authentication and key management mode setting.

Examples

# Set the authentication and key management mode to SAE in mesh profile 1.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1] akm mode sae

Related commands

display wlan mesh-profile

WLAN mesh commands -- display wlan mesh-link (on fat APs)

Use display wlan mesh-link to display mesh link information.

Syntax

display wlan mesh-link [ mesh-profile mesh-profile-number | interface interface-type interface-number | peer-mac-address mac-address ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

mesh-profile mesh-profile-number: Specifies a mesh profile by its profile number. The value range is 1 to 65535.

interface interface-type interface-number: Specifies an interface by its type and number.

peer-mac-address mac-address: Specifies a peer MP by its MAC address in H-H-H format.

Usage guidelines

If you do not specify any parameters, this command displays information about all mesh links.

Examples

# Display information about all mesh links.

<Sysname> display wlan mesh-link

Peer MAC RSSI BSSID Interface Link state Online time

7b2d-23bb-e56f 22 4a1b-517d-23ff WLAN-MeshLink1 Active 00h 08m 31s

6a3b-cc5a-e215 22 4a1b-517d-23ff WLAN-MeshLink2 Active 00h 40m 56s

Table 1 Command output

Field | Description
Peer MAC | MAC address of the peer MP.
Interface | WLAN mesh link interface.
Link state | Link status: · Active—Active link. · Active(T)—Active temporary link.
Online time | Amount of time that the mesh link has been active.

WLAN mesh commands -- display wlan mesh-link ap (on ACs)

Use display wlan mesh-link ap to display mesh link information for APs.

Syntax

display wlan mesh-link ap [ name ap-name [ verbose ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

name ap-name: Specifies an AP by its name, a case-insensitive string of 1 to 64 characters. The string can contain alphanumeric characters, underscores (_), brackets ([]), slashes (/), and hyphens (-). If you do not specify an AP, this command displays mesh link information for all APs.

verbose: Displays detailed mesh link information. If you do not specify this keyword, the command displays brief mesh link information.

Examples

# Display brief mesh link information for AP ap1.

<Sysname> display wlan mesh-link ap name ap1

AP name: ap1

Peer Local Status RSSI Packets(Rx/Tx)

4ab7-c78a-22ff 75bb-c36d-4ef8 Forwarding 22 0/0

Table 2 Command output

Field | Description
Peer | MAC address of the peer MP.
Local | MAC address of the local AP.
Status | Status of the link. This field displays Forwarding if the mesh link is forwarding traffic.
RSSI | RSSI of the mesh link.
Packets(Rx/Tx) | Packet statistics for the mesh link: Rx—Number of received packets. Tx—Number of sent packets.

# Display detailed mesh link information for AP ap1.

<Sysname> display wlan mesh-link ap name ap1 verbose

AP name: ap1

Peer MAC : 4ab7-c78a-22ff

Local MAC : 75bb-c36d-4ef8

Status : Forwarding

RSSI : 67

SNR : 76

Noise : 0 dBm

Cost : 0

Incorrect packets : 0.00 %

Packets

Received : 170

Sent : 157

Resent : 0

Lost : 0

Table 3 Command output

Field | Description
Peer MAC | MAC address of the peer MP.
Local MAC | MAC address of the local AP.
Status | Status of the link. This field displays Forwarding if the mesh link is forwarding traffic.
RSSI | RSSI of the mesh link.
SNR | Signal to noise ratio.
Cost | Link cost.
Incorrect packets | Percentage of sent packets that encountered transmission errors.
Received | Total number of received packets.
Sent | Total number of sent packets.
Resent | Number of retransmitted packets.
Lost | Number of lost packets.

WLAN mesh commands -- display wlan mesh-policy

Use display wlan mesh-policy to display mesh policy information.

Syntax

display wlan mesh-policy [ mesh-policy-name ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

mesh-policy-name: Specifies a mesh policy by its name, a case-insensitive string of 1 to 31 characters. If you do not specify a policy name, this command displays information about all mesh policies.

Examples

# Display information about all mesh policies.

<Sysname> display wlan mesh-policy

Mesh policy name : default_mesh_policy

Mesh link initiation : Enabled

MLSP : Disabled

Max links : 2

Probe request interval : 1000 ms

Link hold RSSI : 15 dBm

Link hold time : 4000 ms

Link switch margin : 10 dBm

Link saturation RSSI : 150 dBm

Link rate mode : fixed

Mesh policy name : abc

Mesh link initiation : Enabled

MLSP : Disabled

Max links : 2

Probe request interval : 1000 ms

Link hold RSSI : 15 dBm

Link hold time : 15 ms

Link switch margin : 10 dBm

Link saturation RSSI : 10 dBm

Link rate mode : fixed

Mesh policy name : bb

Mesh link initiation : Enabled

MLSP : Disabled

Max links : 2

Probe request interval : 1000 ms

Link hold RSSI : 15 dBm

Link hold time : 15 ms

Link switch margin : 10 dBm

Link saturation RSSI : 10 dBm

Link rate mode : Fixed

Table 4 Command output

Field | Description
Mesh link initiation | Status of the mesh link initiation feature: · Enabled. · Disabled.
MLSP | Status of the MLSP feature: · Enabled. · Disabled.
Max links | Maximum number of links.
Link rate mode | Link rate mode: · Fixed—The link operates at a fixed rate. · Real-time—The link rate adapts to RSSI in real time.

WLAN mesh commands -- display wlan mesh-profile

Use display wlan mesh-profile to display mesh profile information.

Syntax

display wlan mesh-profile [ mesh-profile-number ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

mesh-profile-number: Specifies a mesh profile by its number in the range of 1 to 65535. If you do not specify a mesh profile, this command displays information about all mesh profiles.

Examples

# Display information about all mesh profiles.

<Sysname> display wlan mesh-profile

Mesh profile number : 1

Mesh ID : 11

Link keepalive interval : 2 s

Link backhaul rate : 18 Mbps

Mesh profile status : Enabled

Link metric type : Not Configured

AKM mode : None

PSK status : Disabled

Mesh profile number : 2

Mesh ID : 22

Link keepalive interval : 2 s

Link backhaul rate : 18 Mbps

Mesh profile status : Enabled

Link metric type : Not Configured

AKM mode : None

PSK status : Disabled

Table 5 Command output

Field | Description
Mesh profile status | Status of the mesh profile: · Enabled. · Disabled.
AKM mode | Authentication and key management mode: · None—No authentication and key management mode is specified. · SAE—SAE mode is specified.
PSK status | Preshared key configuration status: · Enabled—A preshared key is configured. · Disabled—No preshared key is configured.

WLAN mesh commands -- link-backhaul-rate

Use link-backhaul-rate to set the backhaul rate for mesh links.

Use undo link-backhaul-rate to restore the default.

Syntax

link-backhaul-rate rate

undo link-backhaul-rate

Default

The backhaul rate for mesh links is 18 Mbps.

Views

Mesh profile view

Predefined user roles

network-admin

mdc-admin

Parameters

rate: Specifies a backhaul rate in Mbps. Available values are 1, 2, 5.5, 6, 9, 11, 12, 18, 24, 36, 48, and 54.

Usage guidelines

Make sure the mesh profile is disabled before you set the backhaul rate. The MPs on a mesh link must have the same backhaul rate.

Backhaul rate is the allowed incoming packet rate on a mesh link.

Examples

# Set the backhaul rate to 5.5 Mbps in mesh profile 1.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1] link-backhaul-rate 5.5

Related commands

display wlan mesh-profile

WLAN mesh commands -- link-hold-rssi

Use link-hold-rssi to set the mesh link hold RSSI, the minimum signal strength for a mesh link to be retained.

Use undo link-hold-rssi to restore the default.

Syntax

link-hold-rssi value

undo link-hold-rssi

Default

The mesh link hold RSSI is 15 dBm.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies the mesh link hold RSSI in the range of 5 to 100 dBm.

Examples

# Set the mesh link hold RSSI to 24 dBm in mesh policy abc.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] link-hold-rssi 24

Related commands

display wlan mesh-policy

WLAN mesh commands -- link-hold-time

Use link-hold-time to set the link hold time, the minimum amount of time before a link switchover can occur.

Use undo link-hold-time to restore the default.

Syntax

link-hold-time value

undo link-hold-time

Default

The mesh link hold time is 4000 milliseconds.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies a time value in the range of 1000 to 20000 milliseconds.

Examples

# Set the link hold time to 5000 milliseconds in mesh policy abc.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] link-hold-time 5000

Related commands

display wlan mesh-policy

WLAN mesh commands -- link-initiation enable

Use link-initiation enable to enable mesh link initiation.

Use undo link-initiation enable to disable mesh link initiation.

Syntax

link-initiation enable

undo link-initiation enable

Default

Mesh link initiation is enabled.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Mesh link initiation enables the MP to send Link Open requests to a peer without having received a Link Open request from that peer. If this feature is disabled, the MP must wait for a Link Open request from its peer before it can send one.

Examples

# Disable mesh link initiation.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] undo link-initiation enable

Related commands

display wlan mesh-policy

WLAN mesh commands -- link-keepalive

Use link-keepalive to set the mesh link keepalive interval.

Use undo link-keepalive to restore the default.

Syntax

link-keepalive keepalive-interval

undo link-keepalive

Default

The mesh link keepalive interval is 2 seconds.

Views

Mesh profile view

Predefined user roles

network-admin

mdc-admin

Parameters

keepalive-interval: Specifies a keepalive interval in the range of 1 to 1800 seconds.

Usage guidelines

MPs on a mesh link use keepalive packets to detect mesh link status. The MP with a higher MAC address sends keepalive packets at the keepalive interval to the peer end. The sending MP disconnects the mesh link if it has not received a reply before three consecutive keepalive intervals expire. The receiving MP disconnects the mesh link if it has not received keepalive packets before three consecutive keepalive intervals expire. For correct link status detection, the keepalive interval at the sending end must be equal to or less than three times the keepalive interval at the receiving end.

Examples

# Set the mesh link keepalive interval to 6 seconds in mesh profile 1.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1] link-keepalive 6

Related commands

display wlan mesh-profile

WLAN mesh commands -- link-maximum-number

Use link-maximum-number to set the maximum number of mesh links on a radio.

Use undo link-maximum-number to restore the default.

Syntax

link-maximum-number max-link-number

undo link-maximum-number

Default

A maximum of two mesh links can be established on a radio.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Parameters

max-link-number: Specifies a limit in the range of 1 to 8.

Usage guidelines

The MP will stop establishing new mesh links on a radio after the maximum number of mesh links is reached.

Examples

# Set the maximum number of mesh links to 5 in mesh policy abc.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] link-maximum-number 5

Related commands

display wlan mesh-policy

WLAN mesh commands -- link-metric

Use link-metric rssi to use RSSI as a mesh routing metric.

Use undo link-metric to restore the default.

Syntax

link-metric rssi

undo link-metric

Default

RSSI is not a mesh routing metric.

Views

Mesh profile view

Predefined user roles

network-admin

mdc-admin

Examples

# Use RSSI as a mesh routing metric.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1] link-metric rssi

WLAN mesh commands -- link-rate-mode

Use link-rate-mode to set the link rate mode for mesh links.

Use undo link-rate-mode to restore the default.

Syntax

link-rate-mode { fixed | real-time }

undo link-rate-mode

Default

The default link rate mode for mesh links is fixed mode.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Parameters

fixed: Specifies the fixed mode. In fixed mode, the interface rate of the mesh link is fixed at the maximum value in the current set of radio interface rates.

real-time: Specifies the real-time mode. In real-time mode, the interface rate of the mesh link automatically adapts to RSSI.

Examples

# Specify the real-time mesh link rate mode in mesh policy abc.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] link-rate-mode real-time

Related commands

display wlan mesh-policy

WLAN mesh commands -- link-saturation-rssi

Use link-saturation-rssi to set the link saturation RSSI.

Use undo link-saturation-rssi to restore the default.

Syntax

link-saturation-rssi value

undo link-saturation-rssi

Default

The link saturation RSSI is 150 dBm.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies a link saturation RSSI value in the range of 30 to 150 dBm.

Usage guidelines

Link switchover occurs when the RSSI on an active link exceeds the saturation RSSI.

Examples

# Set the link saturation RSSI to 50 dBm in mesh policy abc.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] link-saturation-rssi 50

Related commands

display wlan mesh-policy

WLAN mesh commands -- link-switch-margin

Use link-switch-margin to set the link switchover margin.

Use undo link-switch-margin to restore the default.

Syntax

link-switch-margin value

undo link-switch-margin

Default

The link switchover margin is 10 dBm.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies a link switchover margin in the range of 1 to 100 dBm.

Usage guidelines

The standby link takes over if its RSSI minus the RSSI on the active link is higher than the link switchover margin.

Examples

# Set the link switchover margin to 50 dBm in mesh policy abc.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] link-switch-margin 50

Related commands

display wlan mesh-policy

WLAN mesh commands -- mesh peer-mac-address

Use mesh peer-mac-address to add an MP to the mesh peer whitelist.

Use undo mesh peer-mac-address to remove MPs from the mesh peer whitelist.

Syntax

mesh peer-mac-address mac-address

undo mesh peer-mac-address { mac-address | all }

Default

The mesh peer whitelist is empty.

Views

ACs:

Radio view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Parameters

mac-address: Specifies the MAC address of an MP in H-H-H format.

all: Removes all MAC addresses from the mesh peer whitelist.

Usage guidelines

Mesh peer whitelist ensures that an MP establishes mesh links only with legitimate MPs.

If you do not configure a whitelist, an MP can establish peer relationships with any MP neighbors.

Examples

# Add the MAC address of an MP to the mesh peer whitelist.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] mesh peer-mac-address 4ab7-c78a-22ff

WLAN mesh commands -- mesh-id

Use mesh-id to assign a mesh ID to a mesh profile.

Use undo mesh-id to restore the default.

Syntax

mesh-id mesh-id

undo mesh-id

Default

A mesh profile does not contain a mesh ID.

Views

Mesh profile view

Predefined user roles

network-admin

mdc-admin

Parameters

mesh-id: Specifies a mesh ID, a case-sensitive string of 1 to 32 characters.

Usage guidelines

The mesh ID in each mesh profile must be unique.

MPs on the same mesh network must use the same mesh ID.

Examples

# Assign mesh ID mesh to mesh profile 1.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1] mesh-id mesh

Related commands

display wlan mesh-profile

WLAN mesh commands -- mesh-policy

Use mesh-policy to bind a mesh policy to a radio.

Use undo mesh-policy to restore the default.

Syntax

mesh-policy policy-name

undo mesh-policy

Default

Default mesh policy default_mesh_policy is bound to radios.

Views

ACs:

Radio view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Parameters

policy-name: Specifies a mesh policy by its name, a case-insensitive string of 1 to 31 characters.

Usage guidelines

You can bind only one mesh policy to a radio. If you execute this command multiple times, the most recent binding takes effect.

Examples

ACs:

# Bind mesh policy abc to radio 1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] mesh-policy abc

Fat APs:

# Bind mesh policy abc to WLAN-Radio 1/0/2.

<Sysname> system-view

[Sysname] interface wlan-radio 1/0/2

[Sysname-WLAN-Radio1/0/2] mesh-policy abc

Related commands

wlan mesh-policy

WLAN mesh commands -- mesh-profile

Use mesh-profile to bind a mesh profile to a radio.

Use undo mesh-profile to restore the default.

Syntax

mesh-profile mesh-profile-number

undo mesh-profile mesh-profile-number

Default

No mesh profile is bound to radios.

Views

ACs:

Radio view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Parameters

mesh-profile-number: Specifies a mesh profile by its number in the range of 1 to 65535.

Usage guidelines

You can bind only one mesh profile to a radio. To bind a new mesh profile to a radio, you must first remove the old mesh profile from the radio.

Examples

ACs:

# Bind mesh profile 1 to radio 1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] mesh-profile 1

Fat APs:

# Bind mesh profile 1 to WLAN-Radio 1/0/2.

<Sysname> system-view

[Sysname] interface wlan-radio 1/0/2

[Sysname-WLAN-Radio1/0/2] mesh-profile 1

Related commands

mesh-profile enable

wlan mesh-profile

WLAN mesh commands -- mesh-profile enable

Use mesh-profile enable to enable a mesh profile.

Use undo mesh-profile enable to disable a mesh profile.

Syntax

mesh-profile enable

undo mesh-profile enable

Default

A mesh profile is disabled.

Views

Mesh profile view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Before you enable a mesh profile, you must assign it a mesh ID.

Examples

# Enable mesh profile 1.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1] mesh-profile enable

Related commands

mesh-id

WLAN mesh commands -- portal-service enable

Use portal-service enable to disable an MPP from sending probe requests.

Use undo portal-service enable to restore the default.

Syntax

portal-service enable

undo portal-service enable

Default

MPPs can send probe requests.

Views

ACs:

AP view

Fat APs:

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

As the point that connects the WLAN mesh network to a wired network, an MPP might need to establish a large number of mesh links. To maintain its performance, you can disable the MPP from sending probe requests for neighbor discovery. The MPP will only respond to the probe requests from other MPs.

Examples

ACs:

# Disable an MPP from sending probe requests.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] portal-service enable

Fat APs:

# Disable the MPP from sending probe requests.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] portal-service enable

WLAN mesh commands -- preshared-key

Use preshared-key to add a preshared key to a mesh profile.

Use undo preshared-key to restore the default.

Syntax

preshared-key { pass-phrase | raw-key } { cipher | simple } string

undo preshared-key

Default

A mesh profile does not contain a preshared key.

Views

Mesh profile view

Predefined user roles

network-admin

mdc-admin

Parameters

pass-phrase: Sets the key in character string form.

raw-key: Sets the key in hexadecimal form.

cipher: Specifies the key in encrypted form.

simple: Specifies the key in plaintext form. For security purposes, the key specified in plaintext form will be stored in encrypted form.

string: Specifies a case-sensitive key string. The following are the key length ranges:

· pass-phrase plaintext—8 to 63 characters.

· pass-phrase ciphertext—41 to 117 characters.

· raw-key plaintext—64 hexadecimal digits.

· raw-key ciphertext—117 characters.

Usage guidelines

Make sure the mesh profile is disabled before you use this command.

You can configure only one preshared key in a mesh profile. If you execute this command multiple times, the most recent configuration takes effect.

Examples

# Add preshared key abcdefghig in plain text to mesh profile 1.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1] preshared-key pass-phrase simple abcdefghig

Related commands

display wlan mesh-profile

WLAN mesh commands -- probe-request-interval

Use probe-request-interval to set the probe request interval.

Use undo probe-request-interval to restore the default.

Syntax

probe-request-interval interval-value

undo probe-request-interval

Default

The probe request interval is 1000 milliseconds.

Views

Mesh policy view

Predefined user roles

network-admin

mdc-admin

Parameters

interval-value: Specifies an interval in the range of 100 to 8191 milliseconds.

Examples

# Set the probe request interval to 500 milliseconds in mesh policy abc.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc] probe-request-interval 500

Related commands

display wlan mesh-policy

WLAN mesh commands -- wlan mesh-policy

Use wlan mesh-policy to create a mesh policy and enter its view, or enter the view of an existing mesh policy.

Use undo wlan mesh-policy to delete a mesh policy.

Syntax

wlan mesh-policy policy-name

undo wlan mesh-policy policy-name

Default

A system-defined mesh policy exists. The policy name is default_mesh_policy.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

policy-name: Specifies a mesh policy by its name, a case-insensitive string of 1 to 31 characters.

Usage guidelines

Before you can modify or delete attribute settings in the mesh policy that is used on a radio, you must disable the mesh profile that is bound to that radio.

You cannot delete or modify the system-defined mesh policy.

Examples

# Create mesh policy abc and enter mesh policy view.

<Sysname> system-view

[Sysname] wlan mesh-policy abc

[Sysname-wlan-mesh-policy-abc]

WLAN mesh commands -- wlan mesh-profile

Use wlan mesh-profile to create a mesh profile and enter its view, or enter the view of an existing mesh profile.

Use undo wlan mesh-profile to delete a mesh profile.

Syntax

wlan mesh-profile mesh-profile-number

undo wlan mesh-profile mesh-profile-number

Default

No mesh profiles exist.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

mesh-profile-number: Specifies a mesh profile by its number in the range of 1 to 65535.

Usage guidelines

To modify attribute settings in a mesh profile, you must first disable the mesh profile.

Examples

# Create mesh profile 1 and enter its view.

<Sysname> system-view

[Sysname] wlan mesh-profile 1

[Sysname-wlan-mesh-profile-1]

Related commands

mesh-profile enable