WAAS probe commands -- waas tfo auto-discovery blacklist

Use waas tfo auto-discovery blacklist to manually add a blacklist entry.

Use undo waas tfo auto-discovery blacklist to manually delete a blacklist entry.

Syntax

waas tfo auto-discovery blacklist { ip-address ip-address | ipv6-address ipv6-address } port port-num

undo waas tfo auto-discovery blacklist { ip-address ip-address | ipv6-address ipv6-address } port port-num

Default

User-defined blacklist entries do not exist.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ip-address ip-address: Specifies the IPv4 address for the blacklist entry.

ipv6-address ipv6-address: Specifies the IPv6 address for the blacklist entry.

port port-num: Specifies the port number for the blacklist entry, in the range of 1 to 65535.