Static routing probe commands -- display system internal route-static nib log

Use display system internal route-static nib log to display static route NIB logs.

Syntax

display system internal route-static nib log [ reverse ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

reverse: Displays logs in reverse chronological order.

Static routing probe commands -- reset system internal route-static nib log

Use reset system internal route-static nib log to clear static route NIB logs.

Syntax

reset system internal route-static nib log

Views

Probe view

Predefined user roles

network-admin

mdc-admin