IPv6 static routing probe commands -- display system internal ipv6 route-static nib log

Use display system internal ipv6 route-static nib log to display IPv6 static route NIB logs.

Syntax

display system internal ipv6 route-static nib log [ reverse ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

reverse: Displays logs in reverse chronological order.

IPv6 static routing probe commands -- reset system internal ipv6 route-static nib log

Use reset system internal ipv6 route-static nib log to clear IPv6 static route NIB logs.

Syntax

reset system internal ipv6 route-static nib log

Views

Probe view

Predefined user roles

network-admin

mdc-admin