WLAN mesh commands -- display system internal wlan mesh-forwarding statistics (on fat APs)

| NOTE: Support for this command depends on the device model.

Use display system internal wlan mesh-forwarding statistics to display mesh forwarding statistics.

Syntax

display system internal wlan mesh-forwarding statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

WLAN mesh commands -- display system internal wlan mesh-mac (on fat APs)

| NOTE: Support for this command depends on the device model.

Use display system internal wlan mesh-mac to display learned MAC addresses.

Syntax

display system internal wlan mesh-mac [ mac-address [ vlan vlan-id ] ] [ source { mac-learn | mesh-route } ] [ type { mp | sta } ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

mac-address: Specifies a MAC address.

vlan vlan-id: Specifies a VLAN.

source: Specifies the MAC learning method.

mac-learn: Specifies MAC address entries that are obtained through source MAC learning.

mesh-route: Specifies MAC address entries that are obtained through mesh routing.

type: Specifies a MAC address type.

mp: Specifies MAC address entries to reach MPs.

sta: Specifies MAC address entries to reach stations.

WLAN mesh commands -- display system internal wlan mesh-packet statistics (on fat APs)

| NOTE: Support for this command depends on the device model.

Use display system internal wlan mesh-packet statistics to display packet processing statistics.

Syntax

display system internal wlan mesh-packet statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

WLAN mesh commands -- display system internal wlan mesh-security (on fat APs)

| NOTE: Support for this command depends on the device model.

Use display system internal wlan mesh-security to display mesh security status information.

Syntax

display system internal wlan mesh-security

Views

Probe view

Predefined user roles

network-admin

mdc-admin