WLAN forwarding probe commands -- debugging system internal wlan forward packet

Use debugging system internal wlan forward packet to enable WLAN forwarding packet debugging and set rules for filtering debugging information.

Use undo debugging system internal wlan forward packet to disable WLAN forwarding packet debugging and delete all rules for filtering debugging information.

Syntax

debugging system internal wlan forward packet content content-hex [ offset bytes ]

undo debugging system internal wlan forward packet

Default

WLAN forwarding packet debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

packet: Enables WLAN forwarding packet debugging.

content content-hex: Specifies the content used for filtering WLAN forwarding packet debugging information. The content-hex argument is in the H:H:H format, where H represents a byte in the debugging information. The number of Hs is in the range of 1 to 256.

offset bytes: Specifies the offset to start for matching debugging information. The bytes argument is in the range of 0 to 127 bytes. The default value is 0 bytes.