Configuration file management probe commands -- display system internal startup cache

Use display system internal startup cache to display the file path of the .mdb binary configuration file used at the current startup.

Syntax

display system internal startup cache

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When you use the save command to save the running configuration, the device automatically saves the running configuration to both an .mdb binary file and a .cfg text file. The two files use the same file name.

At startup, the device uses the following workflow to identify and load a configuration file:

1. The device searches for a valid .cfg next-startup configuration file.

2. If one is found, the device searches for an .mdb file that has the same name and content as the .cfg file.

3. If a matching .mdb file is found, the device starts up with the .mdb file. If this file does not exist, the device starts up with the .cfg file.

The device loads an .mdb file faster than it loads a .cfg file.

This command displays None if the loaded configuration file is a .cfg file.